*. The sampmle project use two buttons.
*. Buttion pins are PA0 and PA1 respectively.
*. Trigger button 0 (PA0) to transmit 29 bits ID (0x04843) message.
*. Trigger button 1 (PA1) to transmit 11 bits ID (0x055) message. 