MG32L003 Standard Peripherals Firmware Library

宏定义
VCMP_VCAP_Division_Slection
MG32L003_StdPeriph_Driver » VCMP » VCMP_Exported_Constants

## 宏定义
#define | VCMP_1P4_VCAPDIV (0x00U)
#define | VCMP_2P4_VCAPDIV (0x01U)
#define | VCMP_3P4_VCAPDIV (0x02U)
#define | VCMP_4P4_VCAPDIV (0x03U)
#define | IS_VCMP_VCAPDIV(VCMP_VCAPDIV)

## 详细描述

## 宏定义说明

## ◆ IS_VCMP_VCAPDIV

#define IS_VCMP_VCAPDIV | ( |  | VCMP_VCAPDIV | ) |

值:
(((VCMP_VCAPDIV) == VCMP_1P4_VCAPDIV) || ((VCMP_VCAPDIV) == VCMP_2P4_VCAPDIV) || \
((VCMP_VCAPDIV) == VCMP_3P4_VCAPDIV) || ((VCMP_VCAPDIV) == VCMP_4P4_VCAPDIV))
VCMP_1P4_VCAPDIV
#define VCMP_1P4_VCAPDIV
Definition: mg32l003_vcmp.h:64
VCMP_4P4_VCAPDIV
#define VCMP_4P4_VCAPDIV
Definition: mg32l003_vcmp.h:67
VCMP_2P4_VCAPDIV
#define VCMP_2P4_VCAPDIV
Definition: mg32l003_vcmp.h:65
VCMP_3P4_VCAPDIV
#define VCMP_3P4_VCAPDIV
Definition: mg32l003_vcmp.h:66

## ◆ VCMP_1P4_VCAPDIV

#define VCMP_1P4_VCAPDIV (0x00U)

Specifies the VCMP 1/4 VCAP

## ◆ VCMP_2P4_VCAPDIV

#define VCMP_2P4_VCAPDIV (0x01U)

Specifies the VCMP 2/4 VCAP

## ◆ VCMP_3P4_VCAPDIV

#define VCMP_3P4_VCAPDIV (0x02U)

Specifies the VCMP 3/4 VCAP

## ◆ VCMP_4P4_VCAPDIV

#define VCMP_4P4_VCAPDIV (0x03U)

Specifies the VCMP VCAP not divided