MG32L003 Standard Peripherals Firmware Library

宏定义
ADC_Interrupts
MG32L003_StdPeriph_Driver » ADC » ADC_Exported_Constants

## 宏定义
#define | ADC_IT_CONTINUE ADC_INTEN_CONT_IEN
#define | ADC_IT_RANGE_THRESHOLD ADC_INTEN_REG_IEN
#define | ADC_IT_HIGH_THRESHOLD ADC_INTEN_HHT_IEN
#define | ADC_IT_LOW_THRESHOLD ADC_INTEN_LLT_IEN
#define | ADC_IT_CHANNEL15 ADC_INTEN_ADCXIEN_15
#define | ADC_IT_CHANNEL14 ADC_INTEN_ADCXIEN_14
#define | ADC_IT_CHANNEL13 ADC_INTEN_ADCXIEN_13
#define | ADC_IT_CHANNEL12 ADC_INTEN_ADCXIEN_12
#define | ADC_IT_CHANNEL11 ADC_INTEN_ADCXIEN_11
#define | ADC_IT_CHANNEL10 ADC_INTEN_ADCXIEN_10
#define | ADC_IT_CHANNEL9 ADC_INTEN_ADCXIEN_9
#define | ADC_IT_CHANNEL8 ADC_INTEN_ADCXIEN_8
#define | ADC_IT_CHANNEL7 ADC_INTEN_ADCXIEN_7
#define | ADC_IT_CHANNEL6 ADC_INTEN_ADCXIEN_6
#define | ADC_IT_CHANNEL5 ADC_INTEN_ADCXIEN_5
#define | ADC_IT_CHANNEL4 ADC_INTEN_ADCXIEN_4
#define | ADC_IT_CHANNEL3 ADC_INTEN_ADCXIEN_3
#define | ADC_IT_CHANNEL2 ADC_INTEN_ADCXIEN_2
#define | ADC_IT_CHANNEL1 ADC_INTEN_ADCXIEN_1
#define | ADC_IT_CHANNEL0 ADC_INTEN_ADCXIEN_0
#define | ADC_IT_MASK (0xFFFFFUL)
#define | IS_ADC_IT(ADC_IT) (((ADC_IT) & ADC_IT_MASK) != 0x00000)

## 详细描述

## 宏定义说明

## ◆ ADC_IT_CHANNEL0

#define ADC_IT_CHANNEL0 ADC_INTEN_ADCXIEN_0

ADC End of channel 0 conversion interrupt source

## ◆ ADC_IT_CHANNEL1

#define ADC_IT_CHANNEL1 ADC_INTEN_ADCXIEN_1

ADC End of channel 1 conversion interrupt source

## ◆ ADC_IT_CHANNEL10

#define ADC_IT_CHANNEL10 ADC_INTEN_ADCXIEN_10

ADC End of channel 10 conversion interrupt source

## ◆ ADC_IT_CHANNEL11

#define ADC_IT_CHANNEL11 ADC_INTEN_ADCXIEN_11

ADC End of channel 11 conversion interrupt source

## ◆ ADC_IT_CHANNEL12

#define ADC_IT_CHANNEL12 ADC_INTEN_ADCXIEN_12

ADC End of channel 12 conversion interrupt source

## ◆ ADC_IT_CHANNEL13

#define ADC_IT_CHANNEL13 ADC_INTEN_ADCXIEN_13

ADC End of channel 13 conversion interrupt source

## ◆ ADC_IT_CHANNEL14

#define ADC_IT_CHANNEL14 ADC_INTEN_ADCXIEN_14

ADC End of channel 14 conversion interrupt source

## ◆ ADC_IT_CHANNEL15

#define ADC_IT_CHANNEL15 ADC_INTEN_ADCXIEN_15

ADC End of channel 15 conversion interrupt source

## ◆ ADC_IT_CHANNEL2

#define ADC_IT_CHANNEL2 ADC_INTEN_ADCXIEN_2

ADC End of channel 2 conversion interrupt source

## ◆ ADC_IT_CHANNEL3

#define ADC_IT_CHANNEL3 ADC_INTEN_ADCXIEN_3

ADC End of channel 3 conversion interrupt source

## ◆ ADC_IT_CHANNEL4

#define ADC_IT_CHANNEL4 ADC_INTEN_ADCXIEN_4

ADC End of channel 4 conversion interrupt source

## ◆ ADC_IT_CHANNEL5

#define ADC_IT_CHANNEL5 ADC_INTEN_ADCXIEN_5

ADC End of channel 5 conversion interrupt source

## ◆ ADC_IT_CHANNEL6

#define ADC_IT_CHANNEL6 ADC_INTEN_ADCXIEN_6

ADC End of channel 6 conversion interrupt source

## ◆ ADC_IT_CHANNEL7

#define ADC_IT_CHANNEL7 ADC_INTEN_ADCXIEN_7

ADC End of channel 7 conversion interrupt source

## ◆ ADC_IT_CHANNEL8

#define ADC_IT_CHANNEL8 ADC_INTEN_ADCXIEN_8

ADC End of channel 8 conversion interrupt source

## ◆ ADC_IT_CHANNEL9

#define ADC_IT_CHANNEL9 ADC_INTEN_ADCXIEN_9

ADC End of channel 9 conversion interrupt source

## ◆ ADC_IT_CONTINUE

#define ADC_IT_CONTINUE ADC_INTEN_CONT_IEN

ADC End of Continue Conversion interrupt source

## ◆ ADC_IT_HIGH_THRESHOLD

#define ADC_IT_HIGH_THRESHOLD ADC_INTEN_HHT_IEN

ADC conversion data above threshold interrupt source

## ◆ ADC_IT_LOW_THRESHOLD

#define ADC_IT_LOW_THRESHOLD ADC_INTEN_LLT_IEN

ADC conversion data below threshold interrupt source

## ◆ ADC_IT_MASK

#define ADC_IT_MASK (0xFFFFFUL)

ADC interrupt mask

## ◆ ADC_IT_RANGE_THRESHOLD

#define ADC_IT_RANGE_THRESHOLD ADC_INTEN_REG_IEN

ADC conversion data in defined range interrupt source