MG32L003 Standard Peripherals Firmware Library

宏定义
ADC_Continue_Channel_Selection
MG32L003_StdPeriph_Driver » ADC » ADC_Exported_Constants

## 宏定义
#define | ADC_CONTINUE_CHANNEL_0 (ADC_CR2_CHEN_0)
#define | ADC_CONTINUE_CHANNEL_1 (ADC_CR2_CHEN_1)
#define | ADC_CONTINUE_CHANNEL_2 (ADC_CR2_CHEN_2)
#define | ADC_CONTINUE_CHANNEL_3 (ADC_CR2_CHEN_3)
#define | ADC_CONTINUE_CHANNEL_4 (ADC_CR2_CHEN_4)
#define | ADC_CONTINUE_CHANNEL_5 (ADC_CR2_CHEN_5)
#define | ADC_CONTINUE_CHANNEL_6 (ADC_CR2_CHEN_6)
#define | ADC_CONTINUE_CHANNEL_7 (ADC_CR2_CHEN_7)
#define | ADC_CONTINUE_CHANNEL_8 (ADC_CR2_CHEN_8 )
#define | ADC_CONTINUE_CHANNEL_9 (ADC_CR2_CHEN_9 )
#define | ADC_CONTINUE_CHANNEL_10 (ADC_CR2_CHEN_10)
#define | ADC_CONTINUE_CHANNEL_11 (ADC_CR2_CHEN_11)
#define | ADC_CONTINUE_CHANNEL_12 (ADC_CR2_CHEN_12)
#define | ADC_CONTINUE_CHANNEL_13 (ADC_CR2_CHEN_13)
#define | ADC_CONTINUE_CHANNEL_14 (ADC_CR2_CHEN_14)
#define | ADC_CONTINUE_CHANNEL_15 (ADC_CR2_CHEN_15)
#define | ADC_CONTINUE_CHANNEL_ALL (0x0FF000FF)
#define | IS_ADC_CONTINUE_CHANNEL(CHANNEL) (((CHANNEL) & ADC_CONTINUE_CHANNEL_ALL) != 0x0000)
#define | IS_ADC_CHANNEL(CHANNEL) ((IS_ADC_SINGLE_CHANNEL(CHANNEL)) || (IS_ADC_CONTINUE_CHANNEL(CHANNEL)))

## 详细描述

## 宏定义说明

## ◆ ADC_CONTINUE_CHANNEL_0

#define ADC_CONTINUE_CHANNEL_0 (ADC_CR2_CHEN_0)

Select ADC channel 0 in continue mode

## ◆ ADC_CONTINUE_CHANNEL_1

#define ADC_CONTINUE_CHANNEL_1 (ADC_CR2_CHEN_1)

Select ADC channel 1 in continue mode

## ◆ ADC_CONTINUE_CHANNEL_10

#define ADC_CONTINUE_CHANNEL_10 (ADC_CR2_CHEN_10)

Select ADC channel 10 in continue mode

## ◆ ADC_CONTINUE_CHANNEL_11

#define ADC_CONTINUE_CHANNEL_11 (ADC_CR2_CHEN_11)

Select ADC channel 11 in continue mode

## ◆ ADC_CONTINUE_CHANNEL_12

#define ADC_CONTINUE_CHANNEL_12 (ADC_CR2_CHEN_12)

Select ADC channel 12 in continue mode

## ◆ ADC_CONTINUE_CHANNEL_13

#define ADC_CONTINUE_CHANNEL_13 (ADC_CR2_CHEN_13)

Select ADC channel 13 in continue mode

## ◆ ADC_CONTINUE_CHANNEL_14

#define ADC_CONTINUE_CHANNEL_14 (ADC_CR2_CHEN_14)

Select ADC channel 14 in continue mode

## ◆ ADC_CONTINUE_CHANNEL_15

#define ADC_CONTINUE_CHANNEL_15 (ADC_CR2_CHEN_15)

Select ADC channel 15 in continue mode

## ◆ ADC_CONTINUE_CHANNEL_2

#define ADC_CONTINUE_CHANNEL_2 (ADC_CR2_CHEN_2)

Select ADC channel 2 in continue mode

## ◆ ADC_CONTINUE_CHANNEL_3

#define ADC_CONTINUE_CHANNEL_3 (ADC_CR2_CHEN_3)

Select ADC channel 3 in continue mode

## ◆ ADC_CONTINUE_CHANNEL_4

#define ADC_CONTINUE_CHANNEL_4 (ADC_CR2_CHEN_4)

Select ADC channel 4 in continue mode

## ◆ ADC_CONTINUE_CHANNEL_5

#define ADC_CONTINUE_CHANNEL_5 (ADC_CR2_CHEN_5)

Select ADC channel 5 in continue mode

## ◆ ADC_CONTINUE_CHANNEL_6

#define ADC_CONTINUE_CHANNEL_6 (ADC_CR2_CHEN_6)

Select ADC channel 6 in continue mode

## ◆ ADC_CONTINUE_CHANNEL_7

#define ADC_CONTINUE_CHANNEL_7 (ADC_CR2_CHEN_7)

Select ADC channel 7(VCAP) in continue mode

## ◆ ADC_CONTINUE_CHANNEL_8

#define ADC_CONTINUE_CHANNEL_8 (ADC_CR2_CHEN_8 )

Select ADC channel 8 in continue mode

## ◆ ADC_CONTINUE_CHANNEL_9

#define ADC_CONTINUE_CHANNEL_9 (ADC_CR2_CHEN_9 )

Select ADC channel 9 in continue mode