MG32L003 Standard Peripherals Firmware Library

结构体 | 宏定义
System Control Block (SCB)
Defines and Type Definitions

Type definitions for the System Control Block Registers 更多...

## 结构体
struct | SCB_Type
| Structure type to access the System Control Block (SCB). 更多...

## 宏定义
#define | SCB_CPUID_IMPLEMENTER_Pos 24U
#define | SCB_CPUID_IMPLEMENTER_Msk (0xFFUL << SCB_CPUID_IMPLEMENTER_Pos)
#define | SCB_CPUID_VARIANT_Pos 20U
#define | SCB_CPUID_VARIANT_Msk (0xFUL << SCB_CPUID_VARIANT_Pos)
#define | SCB_CPUID_ARCHITECTURE_Pos 16U
#define | SCB_CPUID_ARCHITECTURE_Msk (0xFUL << SCB_CPUID_ARCHITECTURE_Pos)
#define | SCB_CPUID_PARTNO_Pos 4U
#define | SCB_CPUID_PARTNO_Msk (0xFFFUL << SCB_CPUID_PARTNO_Pos)
#define | SCB_CPUID_REVISION_Pos 0U
#define | SCB_CPUID_REVISION_Msk (0xFUL /*<< SCB_CPUID_REVISION_Pos*/)
#define | SCB_ICSR_NMIPENDSET_Pos 31U
#define | SCB_ICSR_NMIPENDSET_Msk (1UL << SCB_ICSR_NMIPENDSET_Pos)
#define | SCB_ICSR_PENDSVSET_Pos 28U
#define | SCB_ICSR_PENDSVSET_Msk (1UL << SCB_ICSR_PENDSVSET_Pos)
#define | SCB_ICSR_PENDSVCLR_Pos 27U
#define | SCB_ICSR_PENDSVCLR_Msk (1UL << SCB_ICSR_PENDSVCLR_Pos)
#define | SCB_ICSR_PENDSTSET_Pos 26U
#define | SCB_ICSR_PENDSTSET_Msk (1UL << SCB_ICSR_PENDSTSET_Pos)
#define | SCB_ICSR_PENDSTCLR_Pos 25U
#define | SCB_ICSR_PENDSTCLR_Msk (1UL << SCB_ICSR_PENDSTCLR_Pos)
#define | SCB_ICSR_ISRPREEMPT_Pos 23U
#define | SCB_ICSR_ISRPREEMPT_Msk (1UL << SCB_ICSR_ISRPREEMPT_Pos)
#define | SCB_ICSR_ISRPENDING_Pos 22U
#define | SCB_ICSR_ISRPENDING_Msk (1UL << SCB_ICSR_ISRPENDING_Pos)
#define | SCB_ICSR_VECTPENDING_Pos 12U
#define | SCB_ICSR_VECTPENDING_Msk (0x1FFUL << SCB_ICSR_VECTPENDING_Pos)
#define | SCB_ICSR_VECTACTIVE_Pos 0U
#define | SCB_ICSR_VECTACTIVE_Msk (0x1FFUL /*<< SCB_ICSR_VECTACTIVE_Pos*/)
#define | SCB_AIRCR_VECTKEY_Pos 16U
#define | SCB_AIRCR_VECTKEY_Msk (0xFFFFUL << SCB_AIRCR_VECTKEY_Pos)
#define | SCB_AIRCR_VECTKEYSTAT_Pos 16U
#define | SCB_AIRCR_VECTKEYSTAT_Msk (0xFFFFUL << SCB_AIRCR_VECTKEYSTAT_Pos)
#define | SCB_AIRCR_ENDIANESS_Pos 15U
#define | SCB_AIRCR_ENDIANESS_Msk (1UL << SCB_AIRCR_ENDIANESS_Pos)
#define | SCB_AIRCR_SYSRESETREQ_Pos 2U
#define | SCB_AIRCR_SYSRESETREQ_Msk (1UL << SCB_AIRCR_SYSRESETREQ_Pos)
#define | SCB_AIRCR_VECTCLRACTIVE_Pos 1U
#define | SCB_AIRCR_VECTCLRACTIVE_Msk (1UL << SCB_AIRCR_VECTCLRACTIVE_Pos)
#define | SCB_SCR_SEVONPEND_Pos 4U
#define | SCB_SCR_SEVONPEND_Msk (1UL << SCB_SCR_SEVONPEND_Pos)
#define | SCB_SCR_SLEEPDEEP_Pos 2U
#define | SCB_SCR_SLEEPDEEP_Msk (1UL << SCB_SCR_SLEEPDEEP_Pos)
#define | SCB_SCR_SLEEPONEXIT_Pos 1U
#define | SCB_SCR_SLEEPONEXIT_Msk (1UL << SCB_SCR_SLEEPONEXIT_Pos)
#define | SCB_CCR_STKALIGN_Pos 9U
#define | SCB_CCR_STKALIGN_Msk (1UL << SCB_CCR_STKALIGN_Pos)
#define | SCB_CCR_UNALIGN_TRP_Pos 3U
#define | SCB_CCR_UNALIGN_TRP_Msk (1UL << SCB_CCR_UNALIGN_TRP_Pos)
#define | SCB_SHCSR_SVCALLPENDED_Pos 15U
#define | SCB_SHCSR_SVCALLPENDED_Msk (1UL << SCB_SHCSR_SVCALLPENDED_Pos)

## 详细描述

Type definitions for the System Control Block Registers

## 宏定义说明

## ◆ SCB_AIRCR_ENDIANESS_Msk

#define SCB_AIRCR_ENDIANESS_Msk (1UL << SCB_AIRCR_ENDIANESS_Pos)

SCB AIRCR: ENDIANESS Mask

## ◆ SCB_AIRCR_ENDIANESS_Pos

#define SCB_AIRCR_ENDIANESS_Pos 15U

SCB AIRCR: ENDIANESS Position

## ◆ SCB_AIRCR_SYSRESETREQ_Msk

#define SCB_AIRCR_SYSRESETREQ_Msk (1UL << SCB_AIRCR_SYSRESETREQ_Pos)

SCB AIRCR: SYSRESETREQ Mask

## ◆ SCB_AIRCR_SYSRESETREQ_Pos

#define SCB_AIRCR_SYSRESETREQ_Pos 2U

SCB AIRCR: SYSRESETREQ Position

## ◆ SCB_AIRCR_VECTCLRACTIVE_Msk

#define SCB_AIRCR_VECTCLRACTIVE_Msk (1UL << SCB_AIRCR_VECTCLRACTIVE_Pos)

SCB AIRCR: VECTCLRACTIVE Mask

## ◆ SCB_AIRCR_VECTCLRACTIVE_Pos

#define SCB_AIRCR_VECTCLRACTIVE_Pos 1U

SCB AIRCR: VECTCLRACTIVE Position

## ◆ SCB_AIRCR_VECTKEY_Msk

#define SCB_AIRCR_VECTKEY_Msk (0xFFFFUL << SCB_AIRCR_VECTKEY_Pos)

SCB AIRCR: VECTKEY Mask

## ◆ SCB_AIRCR_VECTKEY_Pos

#define SCB_AIRCR_VECTKEY_Pos 16U

SCB AIRCR: VECTKEY Position

## ◆ SCB_AIRCR_VECTKEYSTAT_Msk

#define SCB_AIRCR_VECTKEYSTAT_Msk (0xFFFFUL << SCB_AIRCR_VECTKEYSTAT_Pos)

SCB AIRCR: VECTKEYSTAT Mask

## ◆ SCB_AIRCR_VECTKEYSTAT_Pos

#define SCB_AIRCR_VECTKEYSTAT_Pos 16U

SCB AIRCR: VECTKEYSTAT Position

## ◆ SCB_CCR_STKALIGN_Msk

#define SCB_CCR_STKALIGN_Msk (1UL << SCB_CCR_STKALIGN_Pos)

SCB CCR: STKALIGN Mask

## ◆ SCB_CCR_STKALIGN_Pos

#define SCB_CCR_STKALIGN_Pos 9U

SCB CCR: STKALIGN Position

## ◆ SCB_CCR_UNALIGN_TRP_Msk

#define SCB_CCR_UNALIGN_TRP_Msk (1UL << SCB_CCR_UNALIGN_TRP_Pos)

SCB CCR: UNALIGN_TRP Mask

## ◆ SCB_CCR_UNALIGN_TRP_Pos

#define SCB_CCR_UNALIGN_TRP_Pos 3U

SCB CCR: UNALIGN_TRP Position

## ◆ SCB_CPUID_ARCHITECTURE_Msk

#define SCB_CPUID_ARCHITECTURE_Msk (0xFUL << SCB_CPUID_ARCHITECTURE_Pos)

SCB CPUID: ARCHITECTURE Mask

## ◆ SCB_CPUID_ARCHITECTURE_Pos

#define SCB_CPUID_ARCHITECTURE_Pos 16U

SCB CPUID: ARCHITECTURE Position

## ◆ SCB_CPUID_IMPLEMENTER_Msk

#define SCB_CPUID_IMPLEMENTER_Msk (0xFFUL << SCB_CPUID_IMPLEMENTER_Pos)

SCB CPUID: IMPLEMENTER Mask

## ◆ SCB_CPUID_IMPLEMENTER_Pos

#define SCB_CPUID_IMPLEMENTER_Pos 24U

SCB CPUID: IMPLEMENTER Position

## ◆ SCB_CPUID_PARTNO_Msk

#define SCB_CPUID_PARTNO_Msk (0xFFFUL << SCB_CPUID_PARTNO_Pos)

SCB CPUID: PARTNO Mask

## ◆ SCB_CPUID_PARTNO_Pos

#define SCB_CPUID_PARTNO_Pos 4U

SCB CPUID: PARTNO Position

## ◆ SCB_CPUID_REVISION_Msk

#define SCB_CPUID_REVISION_Msk (0xFUL /*<< SCB_CPUID_REVISION_Pos*/)

SCB CPUID: REVISION Mask

## ◆ SCB_CPUID_REVISION_Pos

#define SCB_CPUID_REVISION_Pos 0U

SCB CPUID: REVISION Position

## ◆ SCB_CPUID_VARIANT_Msk

#define SCB_CPUID_VARIANT_Msk (0xFUL << SCB_CPUID_VARIANT_Pos)

SCB CPUID: VARIANT Mask

## ◆ SCB_CPUID_VARIANT_Pos

#define SCB_CPUID_VARIANT_Pos 20U

SCB CPUID: VARIANT Position

## ◆ SCB_ICSR_ISRPENDING_Msk

#define SCB_ICSR_ISRPENDING_Msk (1UL << SCB_ICSR_ISRPENDING_Pos)

SCB ICSR: ISRPENDING Mask

## ◆ SCB_ICSR_ISRPENDING_Pos

#define SCB_ICSR_ISRPENDING_Pos 22U

SCB ICSR: ISRPENDING Position

## ◆ SCB_ICSR_ISRPREEMPT_Msk

#define SCB_ICSR_ISRPREEMPT_Msk (1UL << SCB_ICSR_ISRPREEMPT_Pos)

SCB ICSR: ISRPREEMPT Mask

## ◆ SCB_ICSR_ISRPREEMPT_Pos

#define SCB_ICSR_ISRPREEMPT_Pos 23U

SCB ICSR: ISRPREEMPT Position

## ◆ SCB_ICSR_NMIPENDSET_Msk

#define SCB_ICSR_NMIPENDSET_Msk (1UL << SCB_ICSR_NMIPENDSET_Pos)

SCB ICSR: NMIPENDSET Mask

## ◆ SCB_ICSR_NMIPENDSET_Pos

#define SCB_ICSR_NMIPENDSET_Pos 31U

SCB ICSR: NMIPENDSET Position

## ◆ SCB_ICSR_PENDSTCLR_Msk

#define SCB_ICSR_PENDSTCLR_Msk (1UL << SCB_ICSR_PENDSTCLR_Pos)

SCB ICSR: PENDSTCLR Mask

## ◆ SCB_ICSR_PENDSTCLR_Pos

#define SCB_ICSR_PENDSTCLR_Pos 25U

SCB ICSR: PENDSTCLR Position

## ◆ SCB_ICSR_PENDSTSET_Msk

#define SCB_ICSR_PENDSTSET_Msk (1UL << SCB_ICSR_PENDSTSET_Pos)

SCB ICSR: PENDSTSET Mask

## ◆ SCB_ICSR_PENDSTSET_Pos

#define SCB_ICSR_PENDSTSET_Pos 26U

SCB ICSR: PENDSTSET Position

## ◆ SCB_ICSR_PENDSVCLR_Msk

#define SCB_ICSR_PENDSVCLR_Msk (1UL << SCB_ICSR_PENDSVCLR_Pos)

SCB ICSR: PENDSVCLR Mask

## ◆ SCB_ICSR_PENDSVCLR_Pos

#define SCB_ICSR_PENDSVCLR_Pos 27U

SCB ICSR: PENDSVCLR Position

## ◆ SCB_ICSR_PENDSVSET_Msk

#define SCB_ICSR_PENDSVSET_Msk (1UL << SCB_ICSR_PENDSVSET_Pos)

SCB ICSR: PENDSVSET Mask

## ◆ SCB_ICSR_PENDSVSET_Pos

#define SCB_ICSR_PENDSVSET_Pos 28U

SCB ICSR: PENDSVSET Position

## ◆ SCB_ICSR_VECTACTIVE_Msk

#define SCB_ICSR_VECTACTIVE_Msk (0x1FFUL /*<< SCB_ICSR_VECTACTIVE_Pos*/)

SCB ICSR: VECTACTIVE Mask

## ◆ SCB_ICSR_VECTACTIVE_Pos

#define SCB_ICSR_VECTACTIVE_Pos 0U

SCB ICSR: VECTACTIVE Position

## ◆ SCB_ICSR_VECTPENDING_Msk

#define SCB_ICSR_VECTPENDING_Msk (0x1FFUL << SCB_ICSR_VECTPENDING_Pos)

SCB ICSR: VECTPENDING Mask

## ◆ SCB_ICSR_VECTPENDING_Pos

#define SCB_ICSR_VECTPENDING_Pos 12U

SCB ICSR: VECTPENDING Position

## ◆ SCB_SCR_SEVONPEND_Msk

#define SCB_SCR_SEVONPEND_Msk (1UL << SCB_SCR_SEVONPEND_Pos)

SCB SCR: SEVONPEND Mask

## ◆ SCB_SCR_SEVONPEND_Pos

#define SCB_SCR_SEVONPEND_Pos 4U

SCB SCR: SEVONPEND Position

## ◆ SCB_SCR_SLEEPDEEP_Msk

#define SCB_SCR_SLEEPDEEP_Msk (1UL << SCB_SCR_SLEEPDEEP_Pos)

SCB SCR: SLEEPDEEP Mask

## ◆ SCB_SCR_SLEEPDEEP_Pos

#define SCB_SCR_SLEEPDEEP_Pos 2U

SCB SCR: SLEEPDEEP Position

## ◆ SCB_SCR_SLEEPONEXIT_Msk

#define SCB_SCR_SLEEPONEXIT_Msk (1UL << SCB_SCR_SLEEPONEXIT_Pos)

SCB SCR: SLEEPONEXIT Mask

## ◆ SCB_SCR_SLEEPONEXIT_Pos

#define SCB_SCR_SLEEPONEXIT_Pos 1U

SCB SCR: SLEEPONEXIT Position

## ◆ SCB_SHCSR_SVCALLPENDED_Msk

#define SCB_SHCSR_SVCALLPENDED_Msk (1UL << SCB_SHCSR_SVCALLPENDED_Pos)

SCB SHCSR: SVCALLPENDED Mask

## ◆ SCB_SHCSR_SVCALLPENDED_Pos

#define SCB_SHCSR_SVCALLPENDED_Pos 15U

SCB SHCSR: SVCALLPENDED Position