MG32L003 Standard Peripherals Firmware Library

cmsis_armclang.h
浏览该文件的文档.
1 /**************************************************************************/
7 /*
8 * Copyright (c) 2009-2018 Arm Limited. All rights reserved.
9 *
10 * SPDX-License-Identifier: Apache-2.0
11 *
12 * Licensed under the Apache License, Version 2.0 (the License); you may
13 * not use this file except in compliance with the License.
14 * You may obtain a copy of the License at
15 *
16 * www.apache.org/licenses/LICENSE-2.0
17 *
18 * Unless required by applicable law or agreed to in writing, software
19 * distributed under the License is distributed on an AS IS BASIS, WITHOUT
20 * WARRANTIES OR CONDITIONS OF ANY KIND, either express or implied.
21 * See the License for the specific language governing permissions and
22 * limitations under the License.
23 */
24
25 /*lint -esym(9058, IRQn)*/ /* disable MISRA 2012 Rule 2.4 for IRQn */
26
27 #ifndef __CMSIS_ARMCLANG_H
28 #define __CMSIS_ARMCLANG_H
29
30 #pragma clang system_header /* treat file as system include file */
31
32 #ifndef __ARM_COMPAT_H
33 #include <arm_compat.h> /* Compatibility header for Arm Compiler 5 intrinsics */
34 #endif
35
36 /* CMSIS compiler specific defines */
37 #ifndef __ASM
38 #define __ASM __asm
39 #endif
40 #ifndef __INLINE
41 #define __INLINE __inline
42 #endif
43 #ifndef __STATIC_INLINE
44 #define __STATIC_INLINE static __inline
45 #endif
46 #ifndef __STATIC_FORCEINLINE
47 #define __STATIC_FORCEINLINE __attribute__((always_inline)) static __inline
48 #endif
49 #ifndef __NO_RETURN
50 #define __NO_RETURN __attribute__((__noreturn__))
51 #endif
52 #ifndef __USED
53 #define __USED __attribute__((used))
54 #endif
55 #ifndef __WEAK
56 #define __WEAK __attribute__((weak))
57 #endif
58 #ifndef __PACKED
59 #define __PACKED __attribute__((packed, aligned(1)))
60 #endif
61 #ifndef __PACKED_STRUCT
62 #define __PACKED_STRUCT struct __attribute__((packed, aligned(1)))
63 #endif
64 #ifndef __PACKED_UNION
65 #define __PACKED_UNION union __attribute__((packed, aligned(1)))
66 #endif
67 #ifndef __UNALIGNED_UINT32 /* deprecated */
68 #pragma clang diagnostic push
69 #pragma clang diagnostic ignored "-Wpacked"
70 /*lint -esym(9058, T_UINT32)*/ /* disable MISRA 2012 Rule 2.4 for T_UINT32 */
71 struct __attribute__((packed)) T_UINT32 { uint32_t v; };
72 #pragma clang diagnostic pop
73 #define __UNALIGNED_UINT32(x) (((struct T_UINT32 *)(x))->v)
74 #endif
75 #ifndef __UNALIGNED_UINT16_WRITE
76 #pragma clang diagnostic push
77 #pragma clang diagnostic ignored "-Wpacked"
78 /*lint -esym(9058, T_UINT16_WRITE)*/ /* disable MISRA 2012 Rule 2.4 for T_UINT16_WRITE */
79 __PACKED_STRUCT T_UINT16_WRITE { uint16_t v; };
80 #pragma clang diagnostic pop
81 #define __UNALIGNED_UINT16_WRITE(addr, val) (void)((((struct T_UINT16_WRITE *)(void *)(addr))->v) = (val))
82 #endif
83 #ifndef __UNALIGNED_UINT16_READ
84 #pragma clang diagnostic push
85 #pragma clang diagnostic ignored "-Wpacked"
86 /*lint -esym(9058, T_UINT16_READ)*/ /* disable MISRA 2012 Rule 2.4 for T_UINT16_READ */
87 __PACKED_STRUCT T_UINT16_READ { uint16_t v; };
88 #pragma clang diagnostic pop
89 #define __UNALIGNED_UINT16_READ(addr) (((const struct T_UINT16_READ *)(const void *)(addr))->v)
90 #endif
91 #ifndef __UNALIGNED_UINT32_WRITE
92 #pragma clang diagnostic push
93 #pragma clang diagnostic ignored "-Wpacked"
94 /*lint -esym(9058, T_UINT32_WRITE)*/ /* disable MISRA 2012 Rule 2.4 for T_UINT32_WRITE */
95 __PACKED_STRUCT T_UINT32_WRITE { uint32_t v; };
96 #pragma clang diagnostic pop
97 #define __UNALIGNED_UINT32_WRITE(addr, val) (void)((((struct T_UINT32_WRITE *)(void *)(addr))->v) = (val))
98 #endif
99 #ifndef __UNALIGNED_UINT32_READ
100 #pragma clang diagnostic push
101 #pragma clang diagnostic ignored "-Wpacked"
102 /*lint -esym(9058, T_UINT32_READ)*/ /* disable MISRA 2012 Rule 2.4 for T_UINT32_READ */
103 __PACKED_STRUCT T_UINT32_READ { uint32_t v; };
104 #pragma clang diagnostic pop
105 #define __UNALIGNED_UINT32_READ(addr) (((const struct T_UINT32_READ *)(const void *)(addr))->v)
106 #endif
107 #ifndef __ALIGNED
108 #define __ALIGNED(x) __attribute__((aligned(x)))
109 #endif
110 #ifndef __RESTRICT
111 #define __RESTRICT __restrict
112 #endif
113
114
115 /* ########################### Core Function Access ########################### */
126 /* intrinsic void __enable_irq(); see arm_compat.h */
127
128
134 /* intrinsic void __disable_irq(); see arm_compat.h */
135
136
142 __STATIC_FORCEINLINE uint32_t __get_CONTROL(void)
143 {
144 uint32_t result;
145
146 __ASM volatile ("MRS %0, control" : "=r" (result) );
147 return(result);
148 }
149
150
151 #if (defined (__ARM_FEATURE_CMSE ) && (__ARM_FEATURE_CMSE == 3))
152
157 __STATIC_FORCEINLINE uint32_t __TZ_get_CONTROL_NS(void)
158 {
159 uint32_t result;
160
161 __ASM volatile ("MRS %0, control_ns" : "=r" (result) );
162 return(result);
163 }
164 #endif
165
166
172 __STATIC_FORCEINLINE void __set_CONTROL(uint32_t control)
173 {
174 __ASM volatile ("MSR control, %0" : : "r" (control) : "memory");
175 }
176
177
178 #if (defined (__ARM_FEATURE_CMSE ) && (__ARM_FEATURE_CMSE == 3))
179
184 __STATIC_FORCEINLINE void __TZ_set_CONTROL_NS(uint32_t control)
185 {
186 __ASM volatile ("MSR control_ns, %0" : : "r" (control) : "memory");
187 }
188 #endif
189
190
196 __STATIC_FORCEINLINE uint32_t __get_IPSR(void)
197 {
198 uint32_t result;
199
200 __ASM volatile ("MRS %0, ipsr" : "=r" (result) );
201 return(result);
202 }
203
204
210 __STATIC_FORCEINLINE uint32_t __get_APSR(void)
211 {
212 uint32_t result;
213
214 __ASM volatile ("MRS %0, apsr" : "=r" (result) );
215 return(result);
216 }
217
218
224 __STATIC_FORCEINLINE uint32_t __get_xPSR(void)
225 {
226 uint32_t result;
227
228 __ASM volatile ("MRS %0, xpsr" : "=r" (result) );
229 return(result);
230 }
231
232
238 __STATIC_FORCEINLINE uint32_t __get_PSP(void)
239 {
240 uint32_t result;
241
242 __ASM volatile ("MRS %0, psp" : "=r" (result) );
243 return(result);
244 }
245
246
247 #if (defined (__ARM_FEATURE_CMSE ) && (__ARM_FEATURE_CMSE == 3))
248
253 __STATIC_FORCEINLINE uint32_t __TZ_get_PSP_NS(void)
254 {
255 uint32_t result;
256
257 __ASM volatile ("MRS %0, psp_ns" : "=r" (result) );
258 return(result);
259 }
260 #endif
261
262
268 __STATIC_FORCEINLINE void __set_PSP(uint32_t topOfProcStack)
269 {
270 __ASM volatile ("MSR psp, %0" : : "r" (topOfProcStack) : );
271 }
272
273
274 #if (defined (__ARM_FEATURE_CMSE ) && (__ARM_FEATURE_CMSE == 3))
275
280 __STATIC_FORCEINLINE void __TZ_set_PSP_NS(uint32_t topOfProcStack)
281 {
282 __ASM volatile ("MSR psp_ns, %0" : : "r" (topOfProcStack) : );
283 }
284 #endif
285
286
292 __STATIC_FORCEINLINE uint32_t __get_MSP(void)
293 {
294 uint32_t result;
295
296 __ASM volatile ("MRS %0, msp" : "=r" (result) );
297 return(result);
298 }
299
300
301 #if (defined (__ARM_FEATURE_CMSE ) && (__ARM_FEATURE_CMSE == 3))
302
307 __STATIC_FORCEINLINE uint32_t __TZ_get_MSP_NS(void)
308 {
309 uint32_t result;
310
311 __ASM volatile ("MRS %0, msp_ns" : "=r" (result) );
312 return(result);
313 }
314 #endif
315
316
322 __STATIC_FORCEINLINE void __set_MSP(uint32_t topOfMainStack)
323 {
324 __ASM volatile ("MSR msp, %0" : : "r" (topOfMainStack) : );
325 }
326
327
328 #if (defined (__ARM_FEATURE_CMSE ) && (__ARM_FEATURE_CMSE == 3))
329
334 __STATIC_FORCEINLINE void __TZ_set_MSP_NS(uint32_t topOfMainStack)
335 {
336 __ASM volatile ("MSR msp_ns, %0" : : "r" (topOfMainStack) : );
337 }
338 #endif
339
340
341 #if (defined (__ARM_FEATURE_CMSE ) && (__ARM_FEATURE_CMSE == 3))
342
347 __STATIC_FORCEINLINE uint32_t __TZ_get_SP_NS(void)
348 {
349 uint32_t result;
350
351 __ASM volatile ("MRS %0, sp_ns" : "=r" (result) );
352 return(result);
353 }
354
355
361 __STATIC_FORCEINLINE void __TZ_set_SP_NS(uint32_t topOfStack)
362 {
363 __ASM volatile ("MSR sp_ns, %0" : : "r" (topOfStack) : );
364 }
365 #endif
366
367
373 __STATIC_FORCEINLINE uint32_t __get_PRIMASK(void)
374 {
375 uint32_t result;
376
377 __ASM volatile ("MRS %0, primask" : "=r" (result) );
378 return(result);
379 }
380
381
382 #if (defined (__ARM_FEATURE_CMSE ) && (__ARM_FEATURE_CMSE == 3))
383
388 __STATIC_FORCEINLINE uint32_t __TZ_get_PRIMASK_NS(void)
389 {
390 uint32_t result;
391
392 __ASM volatile ("MRS %0, primask_ns" : "=r" (result) );
393 return(result);
394 }
395 #endif
396
397
403 __STATIC_FORCEINLINE void __set_PRIMASK(uint32_t priMask)
404 {
405 __ASM volatile ("MSR primask, %0" : : "r" (priMask) : "memory");
406 }
407
408
409 #if (defined (__ARM_FEATURE_CMSE ) && (__ARM_FEATURE_CMSE == 3))
410
415 __STATIC_FORCEINLINE void __TZ_set_PRIMASK_NS(uint32_t priMask)
416 {
417 __ASM volatile ("MSR primask_ns, %0" : : "r" (priMask) : "memory");
418 }
419 #endif
420
421
422 #if ((defined (__ARM_ARCH_7M__ ) && (__ARM_ARCH_7M__ == 1)) || \
423 (defined (__ARM_ARCH_7EM__ ) && (__ARM_ARCH_7EM__ == 1)) || \
424 (defined (__ARM_ARCH_8M_MAIN__ ) && (__ARM_ARCH_8M_MAIN__ == 1)) )
425
430 #define __enable_fault_irq __enable_fiq /* see arm_compat.h */
431
432
438 #define __disable_fault_irq __disable_fiq /* see arm_compat.h */
439
440
446 __STATIC_FORCEINLINE uint32_t __get_BASEPRI(void)
447 {
448 uint32_t result;
449
450 __ASM volatile ("MRS %0, basepri" : "=r" (result) );
451 return(result);
452 }
453
454
455 #if (defined (__ARM_FEATURE_CMSE ) && (__ARM_FEATURE_CMSE == 3))
456
461 __STATIC_FORCEINLINE uint32_t __TZ_get_BASEPRI_NS(void)
462 {
463 uint32_t result;
464
465 __ASM volatile ("MRS %0, basepri_ns" : "=r" (result) );
466 return(result);
467 }
468 #endif
469
470
476 __STATIC_FORCEINLINE void __set_BASEPRI(uint32_t basePri)
477 {
478 __ASM volatile ("MSR basepri, %0" : : "r" (basePri) : "memory");
479 }
480
481
482 #if (defined (__ARM_FEATURE_CMSE ) && (__ARM_FEATURE_CMSE == 3))
483
488 __STATIC_FORCEINLINE void __TZ_set_BASEPRI_NS(uint32_t basePri)
489 {
490 __ASM volatile ("MSR basepri_ns, %0" : : "r" (basePri) : "memory");
491 }
492 #endif
493
494
501 __STATIC_FORCEINLINE void __set_BASEPRI_MAX(uint32_t basePri)
502 {
503 __ASM volatile ("MSR basepri_max, %0" : : "r" (basePri) : "memory");
504 }
505
506
512 __STATIC_FORCEINLINE uint32_t __get_FAULTMASK(void)
513 {
514 uint32_t result;
515
516 __ASM volatile ("MRS %0, faultmask" : "=r" (result) );
517 return(result);
518 }
519
520
521 #if (defined (__ARM_FEATURE_CMSE ) && (__ARM_FEATURE_CMSE == 3))
522
527 __STATIC_FORCEINLINE uint32_t __TZ_get_FAULTMASK_NS(void)
528 {
529 uint32_t result;
530
531 __ASM volatile ("MRS %0, faultmask_ns" : "=r" (result) );
532 return(result);
533 }
534 #endif
535
536
542 __STATIC_FORCEINLINE void __set_FAULTMASK(uint32_t faultMask)
543 {
544 __ASM volatile ("MSR faultmask, %0" : : "r" (faultMask) : "memory");
545 }
546
547
548 #if (defined (__ARM_FEATURE_CMSE ) && (__ARM_FEATURE_CMSE == 3))
549
554 __STATIC_FORCEINLINE void __TZ_set_FAULTMASK_NS(uint32_t faultMask)
555 {
556 __ASM volatile ("MSR faultmask_ns, %0" : : "r" (faultMask) : "memory");
557 }
558 #endif
559
560 #endif /* ((defined (__ARM_ARCH_7M__ ) && (__ARM_ARCH_7M__ == 1)) || \
561 (defined (__ARM_ARCH_7EM__ ) && (__ARM_ARCH_7EM__ == 1)) || \
562 (defined (__ARM_ARCH_8M_MAIN__ ) && (__ARM_ARCH_8M_MAIN__ == 1)) ) */
563
564
565 #if ((defined (__ARM_ARCH_8M_MAIN__ ) && (__ARM_ARCH_8M_MAIN__ == 1)) || \
566 (defined (__ARM_ARCH_8M_BASE__ ) && (__ARM_ARCH_8M_BASE__ == 1)) )
567
577 __STATIC_FORCEINLINE uint32_t __get_PSPLIM(void)
578 {
579 #if (!(defined (__ARM_ARCH_8M_MAIN__ ) && (__ARM_ARCH_8M_MAIN__ == 1)) && \
580 (!defined (__ARM_FEATURE_CMSE) || (__ARM_FEATURE_CMSE < 3)))
581 // without main extensions, the non-secure PSPLIM is RAZ/WI
582 return 0U;
583 #else
584 uint32_t result;
585 __ASM volatile ("MRS %0, psplim" : "=r" (result) );
586 return result;
587 #endif
588 }
589
590 #if (defined (__ARM_FEATURE_CMSE) && (__ARM_FEATURE_CMSE == 3))
591
600 __STATIC_FORCEINLINE uint32_t __TZ_get_PSPLIM_NS(void)
601 {
602 #if (!(defined (__ARM_ARCH_8M_MAIN__ ) && (__ARM_ARCH_8M_MAIN__ == 1)))
603 // without main extensions, the non-secure PSPLIM is RAZ/WI
604 return 0U;
605 #else
606 uint32_t result;
607 __ASM volatile ("MRS %0, psplim_ns" : "=r" (result) );
608 return result;
609 #endif
610 }
611 #endif
612
613
623 __STATIC_FORCEINLINE void __set_PSPLIM(uint32_t ProcStackPtrLimit)
624 {
625 #if (!(defined (__ARM_ARCH_8M_MAIN__ ) && (__ARM_ARCH_8M_MAIN__ == 1)) && \
626 (!defined (__ARM_FEATURE_CMSE) || (__ARM_FEATURE_CMSE < 3)))
627 // without main extensions, the non-secure PSPLIM is RAZ/WI
628 (void)ProcStackPtrLimit;
629 #else
630 __ASM volatile ("MSR psplim, %0" : : "r" (ProcStackPtrLimit));
631 #endif
632 }
633
634
635 #if (defined (__ARM_FEATURE_CMSE ) && (__ARM_FEATURE_CMSE == 3))
636
645 __STATIC_FORCEINLINE void __TZ_set_PSPLIM_NS(uint32_t ProcStackPtrLimit)
646 {
647 #if (!(defined (__ARM_ARCH_8M_MAIN__ ) && (__ARM_ARCH_8M_MAIN__ == 1)))
648 // without main extensions, the non-secure PSPLIM is RAZ/WI
649 (void)ProcStackPtrLimit;
650 #else
651 __ASM volatile ("MSR psplim_ns, %0\n" : : "r" (ProcStackPtrLimit));
652 #endif
653 }
654 #endif
655
656
665 __STATIC_FORCEINLINE uint32_t __get_MSPLIM(void)
666 {
667 #if (!(defined (__ARM_ARCH_8M_MAIN__ ) && (__ARM_ARCH_8M_MAIN__ == 1)) && \
668 (!defined (__ARM_FEATURE_CMSE) || (__ARM_FEATURE_CMSE < 3)))
669 // without main extensions, the non-secure MSPLIM is RAZ/WI
670 return 0U;
671 #else
672 uint32_t result;
673 __ASM volatile ("MRS %0, msplim" : "=r" (result) );
674 return result;
675 #endif
676 }
677
678
679 #if (defined (__ARM_FEATURE_CMSE ) && (__ARM_FEATURE_CMSE == 3))
680
688 __STATIC_FORCEINLINE uint32_t __TZ_get_MSPLIM_NS(void)
689 {
690 #if (!(defined (__ARM_ARCH_8M_MAIN__ ) && (__ARM_ARCH_8M_MAIN__ == 1)))
691 // without main extensions, the non-secure MSPLIM is RAZ/WI
692 return 0U;
693 #else
694 uint32_t result;
695 __ASM volatile ("MRS %0, msplim_ns" : "=r" (result) );
696 return result;
697 #endif
698 }
699 #endif
700
701
710 __STATIC_FORCEINLINE void __set_MSPLIM(uint32_t MainStackPtrLimit)
711 {
712 #if (!(defined (__ARM_ARCH_8M_MAIN__ ) && (__ARM_ARCH_8M_MAIN__ == 1)) && \
713 (!defined (__ARM_FEATURE_CMSE) || (__ARM_FEATURE_CMSE < 3)))
714 // without main extensions, the non-secure MSPLIM is RAZ/WI
715 (void)MainStackPtrLimit;
716 #else
717 __ASM volatile ("MSR msplim, %0" : : "r" (MainStackPtrLimit));
718 #endif
719 }
720
721
722 #if (defined (__ARM_FEATURE_CMSE ) && (__ARM_FEATURE_CMSE == 3))
723
731 __STATIC_FORCEINLINE void __TZ_set_MSPLIM_NS(uint32_t MainStackPtrLimit)
732 {
733 #if (!(defined (__ARM_ARCH_8M_MAIN__ ) && (__ARM_ARCH_8M_MAIN__ == 1)))
734 // without main extensions, the non-secure MSPLIM is RAZ/WI
735 (void)MainStackPtrLimit;
736 #else
737 __ASM volatile ("MSR msplim_ns, %0" : : "r" (MainStackPtrLimit));
738 #endif
739 }
740 #endif
741
742 #endif /* ((defined (__ARM_ARCH_8M_MAIN__ ) && (__ARM_ARCH_8M_MAIN__ == 1)) || \
743 (defined (__ARM_ARCH_8M_BASE__ ) && (__ARM_ARCH_8M_BASE__ == 1)) ) */
744
750 #if ((defined (__FPU_PRESENT) && (__FPU_PRESENT == 1U)) && \
751 (defined (__FPU_USED ) && (__FPU_USED == 1U)) )
752 #define __get_FPSCR (uint32_t)__builtin_arm_get_fpscr
753 #else
754 #define __get_FPSCR() ((uint32_t)0U)
755 #endif
756
762 #if ((defined (__FPU_PRESENT) && (__FPU_PRESENT == 1U)) && \
763 (defined (__FPU_USED ) && (__FPU_USED == 1U)) )
764 #define __set_FPSCR __builtin_arm_set_fpscr
765 #else
766 #define __set_FPSCR(x) ((void)(x))
767 #endif
768
769
773 /* ########################## Core Instruction Access ######################### */
779 /* Define macros for porting to both thumb1 and thumb2.
780 * For thumb1, use low register (r0-r7), specified by constraint "l"
781 * Otherwise, use general registers, specified by constraint "r" */
782 #if defined (__thumb__) && !defined (__thumb2__)
783 #define __CMSIS_GCC_OUT_REG(r) "=l" (r)
784 #define __CMSIS_GCC_USE_REG(r) "l" (r)
785 #else
786 #define __CMSIS_GCC_OUT_REG(r) "=r" (r)
787 #define __CMSIS_GCC_USE_REG(r) "r" (r)
788 #endif
789
794 #define __NOP __builtin_arm_nop
795
800 #define __WFI __builtin_arm_wfi
801
802
808 #define __WFE __builtin_arm_wfe
809
810
815 #define __SEV __builtin_arm_sev
816
817
824 #define __ISB() __builtin_arm_isb(0xF);
825
831 #define __DSB() __builtin_arm_dsb(0xF);
832
833
839 #define __DMB() __builtin_arm_dmb(0xF);
840
841
848 #define __REV(value) __builtin_bswap32(value)
849
850
857 #define __REV16(value) __ROR(__REV(value), 16)
858
859
866 #define __REVSH(value) (int16_t)__builtin_bswap16(value)
867
868
876 __STATIC_FORCEINLINE uint32_t __ROR(uint32_t op1, uint32_t op2)
877 {
878 op2 %= 32U;
879 if (op2 == 0U)
880 {
881 return op1;
882 }
883 return (op1 >> op2) | (op1 << (32U - op2));
884 }
885
886
894 #define __BKPT(value) __ASM volatile ("bkpt "#value)
895
896
903 #define __RBIT __builtin_arm_rbit
904
911 #define __CLZ (uint8_t)__builtin_clz
912
913
914 #if ((defined (__ARM_ARCH_7M__ ) && (__ARM_ARCH_7M__ == 1)) || \
915 (defined (__ARM_ARCH_7EM__ ) && (__ARM_ARCH_7EM__ == 1)) || \
916 (defined (__ARM_ARCH_8M_MAIN__ ) && (__ARM_ARCH_8M_MAIN__ == 1)) || \
917 (defined (__ARM_ARCH_8M_BASE__ ) && (__ARM_ARCH_8M_BASE__ == 1)) )
918
924 #define __LDREXB (uint8_t)__builtin_arm_ldrex
925
926
933 #define __LDREXH (uint16_t)__builtin_arm_ldrex
934
935
942 #define __LDREXW (uint32_t)__builtin_arm_ldrex
943
944
953 #define __STREXB (uint32_t)__builtin_arm_strex
954
955
964 #define __STREXH (uint32_t)__builtin_arm_strex
965
966
975 #define __STREXW (uint32_t)__builtin_arm_strex
976
977
982 #define __CLREX __builtin_arm_clrex
983
984 #endif /* ((defined (__ARM_ARCH_7M__ ) && (__ARM_ARCH_7M__ == 1)) || \
985 (defined (__ARM_ARCH_7EM__ ) && (__ARM_ARCH_7EM__ == 1)) || \
986 (defined (__ARM_ARCH_8M_MAIN__ ) && (__ARM_ARCH_8M_MAIN__ == 1)) || \
987 (defined (__ARM_ARCH_8M_BASE__ ) && (__ARM_ARCH_8M_BASE__ == 1)) ) */
988
989
990 #if ((defined (__ARM_ARCH_7M__ ) && (__ARM_ARCH_7M__ == 1)) || \
991 (defined (__ARM_ARCH_7EM__ ) && (__ARM_ARCH_7EM__ == 1)) || \
992 (defined (__ARM_ARCH_8M_MAIN__ ) && (__ARM_ARCH_8M_MAIN__ == 1)) )
993
1001 #define __SSAT __builtin_arm_ssat
1002
1003
1011 #define __USAT __builtin_arm_usat
1012
1013
1021 __STATIC_FORCEINLINE uint32_t __RRX(uint32_t value)
1022 {
1023 uint32_t result;
1024
1025 __ASM volatile ("rrx %0, %1" : __CMSIS_GCC_OUT_REG (result) : __CMSIS_GCC_USE_REG (value) );
1026 return(result);
1027 }
1028
1029
1036 __STATIC_FORCEINLINE uint8_t __LDRBT(volatile uint8_t *ptr)
1037 {
1038 uint32_t result;
1039
1040 __ASM volatile ("ldrbt %0, %1" : "=r" (result) : "Q" (*ptr) );
1041 return ((uint8_t) result); /* Add explicit type cast here */
1042 }
1043
1044
1051 __STATIC_FORCEINLINE uint16_t __LDRHT(volatile uint16_t *ptr)
1052 {
1053 uint32_t result;
1054
1055 __ASM volatile ("ldrht %0, %1" : "=r" (result) : "Q" (*ptr) );
1056 return ((uint16_t) result); /* Add explicit type cast here */
1057 }
1058
1059
1066 __STATIC_FORCEINLINE uint32_t __LDRT(volatile uint32_t *ptr)
1067 {
1068 uint32_t result;
1069
1070 __ASM volatile ("ldrt %0, %1" : "=r" (result) : "Q" (*ptr) );
1071 return(result);
1072 }
1073
1074
1081 __STATIC_FORCEINLINE void __STRBT(uint8_t value, volatile uint8_t *ptr)
1082 {
1083 __ASM volatile ("strbt %1, %0" : "=Q" (*ptr) : "r" ((uint32_t)value) );
1084 }
1085
1086
1093 __STATIC_FORCEINLINE void __STRHT(uint16_t value, volatile uint16_t *ptr)
1094 {
1095 __ASM volatile ("strht %1, %0" : "=Q" (*ptr) : "r" ((uint32_t)value) );
1096 }
1097
1098
1105 __STATIC_FORCEINLINE void __STRT(uint32_t value, volatile uint32_t *ptr)
1106 {
1107 __ASM volatile ("strt %1, %0" : "=Q" (*ptr) : "r" (value) );
1108 }
1109
1110 #else /* ((defined (__ARM_ARCH_7M__ ) && (__ARM_ARCH_7M__ == 1)) || \
1111 (defined (__ARM_ARCH_7EM__ ) && (__ARM_ARCH_7EM__ == 1)) || \
1112 (defined (__ARM_ARCH_8M_MAIN__ ) && (__ARM_ARCH_8M_MAIN__ == 1)) ) */
1113
1121 __STATIC_FORCEINLINE int32_t __SSAT(int32_t val, uint32_t sat)
1122 {
1123 if ((sat >= 1U) && (sat <= 32U))
1124 {
1125 const int32_t max = (int32_t)((1U << (sat - 1U)) - 1U);
1126 const int32_t min = -1 - max ;
1127 if (val > max)
1128 {
1129 return max;
1130 }
1131 else if (val < min)
1132 {
1133 return min;
1134 }
1135 }
1136 return val;
1137 }
1138
1146 __STATIC_FORCEINLINE uint32_t __USAT(int32_t val, uint32_t sat)
1147 {
1148 if (sat <= 31U)
1149 {
1150 const uint32_t max = ((1U << sat) - 1U);
1151 if (val > (int32_t)max)
1152 {
1153 return max;
1154 }
1155 else if (val < 0)
1156 {
1157 return 0U;
1158 }
1159 }
1160 return (uint32_t)val;
1161 }
1162
1163 #endif /* ((defined (__ARM_ARCH_7M__ ) && (__ARM_ARCH_7M__ == 1)) || \
1164 (defined (__ARM_ARCH_7EM__ ) && (__ARM_ARCH_7EM__ == 1)) || \
1165 (defined (__ARM_ARCH_8M_MAIN__ ) && (__ARM_ARCH_8M_MAIN__ == 1)) ) */
1166
1167
1168 #if ((defined (__ARM_ARCH_8M_MAIN__ ) && (__ARM_ARCH_8M_MAIN__ == 1)) || \
1169 (defined (__ARM_ARCH_8M_BASE__ ) && (__ARM_ARCH_8M_BASE__ == 1)) )
1170
1176 __STATIC_FORCEINLINE uint8_t __LDAB(volatile uint8_t *ptr)
1177 {
1178 uint32_t result;
1179
1180 __ASM volatile ("ldab %0, %1" : "=r" (result) : "Q" (*ptr) );
1181 return ((uint8_t) result);
1182 }
1183
1184
1191 __STATIC_FORCEINLINE uint16_t __LDAH(volatile uint16_t *ptr)
1192 {
1193 uint32_t result;
1194
1195 __ASM volatile ("ldah %0, %1" : "=r" (result) : "Q" (*ptr) );
1196 return ((uint16_t) result);
1197 }
1198
1199
1206 __STATIC_FORCEINLINE uint32_t __LDA(volatile uint32_t *ptr)
1207 {
1208 uint32_t result;
1209
1210 __ASM volatile ("lda %0, %1" : "=r" (result) : "Q" (*ptr) );
1211 return(result);
1212 }
1213
1214
1221 __STATIC_FORCEINLINE void __STLB(uint8_t value, volatile uint8_t *ptr)
1222 {
1223 __ASM volatile ("stlb %1, %0" : "=Q" (*ptr) : "r" ((uint32_t)value) );
1224 }
1225
1226
1233 __STATIC_FORCEINLINE void __STLH(uint16_t value, volatile uint16_t *ptr)
1234 {
1235 __ASM volatile ("stlh %1, %0" : "=Q" (*ptr) : "r" ((uint32_t)value) );
1236 }
1237
1238
1245 __STATIC_FORCEINLINE void __STL(uint32_t value, volatile uint32_t *ptr)
1246 {
1247 __ASM volatile ("stl %1, %0" : "=Q" (*ptr) : "r" ((uint32_t)value) );
1248 }
1249
1250
1257 #define __LDAEXB (uint8_t)__builtin_arm_ldaex
1258
1259
1266 #define __LDAEXH (uint16_t)__builtin_arm_ldaex
1267
1268
1275 #define __LDAEX (uint32_t)__builtin_arm_ldaex
1276
1277
1286 #define __STLEXB (uint32_t)__builtin_arm_stlex
1287
1288
1297 #define __STLEXH (uint32_t)__builtin_arm_stlex
1298
1299
1308 #define __STLEX (uint32_t)__builtin_arm_stlex
1309
1310 #endif /* ((defined (__ARM_ARCH_8M_MAIN__ ) && (__ARM_ARCH_8M_MAIN__ == 1)) || \
1311 (defined (__ARM_ARCH_8M_BASE__ ) && (__ARM_ARCH_8M_BASE__ == 1)) ) */
1312 /* end of group CMSIS_Core_InstructionInterface */
1314
1315
1316 /* ################### Compiler specific Intrinsics ########################### */
1322 #if (defined (__ARM_FEATURE_DSP) && (__ARM_FEATURE_DSP == 1))
1323
1324 __STATIC_FORCEINLINE uint32_t __SADD8(uint32_t op1, uint32_t op2)
1325 {
1326 uint32_t result;
1327
1328 __ASM volatile ("sadd8 %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1329 return(result);
1330 }
1331
1332 __STATIC_FORCEINLINE uint32_t __QADD8(uint32_t op1, uint32_t op2)
1333 {
1334 uint32_t result;
1335
1336 __ASM volatile ("qadd8 %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1337 return(result);
1338 }
1339
1340 __STATIC_FORCEINLINE uint32_t __SHADD8(uint32_t op1, uint32_t op2)
1341 {
1342 uint32_t result;
1343
1344 __ASM volatile ("shadd8 %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1345 return(result);
1346 }
1347
1348 __STATIC_FORCEINLINE uint32_t __UADD8(uint32_t op1, uint32_t op2)
1349 {
1350 uint32_t result;
1351
1352 __ASM volatile ("uadd8 %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1353 return(result);
1354 }
1355
1356 __STATIC_FORCEINLINE uint32_t __UQADD8(uint32_t op1, uint32_t op2)
1357 {
1358 uint32_t result;
1359
1360 __ASM volatile ("uqadd8 %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1361 return(result);
1362 }
1363
1364 __STATIC_FORCEINLINE uint32_t __UHADD8(uint32_t op1, uint32_t op2)
1365 {
1366 uint32_t result;
1367
1368 __ASM volatile ("uhadd8 %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1369 return(result);
1370 }
1371
1372
1373 __STATIC_FORCEINLINE uint32_t __SSUB8(uint32_t op1, uint32_t op2)
1374 {
1375 uint32_t result;
1376
1377 __ASM volatile ("ssub8 %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1378 return(result);
1379 }
1380
1381 __STATIC_FORCEINLINE uint32_t __QSUB8(uint32_t op1, uint32_t op2)
1382 {
1383 uint32_t result;
1384
1385 __ASM volatile ("qsub8 %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1386 return(result);
1387 }
1388
1389 __STATIC_FORCEINLINE uint32_t __SHSUB8(uint32_t op1, uint32_t op2)
1390 {
1391 uint32_t result;
1392
1393 __ASM volatile ("shsub8 %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1394 return(result);
1395 }
1396
1397 __STATIC_FORCEINLINE uint32_t __USUB8(uint32_t op1, uint32_t op2)
1398 {
1399 uint32_t result;
1400
1401 __ASM volatile ("usub8 %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1402 return(result);
1403 }
1404
1405 __STATIC_FORCEINLINE uint32_t __UQSUB8(uint32_t op1, uint32_t op2)
1406 {
1407 uint32_t result;
1408
1409 __ASM volatile ("uqsub8 %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1410 return(result);
1411 }
1412
1413 __STATIC_FORCEINLINE uint32_t __UHSUB8(uint32_t op1, uint32_t op2)
1414 {
1415 uint32_t result;
1416
1417 __ASM volatile ("uhsub8 %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1418 return(result);
1419 }
1420
1421
1422 __STATIC_FORCEINLINE uint32_t __SADD16(uint32_t op1, uint32_t op2)
1423 {
1424 uint32_t result;
1425
1426 __ASM volatile ("sadd16 %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1427 return(result);
1428 }
1429
1430 __STATIC_FORCEINLINE uint32_t __QADD16(uint32_t op1, uint32_t op2)
1431 {
1432 uint32_t result;
1433
1434 __ASM volatile ("qadd16 %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1435 return(result);
1436 }
1437
1438 __STATIC_FORCEINLINE uint32_t __SHADD16(uint32_t op1, uint32_t op2)
1439 {
1440 uint32_t result;
1441
1442 __ASM volatile ("shadd16 %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1443 return(result);
1444 }
1445
1446 __STATIC_FORCEINLINE uint32_t __UADD16(uint32_t op1, uint32_t op2)
1447 {
1448 uint32_t result;
1449
1450 __ASM volatile ("uadd16 %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1451 return(result);
1452 }
1453
1454 __STATIC_FORCEINLINE uint32_t __UQADD16(uint32_t op1, uint32_t op2)
1455 {
1456 uint32_t result;
1457
1458 __ASM volatile ("uqadd16 %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1459 return(result);
1460 }
1461
1462 __STATIC_FORCEINLINE uint32_t __UHADD16(uint32_t op1, uint32_t op2)
1463 {
1464 uint32_t result;
1465
1466 __ASM volatile ("uhadd16 %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1467 return(result);
1468 }
1469
1470 __STATIC_FORCEINLINE uint32_t __SSUB16(uint32_t op1, uint32_t op2)
1471 {
1472 uint32_t result;
1473
1474 __ASM volatile ("ssub16 %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1475 return(result);
1476 }
1477
1478 __STATIC_FORCEINLINE uint32_t __QSUB16(uint32_t op1, uint32_t op2)
1479 {
1480 uint32_t result;
1481
1482 __ASM volatile ("qsub16 %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1483 return(result);
1484 }
1485
1486 __STATIC_FORCEINLINE uint32_t __SHSUB16(uint32_t op1, uint32_t op2)
1487 {
1488 uint32_t result;
1489
1490 __ASM volatile ("shsub16 %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1491 return(result);
1492 }
1493
1494 __STATIC_FORCEINLINE uint32_t __USUB16(uint32_t op1, uint32_t op2)
1495 {
1496 uint32_t result;
1497
1498 __ASM volatile ("usub16 %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1499 return(result);
1500 }
1501
1502 __STATIC_FORCEINLINE uint32_t __UQSUB16(uint32_t op1, uint32_t op2)
1503 {
1504 uint32_t result;
1505
1506 __ASM volatile ("uqsub16 %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1507 return(result);
1508 }
1509
1510 __STATIC_FORCEINLINE uint32_t __UHSUB16(uint32_t op1, uint32_t op2)
1511 {
1512 uint32_t result;
1513
1514 __ASM volatile ("uhsub16 %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1515 return(result);
1516 }
1517
1518 __STATIC_FORCEINLINE uint32_t __SASX(uint32_t op1, uint32_t op2)
1519 {
1520 uint32_t result;
1521
1522 __ASM volatile ("sasx %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1523 return(result);
1524 }
1525
1526 __STATIC_FORCEINLINE uint32_t __QASX(uint32_t op1, uint32_t op2)
1527 {
1528 uint32_t result;
1529
1530 __ASM volatile ("qasx %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1531 return(result);
1532 }
1533
1534 __STATIC_FORCEINLINE uint32_t __SHASX(uint32_t op1, uint32_t op2)
1535 {
1536 uint32_t result;
1537
1538 __ASM volatile ("shasx %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1539 return(result);
1540 }
1541
1542 __STATIC_FORCEINLINE uint32_t __UASX(uint32_t op1, uint32_t op2)
1543 {
1544 uint32_t result;
1545
1546 __ASM volatile ("uasx %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1547 return(result);
1548 }
1549
1550 __STATIC_FORCEINLINE uint32_t __UQASX(uint32_t op1, uint32_t op2)
1551 {
1552 uint32_t result;
1553
1554 __ASM volatile ("uqasx %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1555 return(result);
1556 }
1557
1558 __STATIC_FORCEINLINE uint32_t __UHASX(uint32_t op1, uint32_t op2)
1559 {
1560 uint32_t result;
1561
1562 __ASM volatile ("uhasx %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1563 return(result);
1564 }
1565
1566 __STATIC_FORCEINLINE uint32_t __SSAX(uint32_t op1, uint32_t op2)
1567 {
1568 uint32_t result;
1569
1570 __ASM volatile ("ssax %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1571 return(result);
1572 }
1573
1574 __STATIC_FORCEINLINE uint32_t __QSAX(uint32_t op1, uint32_t op2)
1575 {
1576 uint32_t result;
1577
1578 __ASM volatile ("qsax %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1579 return(result);
1580 }
1581
1582 __STATIC_FORCEINLINE uint32_t __SHSAX(uint32_t op1, uint32_t op2)
1583 {
1584 uint32_t result;
1585
1586 __ASM volatile ("shsax %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1587 return(result);
1588 }
1589
1590 __STATIC_FORCEINLINE uint32_t __USAX(uint32_t op1, uint32_t op2)
1591 {
1592 uint32_t result;
1593
1594 __ASM volatile ("usax %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1595 return(result);
1596 }
1597
1598 __STATIC_FORCEINLINE uint32_t __UQSAX(uint32_t op1, uint32_t op2)
1599 {
1600 uint32_t result;
1601
1602 __ASM volatile ("uqsax %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1603 return(result);
1604 }
1605
1606 __STATIC_FORCEINLINE uint32_t __UHSAX(uint32_t op1, uint32_t op2)
1607 {
1608 uint32_t result;
1609
1610 __ASM volatile ("uhsax %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1611 return(result);
1612 }
1613
1614 __STATIC_FORCEINLINE uint32_t __USAD8(uint32_t op1, uint32_t op2)
1615 {
1616 uint32_t result;
1617
1618 __ASM volatile ("usad8 %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1619 return(result);
1620 }
1621
1622 __STATIC_FORCEINLINE uint32_t __USADA8(uint32_t op1, uint32_t op2, uint32_t op3)
1623 {
1624 uint32_t result;
1625
1626 __ASM volatile ("usada8 %0, %1, %2, %3" : "=r" (result) : "r" (op1), "r" (op2), "r" (op3) );
1627 return(result);
1628 }
1629
1630 #define __SSAT16(ARG1,ARG2) \
1631 ({ \
1632 int32_t __RES, __ARG1 = (ARG1); \
1633 __ASM ("ssat16 %0, %1, %2" : "=r" (__RES) : "I" (ARG2), "r" (__ARG1) ); \
1634 __RES; \
1635 })
1636
1637 #define __USAT16(ARG1,ARG2) \
1638 ({ \
1639 uint32_t __RES, __ARG1 = (ARG1); \
1640 __ASM ("usat16 %0, %1, %2" : "=r" (__RES) : "I" (ARG2), "r" (__ARG1) ); \
1641 __RES; \
1642 })
1643
1644 __STATIC_FORCEINLINE uint32_t __UXTB16(uint32_t op1)
1645 {
1646 uint32_t result;
1647
1648 __ASM volatile ("uxtb16 %0, %1" : "=r" (result) : "r" (op1));
1649 return(result);
1650 }
1651
1652 __STATIC_FORCEINLINE uint32_t __UXTAB16(uint32_t op1, uint32_t op2)
1653 {
1654 uint32_t result;
1655
1656 __ASM volatile ("uxtab16 %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1657 return(result);
1658 }
1659
1660 __STATIC_FORCEINLINE uint32_t __SXTB16(uint32_t op1)
1661 {
1662 uint32_t result;
1663
1664 __ASM volatile ("sxtb16 %0, %1" : "=r" (result) : "r" (op1));
1665 return(result);
1666 }
1667
1668 __STATIC_FORCEINLINE uint32_t __SXTAB16(uint32_t op1, uint32_t op2)
1669 {
1670 uint32_t result;
1671
1672 __ASM volatile ("sxtab16 %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1673 return(result);
1674 }
1675
1676 __STATIC_FORCEINLINE uint32_t __SMUAD (uint32_t op1, uint32_t op2)
1677 {
1678 uint32_t result;
1679
1680 __ASM volatile ("smuad %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1681 return(result);
1682 }
1683
1684 __STATIC_FORCEINLINE uint32_t __SMUADX (uint32_t op1, uint32_t op2)
1685 {
1686 uint32_t result;
1687
1688 __ASM volatile ("smuadx %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1689 return(result);
1690 }
1691
1692 __STATIC_FORCEINLINE uint32_t __SMLAD (uint32_t op1, uint32_t op2, uint32_t op3)
1693 {
1694 uint32_t result;
1695
1696 __ASM volatile ("smlad %0, %1, %2, %3" : "=r" (result) : "r" (op1), "r" (op2), "r" (op3) );
1697 return(result);
1698 }
1699
1700 __STATIC_FORCEINLINE uint32_t __SMLADX (uint32_t op1, uint32_t op2, uint32_t op3)
1701 {
1702 uint32_t result;
1703
1704 __ASM volatile ("smladx %0, %1, %2, %3" : "=r" (result) : "r" (op1), "r" (op2), "r" (op3) );
1705 return(result);
1706 }
1707
1708 __STATIC_FORCEINLINE uint64_t __SMLALD (uint32_t op1, uint32_t op2, uint64_t acc)
1709 {
1710 union llreg_u{
1711 uint32_t w32[2];
1712 uint64_t w64;
1713 } llr;
1714 llr.w64 = acc;
1715
1716 #ifndef __ARMEB__ /* Little endian */
1717 __ASM volatile ("smlald %0, %1, %2, %3" : "=r" (llr.w32[0]), "=r" (llr.w32[1]): "r" (op1), "r" (op2) , "0" (llr.w32[0]), "1" (llr.w32[1]) );
1718 #else /* Big endian */
1719 __ASM volatile ("smlald %0, %1, %2, %3" : "=r" (llr.w32[1]), "=r" (llr.w32[0]): "r" (op1), "r" (op2) , "0" (llr.w32[1]), "1" (llr.w32[0]) );
1720 #endif
1721
1722 return(llr.w64);
1723 }
1724
1725 __STATIC_FORCEINLINE uint64_t __SMLALDX (uint32_t op1, uint32_t op2, uint64_t acc)
1726 {
1727 union llreg_u{
1728 uint32_t w32[2];
1729 uint64_t w64;
1730 } llr;
1731 llr.w64 = acc;
1732
1733 #ifndef __ARMEB__ /* Little endian */
1734 __ASM volatile ("smlaldx %0, %1, %2, %3" : "=r" (llr.w32[0]), "=r" (llr.w32[1]): "r" (op1), "r" (op2) , "0" (llr.w32[0]), "1" (llr.w32[1]) );
1735 #else /* Big endian */
1736 __ASM volatile ("smlaldx %0, %1, %2, %3" : "=r" (llr.w32[1]), "=r" (llr.w32[0]): "r" (op1), "r" (op2) , "0" (llr.w32[1]), "1" (llr.w32[0]) );
1737 #endif
1738
1739 return(llr.w64);
1740 }
1741
1742 __STATIC_FORCEINLINE uint32_t __SMUSD (uint32_t op1, uint32_t op2)
1743 {
1744 uint32_t result;
1745
1746 __ASM volatile ("smusd %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1747 return(result);
1748 }
1749
1750 __STATIC_FORCEINLINE uint32_t __SMUSDX (uint32_t op1, uint32_t op2)
1751 {
1752 uint32_t result;
1753
1754 __ASM volatile ("smusdx %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1755 return(result);
1756 }
1757
1758 __STATIC_FORCEINLINE uint32_t __SMLSD (uint32_t op1, uint32_t op2, uint32_t op3)
1759 {
1760 uint32_t result;
1761
1762 __ASM volatile ("smlsd %0, %1, %2, %3" : "=r" (result) : "r" (op1), "r" (op2), "r" (op3) );
1763 return(result);
1764 }
1765
1766 __STATIC_FORCEINLINE uint32_t __SMLSDX (uint32_t op1, uint32_t op2, uint32_t op3)
1767 {
1768 uint32_t result;
1769
1770 __ASM volatile ("smlsdx %0, %1, %2, %3" : "=r" (result) : "r" (op1), "r" (op2), "r" (op3) );
1771 return(result);
1772 }
1773
1774 __STATIC_FORCEINLINE uint64_t __SMLSLD (uint32_t op1, uint32_t op2, uint64_t acc)
1775 {
1776 union llreg_u{
1777 uint32_t w32[2];
1778 uint64_t w64;
1779 } llr;
1780 llr.w64 = acc;
1781
1782 #ifndef __ARMEB__ /* Little endian */
1783 __ASM volatile ("smlsld %0, %1, %2, %3" : "=r" (llr.w32[0]), "=r" (llr.w32[1]): "r" (op1), "r" (op2) , "0" (llr.w32[0]), "1" (llr.w32[1]) );
1784 #else /* Big endian */
1785 __ASM volatile ("smlsld %0, %1, %2, %3" : "=r" (llr.w32[1]), "=r" (llr.w32[0]): "r" (op1), "r" (op2) , "0" (llr.w32[1]), "1" (llr.w32[0]) );
1786 #endif
1787
1788 return(llr.w64);
1789 }
1790
1791 __STATIC_FORCEINLINE uint64_t __SMLSLDX (uint32_t op1, uint32_t op2, uint64_t acc)
1792 {
1793 union llreg_u{
1794 uint32_t w32[2];
1795 uint64_t w64;
1796 } llr;
1797 llr.w64 = acc;
1798
1799 #ifndef __ARMEB__ /* Little endian */
1800 __ASM volatile ("smlsldx %0, %1, %2, %3" : "=r" (llr.w32[0]), "=r" (llr.w32[1]): "r" (op1), "r" (op2) , "0" (llr.w32[0]), "1" (llr.w32[1]) );
1801 #else /* Big endian */
1802 __ASM volatile ("smlsldx %0, %1, %2, %3" : "=r" (llr.w32[1]), "=r" (llr.w32[0]): "r" (op1), "r" (op2) , "0" (llr.w32[1]), "1" (llr.w32[0]) );
1803 #endif
1804
1805 return(llr.w64);
1806 }
1807
1808 __STATIC_FORCEINLINE uint32_t __SEL (uint32_t op1, uint32_t op2)
1809 {
1810 uint32_t result;
1811
1812 __ASM volatile ("sel %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1813 return(result);
1814 }
1815
1816 __STATIC_FORCEINLINE int32_t __QADD( int32_t op1, int32_t op2)
1817 {
1818 int32_t result;
1819
1820 __ASM volatile ("qadd %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1821 return(result);
1822 }
1823
1824 __STATIC_FORCEINLINE int32_t __QSUB( int32_t op1, int32_t op2)
1825 {
1826 int32_t result;
1827
1828 __ASM volatile ("qsub %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1829 return(result);
1830 }
1831
1832 #if 0
1833 #define __PKHBT(ARG1,ARG2,ARG3) \
1834 ({ \
1835 uint32_t __RES, __ARG1 = (ARG1), __ARG2 = (ARG2); \
1836 __ASM ("pkhbt %0, %1, %2, lsl %3" : "=r" (__RES) : "r" (__ARG1), "r" (__ARG2), "I" (ARG3) ); \
1837 __RES; \
1838 })
1839
1840 #define __PKHTB(ARG1,ARG2,ARG3) \
1841 ({ \
1842 uint32_t __RES, __ARG1 = (ARG1), __ARG2 = (ARG2); \
1843 if (ARG3 == 0) \
1844 __ASM ("pkhtb %0, %1, %2" : "=r" (__RES) : "r" (__ARG1), "r" (__ARG2) ); \
1845 else \
1846 __ASM ("pkhtb %0, %1, %2, asr %3" : "=r" (__RES) : "r" (__ARG1), "r" (__ARG2), "I" (ARG3) ); \
1847 __RES; \
1848 })
1849 #endif
1850
1851 #define __PKHBT(ARG1,ARG2,ARG3) ( ((((uint32_t)(ARG1)) ) & 0x0000FFFFUL) | \
1852 ((((uint32_t)(ARG2)) << (ARG3)) & 0xFFFF0000UL) )
1853
1854 #define __PKHTB(ARG1,ARG2,ARG3) ( ((((uint32_t)(ARG1)) ) & 0xFFFF0000UL) | \
1855 ((((uint32_t)(ARG2)) >> (ARG3)) & 0x0000FFFFUL) )
1856
1857 __STATIC_FORCEINLINE int32_t __SMMLA (int32_t op1, int32_t op2, int32_t op3)
1858 {
1859 int32_t result;
1860
1861 __ASM volatile ("smmla %0, %1, %2, %3" : "=r" (result): "r" (op1), "r" (op2), "r" (op3) );
1862 return(result);
1863 }
1864
1865 #endif /* (__ARM_FEATURE_DSP == 1) */
1866
1869 #endif /* __CMSIS_ARMCLANG_H */
__get_CONTROL
__STATIC_INLINE uint32_t __get_CONTROL(void)
Enable IRQ Interrupts
Definition: cmsis_armcc.h:130
__get_IPSR
__STATIC_INLINE uint32_t __get_IPSR(void)
Get IPSR Register
Definition: cmsis_armcc.h:154
__USAT
__STATIC_FORCEINLINE uint32_t __USAT(int32_t val, uint32_t sat)
Unsigned Saturate
Definition: cmsis_armclang.h:1146
__get_PSP
__STATIC_INLINE uint32_t __get_PSP(void)
Get Process Stack Pointer
Definition: cmsis_armcc.h:190
__attribute__
__attribute__((section(".rev16_text"))) __STATIC_INLINE __ASM uint32_t __REV16(uint32_t value)
Reverse byte order (16 bit)
Definition: cmsis_armcc.h:463
__set_PSP
__STATIC_INLINE void __set_PSP(uint32_t topOfProcStack)
Set Process Stack Pointer
Definition: cmsis_armcc.h:202
__get_xPSR
__STATIC_INLINE uint32_t __get_xPSR(void)
Get xPSR Register
Definition: cmsis_armcc.h:178
__set_MSP
__STATIC_INLINE void __set_MSP(uint32_t topOfMainStack)
Set Main Stack Pointer
Definition: cmsis_armcc.h:226
__set_PRIMASK
__STATIC_INLINE void __set_PRIMASK(uint32_t priMask)
Set Priority Mask
Definition: cmsis_armcc.h:250
__get_APSR
__STATIC_INLINE uint32_t __get_APSR(void)
Get APSR Register
Definition: cmsis_armcc.h:166
__get_PRIMASK
__STATIC_INLINE uint32_t __get_PRIMASK(void)
Get Priority Mask
Definition: cmsis_armcc.h:238
__get_MSP
__STATIC_INLINE uint32_t __get_MSP(void)
Get Main Stack Pointer
Definition: cmsis_armcc.h:214
__ROR
__STATIC_FORCEINLINE uint32_t __ROR(uint32_t op1, uint32_t op2)
Rotate Right in unsigned value (32 bit)
Definition: cmsis_armclang.h:876
__set_CONTROL
__STATIC_INLINE void __set_CONTROL(uint32_t control)
Set Control Register
Definition: cmsis_armcc.h:142
__SSAT
__STATIC_FORCEINLINE int32_t __SSAT(int32_t val, uint32_t sat)
Signed Saturate
Definition: cmsis_armclang.h:1121