MG32L003 Standard Peripherals Firmware Library

成员变量
OWIRE_TypeDef结构体 参考
CMSIS » Mg32l003 » Device_Peripheral_peripherals

## 成员变量
__IOM uint32_t | CR
__IOM uint32_t | NFCR
__IOM uint32_t | RSTCNT
__IOM uint32_t | PRESCNT
__IOM uint32_t | BITRATECNT
__IOM uint32_t | DRVCNT
__IOM uint32_t | RDSMPCNT
__IOM uint32_t | RECCNT
__IOM uint32_t | DATA
__IOM uint32_t | CMD
__IOM uint32_t | INTEN
__IOM uint32_t | SR
__IOM uint32_t | INTCLR

## 结构体成员变量说明

## ◆ BITRATECNT

__IOM uint32_t BITRATECNT

One-wire bit rate design count register, Address offset: 0x010

## ◆ CMD

__IOM uint32_t CMD

One_wire bus operate command register, Address offset: 0x024

## ◆ CR

__IOM uint32_t CR

One-wire model control register, Address offset: 0x000

## ◆ DATA

__IOM uint32_t DATA

One_wire data register, Address offset: 0x020

## ◆ DRVCNT

__IOM uint32_t DRVCNT

One-wire main read/write pull0 drive time register, Address offset: 0x014

## ◆ INTCLR

__IOM uint32_t INTCLR

One-wire interrupt status clean register, Address offset: 0x030

## ◆ INTEN

__IOM uint32_t INTEN

One-wire interrupt enable register, Address offset: 0x028

## ◆ NFCR

__IOM uint32_t NFCR

One-wire input endpoint control register, Address offset: 0x004

## ◆ PRESCNT

__IOM uint32_t PRESCNT

One-wire device presence pulse count register, Address offset: 0x00C

## ◆ RDSMPCNT

__IOM uint32_t RDSMPCNT

One-wire main read sample time setting register, Address offset: 0x018

## ◆ RECCNT

__IOM uint32_t RECCNT

One-wire recover time count register, Address offset: 0x01C

## ◆ RSTCNT

__IOM uint32_t RSTCNT

One-wire master reset pulse count register, Address offset: 0x008

## ◆ SR

__IOM uint32_t SR

One-wire status register, Address offset: 0x02C

该结构体的文档由以下文件生成:

- mg32l003.h