MG32L003 Standard Peripherals Firmware Library

宏定义
RCC_HSI_Calibration_Config
MG32L003_StdPeriph_Driver » RCC » RCC_Exported_Constants

## 宏定义
#define | HSI24M_TRIM_ADDR ((uint32_t)0x180000A0)
#define | HSI22M_TRIM_ADDR ((uint32_t)0x180000A2)
#define | HSI16M_TRIM_ADDR ((uint32_t)0x180000A4)
#define | HSI8M_TRIM_ADDR ((uint32_t)0x180000A6)
#define | HSI4M_TRIM_ADDR ((uint32_t)0x180000A8)
#define | HSI24M_TC_ADDR ((uint32_t)0x18000090)
#define | HSI22M_TC_ADDR ((uint32_t)0x18000092)
#define | HSI16M_TC_ADDR ((uint32_t)0x18000094)
#define | HSI8M_TC_ADDR ((uint32_t)0x18000096)
#define | HSI4M_TC_ADDR ((uint32_t)0x18000098)
#define | RCC_HSITRIM_24M (*(uint16_t *)(HSI24M_TRIM_ADDR))
#define | RCC_HSITRIM_22M (*(uint16_t *)(HSI22M_TRIM_ADDR))
#define | RCC_HSITRIM_16M (*(uint16_t *)(HSI16M_TRIM_ADDR))
#define | RCC_HSITRIM_8M (*(uint16_t *)(HSI8M_TRIM_ADDR))
#define | RCC_HSITRIM_4M (*(uint16_t *)(HSI4M_TRIM_ADDR))
#define | RCC_HSITC_24M (*(uint16_t *)(HSI24M_TC_ADDR))
#define | RCC_HSITC_22M (*(uint16_t *)(HSI22M_TC_ADDR))
#define | RCC_HSITC_16M (*(uint16_t *)(HSI16M_TC_ADDR))
#define | RCC_HSITC_8M (*(uint16_t *)(HSI8M_TC_ADDR))
#define | RCC_HSITC_4M (*(uint16_t *)(HSI4M_TC_ADDR))
#define | RCC_HSICALIBRATION_DEFAULT ((uint32_t)0x00000312)

## 详细描述