MG32L003 Standard Peripherals Firmware Library

函数
BEEP_Private_Functions
MG32L003_StdPeriph_Driver » BEEP

## 函数
void | BEEP_DeInit (BEEP_TypeDef *BEEPx)
| Deinitializes the BEEP peripheral registers to their default reset values. 更多...
void | BEEP_Init (BEEP_TypeDef *BEEPx, BEEP_InitTypeDef *BEEP_InitStruct)
| Initializes the BEEP peripheral according to the specified parameters in the BEEP_InitStruct. 更多...
void | BEEP_Cmd (BEEP_TypeDef *BEEPx, FunctionalState NewState)
| Enables or disables BEEP peripheral. 更多...

## 详细描述

## 函数说明

## ◆ BEEP_Cmd()

void BEEP_Cmd | ( | BEEP_TypeDef * | BEEPx,
|  | FunctionalState | NewState
| ) |  |

Enables or disables BEEP peripheral.

参数

  BEEPx | Pointer to selected BEEP peripheral. This parameter can be one of the following values: BEEP.
  NewState | The new state of the BEEP peripheral. This parameter can be: ENABLE or DISABLE.

返回值

  None |

## ◆ BEEP_DeInit()

void BEEP_DeInit | ( | BEEP_TypeDef * | BEEPx | ) |

Deinitializes the BEEP peripheral registers to their default reset values.

参数

  BEEPx | Pointer to selected BEEP peripheral. This parameter can be one of the following values: BEEP.

返回值

  None |

## ◆ BEEP_Init()

void BEEP_Init | ( | BEEP_TypeDef * | BEEPx,
|  | BEEP_InitTypeDef * | BEEP_InitStruct
| ) |  |

Initializes the BEEP peripheral according to the specified parameters in the BEEP_InitStruct.

参数

  BEEPx | Pointer to selected BEEP peripheral. This parameter can be one of the following values: BEEP.
  BEEP_InitStruct | Pointer to BEEP initialization struct

返回值

  None |