/**
  @page ADC_Accumulation ADC atuto accumulation example
  
  @verbatim
  ****************** (C) COPYRIGHT 2023 megawin Technology *******************
  * @file    ADC/ADC_Accumulation/readme.txt 
  * @author  megawin Application Team
  * @version V0.0.5
  * @date    13-August-2024
  * @brief   Description of the ADC ADC_Accumulation example.
  ******************************************************************************
  * THE PRESENT FIRMWARE WHICH IS FOR GUIDANCE ONLY AIMS AT PROVIDING CUSTOMERS
  * WITH CODING INFORMATION REGARDING THEIR PRODUCTS IN ORDER FOR THEM TO SAVE
  * TIME. AS A RESULT, MEGAWIN SHALL NOT BE HELD LIABLE FOR ANY DIRECT,
  * INDIRECT OR CONSEQUENTIAL DAMAGES WITH RESPECT TO ANY CLAIMS ARISING FROM
  * THE CONTENT OF SUCH FIRMWARE AND/OR THE USE MADE BY CUSTOMERS OF THE
  * CODING INFORMATION CONTAINED HEREIN IN CONNECTION WITH THEIR PRODUCTS.
  ******************************************************************************
   @endverbatim

@par 例程描述 

本例程演示使用ADC的自动累加功能。

本例程系统时钟工作在24Mhz。

串口1按照如下配置：
- 波特率：115200
- 数据位：8

ADC被配置为自动积累采样通道0(PC6)转换结果的模式。


@par 目录内容 

  - ADC/ADC_Accumulation/ADC_Accumulation.uvprojx      MDK5工程文件
  - ADC/ADC_Accumulation/ADC_Accumulation.uvoptx       MDK5工程配置文件
  - ADC/ADC_Accumulation/JLinkSettings.ini             Jlink配置文件
  - ADC/ADC_Accumulation/main.c                        主程序


@par 硬件和软件环境 

  - 硬件平台搭建
    - 芯片管脚按如下连接：
      - UART1 (PD5, PD6) 连接到串口


@par 如何使用？ 

为了使程序工作，您必须执行以下操作 :
 - 使用 MDK5 打开此例程文件夹中的 ADC_Accumulation.uvprojx 工程
 - 重新编译该工程并下载到目标存储器中
 - 运行此例程
   
 * <h3><center>&copy; COPYRIGHT 2023 megawin Technology</center></h3>
 */
