MG32L003 Standard Peripherals Firmware Library

宏定义
VCMP_Filter_Clock_Selection
MG32L003_StdPeriph_Driver » VCMP » VCMP_Exported_Constants

## 宏定义
#define | VCMP_FILTER_CLK_NONE (0x00U)
#define | VCMP_FILTER_CLK_PCLK (0x01U << VCMP_CR1_VCMP_FLTCLK_SEL_Pos)
#define | VCMP_FILTER_CLK_LSI (0x02U << VCMP_CR1_VCMP_FLTCLK_SEL_Pos)
#define | IS_VCMP_FILTER_CLOCK(FILTER_CLOCK)

## 详细描述

## 宏定义说明

## ◆ IS_VCMP_FILTER_CLOCK

#define IS_VCMP_FILTER_CLOCK | ( |  | FILTER_CLOCK | ) |

值:
(((FILTER_CLOCK) == VCMP_FILTER_CLK_NONE) || \
((FILTER_CLOCK) == VCMP_FILTER_CLK_PCLK) || \
((FILTER_CLOCK) == VCMP_FILTER_CLK_LSI))
VCMP_FILTER_CLK_LSI
#define VCMP_FILTER_CLK_LSI
Definition: mg32l003_vcmp.h:120
VCMP_FILTER_CLK_PCLK
#define VCMP_FILTER_CLK_PCLK
Definition: mg32l003_vcmp.h:119
VCMP_FILTER_CLK_NONE
#define VCMP_FILTER_CLK_NONE
Definition: mg32l003_vcmp.h:118

## ◆ VCMP_FILTER_CLK_LSI

#define VCMP_FILTER_CLK_LSI (0x02U << VCMP_CR1_VCMP_FLTCLK_SEL_Pos)

VCMP Filter clock select LSI

## ◆ VCMP_FILTER_CLK_NONE

#define VCMP_FILTER_CLK_NONE (0x00U)

VCMP Filter clock select NONE

## ◆ VCMP_FILTER_CLK_PCLK

#define VCMP_FILTER_CLK_PCLK (0x01U << VCMP_CR1_VCMP_FLTCLK_SEL_Pos)

VCMP Filter clock select PCLK