MG32L003 Standard Peripherals Firmware Library

成员变量
TIM_TypeDef结构体 参考
CMSIS » Mg32l003 » Device_Peripheral_peripherals

## 成员变量
__IOM uint32_t | CR1
__IOM uint32_t | CR2
__IOM uint32_t | SMCR
__IOM uint32_t | DIER
__IOM uint32_t | SR
__IOM uint32_t | EGR
__IOM uint32_t | CCMR1
__IOM uint32_t | CCMR2
__IOM uint32_t | CCER
__IOM uint32_t | CNT
__IOM uint32_t | PSC
__IOM uint32_t | ARR
__IOM uint32_t | RCR
__IOM uint32_t | CCR1
__IOM uint32_t | CCR2
__IOM uint32_t | CCR3
__IOM uint32_t | CCR4
__IOM uint32_t | BDTR

## 结构体成员变量说明

## ◆ ARR

__IOM uint32_t ARR

TIM auto load register, Address offset: 0x02C

## ◆ BDTR

__IOM uint32_t BDTR

TIM brush and dead register, Address offset: 0x044

## ◆ CCER

__IOM uint32_t CCER

TIM captuer/compare enable register, Address offset: 0x020

## ◆ CCMR1

__IOM uint32_t CCMR1

TIM capture/compare mode register 1, Address offset: 0x018

## ◆ CCMR2

__IOM uint32_t CCMR2

TIM capture/compare mode register 2, Address offset: 0x01C

## ◆ CCR1

__IOM uint32_t CCR1

TIM captuer/compare register 1, Address offset: 0x034

## ◆ CCR2

__IOM uint32_t CCR2

TIM capture/compare register 2, Address offset: 0x038

## ◆ CCR3

__IOM uint32_t CCR3

TIM capture/compare register 3, Address offset: 0x03C

## ◆ CCR4

__IOM uint32_t CCR4

TIM capture/compare register 4, Address offset: 0x040

## ◆ CNT

__IOM uint32_t CNT

TIM count register, Address offset: 0x024

## ◆ CR1

__IOM uint32_t CR1

TIM control register 1, Address offset: 0x000

## ◆ CR2

__IOM uint32_t CR2

TIM control register 2, Address offset: 0x004

## ◆ DIER

__IOM uint32_t DIER

TIM interrupt enable register, Address offset: 0x00C

## ◆ EGR

__IOM uint32_t EGR

TIM event trig register, Address offset: 0x014

## ◆ PSC

__IOM uint32_t PSC

TIM prescale register, Address offset: 0x028

## ◆ RCR

__IOM uint32_t RCR

TIM repeate count register, Address offset: 0x030

## ◆ SMCR

__IOM uint32_t SMCR

TIM slave mode control register, Address offset: 0x008

## ◆ SR

__IOM uint32_t SR

TIM status register, Address offset: 0x010

该结构体的文档由以下文件生成:

- mg32l003.h