MG32L003 Standard Peripherals Firmware Library

成员变量
NVIC_Type结构体 参考
Defines and Type Definitions » Nested Vectored Interrupt Controller (NVIC)

Structure type to access the Nested Vectored Interrupt Controller (NVIC). 更多...

`#include <core_cm0plus.h>`

## 成员变量
__IOM uint32_t | ISER [1U]
uint32_t | RESERVED0 [31U]
__IOM uint32_t | ICER [1U]
uint32_t | RSERVED1 [31U]
__IOM uint32_t | ISPR [1U]
uint32_t | RESERVED2 [31U]
__IOM uint32_t | ICPR [1U]
uint32_t | RESERVED3 [31U]
uint32_t | RESERVED4 [64U]
__IOM uint32_t | IP [8U]

## 详细描述

Structure type to access the Nested Vectored Interrupt Controller (NVIC).

## 结构体成员变量说明

## ◆ ICER

__IOM uint32_t ICER[1U]

Offset: 0x080 (R/W) Interrupt Clear Enable Register

## ◆ ICPR

__IOM uint32_t ICPR[1U]

Offset: 0x180 (R/W) Interrupt Clear Pending Register

## ◆ IP

__IOM uint32_t IP[8U]

Offset: 0x300 (R/W) Interrupt Priority Register

## ◆ ISER

__IOM uint32_t ISER[1U]

Offset: 0x000 (R/W) Interrupt Set Enable Register

## ◆ ISPR

__IOM uint32_t ISPR[1U]

Offset: 0x100 (R/W) Interrupt Set Pending Register

该结构体的文档由以下文件生成:

- core_cm0plus.h