MG32L003 Standard Peripherals Firmware Library

cmsis_gcc.h
浏览该文件的文档.
1 /**************************************************************************/
7 /*
8 * Copyright (c) 2009-2018 Arm Limited. All rights reserved.
9 *
10 * SPDX-License-Identifier: Apache-2.0
11 *
12 * Licensed under the Apache License, Version 2.0 (the License); you may
13 * not use this file except in compliance with the License.
14 * You may obtain a copy of the License at
15 *
16 * www.apache.org/licenses/LICENSE-2.0
17 *
18 * Unless required by applicable law or agreed to in writing, software
19 * distributed under the License is distributed on an AS IS BASIS, WITHOUT
20 * WARRANTIES OR CONDITIONS OF ANY KIND, either express or implied.
21 * See the License for the specific language governing permissions and
22 * limitations under the License.
23 */
24
25 #ifndef __CMSIS_GCC_H
26 #define __CMSIS_GCC_H
27
28 /* ignore some GCC warnings */
29 #pragma GCC diagnostic push
30 #pragma GCC diagnostic ignored "-Wsign-conversion"
31 #pragma GCC diagnostic ignored "-Wconversion"
32 #pragma GCC diagnostic ignored "-Wunused-parameter"
33
34 /* Fallback for __has_builtin */
35 #ifndef __has_builtin
36 #define __has_builtin(x) (0)
37 #endif
38
39 /* CMSIS compiler specific defines */
40 #ifndef __ASM
41 #define __ASM __asm
42 #endif
43 #ifndef __INLINE
44 #define __INLINE inline
45 #endif
46 #ifndef __STATIC_INLINE
47 #define __STATIC_INLINE static inline
48 #endif
49 #ifndef __STATIC_FORCEINLINE
50 #define __STATIC_FORCEINLINE __attribute__((always_inline)) static inline
51 #endif
52 #ifndef __NO_RETURN
53 #define __NO_RETURN __attribute__((__noreturn__))
54 #endif
55 #ifndef __USED
56 #define __USED __attribute__((used))
57 #endif
58 #ifndef __WEAK
59 #define __WEAK __attribute__((weak))
60 #endif
61 #ifndef __PACKED
62 #define __PACKED __attribute__((packed, aligned(1)))
63 #endif
64 #ifndef __PACKED_STRUCT
65 #define __PACKED_STRUCT struct __attribute__((packed, aligned(1)))
66 #endif
67 #ifndef __PACKED_UNION
68 #define __PACKED_UNION union __attribute__((packed, aligned(1)))
69 #endif
70 #ifndef __UNALIGNED_UINT32 /* deprecated */
71 #pragma GCC diagnostic push
72 #pragma GCC diagnostic ignored "-Wpacked"
73 #pragma GCC diagnostic ignored "-Wattributes"
74 struct __attribute__((packed)) T_UINT32 { uint32_t v; };
75 #pragma GCC diagnostic pop
76 #define __UNALIGNED_UINT32(x) (((struct T_UINT32 *)(x))->v)
77 #endif
78 #ifndef __UNALIGNED_UINT16_WRITE
79 #pragma GCC diagnostic push
80 #pragma GCC diagnostic ignored "-Wpacked"
81 #pragma GCC diagnostic ignored "-Wattributes"
82 __PACKED_STRUCT T_UINT16_WRITE { uint16_t v; };
83 #pragma GCC diagnostic pop
84 #define __UNALIGNED_UINT16_WRITE(addr, val) (void)((((struct T_UINT16_WRITE *)(void *)(addr))->v) = (val))
85 #endif
86 #ifndef __UNALIGNED_UINT16_READ
87 #pragma GCC diagnostic push
88 #pragma GCC diagnostic ignored "-Wpacked"
89 #pragma GCC diagnostic ignored "-Wattributes"
90 __PACKED_STRUCT T_UINT16_READ { uint16_t v; };
91 #pragma GCC diagnostic pop
92 #define __UNALIGNED_UINT16_READ(addr) (((const struct T_UINT16_READ *)(const void *)(addr))->v)
93 #endif
94 #ifndef __UNALIGNED_UINT32_WRITE
95 #pragma GCC diagnostic push
96 #pragma GCC diagnostic ignored "-Wpacked"
97 #pragma GCC diagnostic ignored "-Wattributes"
98 __PACKED_STRUCT T_UINT32_WRITE { uint32_t v; };
99 #pragma GCC diagnostic pop
100 #define __UNALIGNED_UINT32_WRITE(addr, val) (void)((((struct T_UINT32_WRITE *)(void *)(addr))->v) = (val))
101 #endif
102 #ifndef __UNALIGNED_UINT32_READ
103 #pragma GCC diagnostic push
104 #pragma GCC diagnostic ignored "-Wpacked"
105 #pragma GCC diagnostic ignored "-Wattributes"
106 __PACKED_STRUCT T_UINT32_READ { uint32_t v; };
107 #pragma GCC diagnostic pop
108 #define __UNALIGNED_UINT32_READ(addr) (((const struct T_UINT32_READ *)(const void *)(addr))->v)
109 #endif
110 #ifndef __ALIGNED
111 #define __ALIGNED(x) __attribute__((aligned(x)))
112 #endif
113 #ifndef __RESTRICT
114 #define __RESTRICT __restrict
115 #endif
116
117
118 /* ########################### Core Function Access ########################### */
129 __STATIC_FORCEINLINE void __enable_irq(void)
130 {
131 __ASM volatile ("cpsie i" : : : "memory");
132 }
133
134
140 __STATIC_FORCEINLINE void __disable_irq(void)
141 {
142 __ASM volatile ("cpsid i" : : : "memory");
143 }
144
145
151 __STATIC_FORCEINLINE uint32_t __get_CONTROL(void)
152 {
153 uint32_t result;
154
155 __ASM volatile ("MRS %0, control" : "=r" (result) );
156 return(result);
157 }
158
159
160 #if (defined (__ARM_FEATURE_CMSE ) && (__ARM_FEATURE_CMSE == 3))
161
166 __STATIC_FORCEINLINE uint32_t __TZ_get_CONTROL_NS(void)
167 {
168 uint32_t result;
169
170 __ASM volatile ("MRS %0, control_ns" : "=r" (result) );
171 return(result);
172 }
173 #endif
174
175
181 __STATIC_FORCEINLINE void __set_CONTROL(uint32_t control)
182 {
183 __ASM volatile ("MSR control, %0" : : "r" (control) : "memory");
184 }
185
186
187 #if (defined (__ARM_FEATURE_CMSE ) && (__ARM_FEATURE_CMSE == 3))
188
193 __STATIC_FORCEINLINE void __TZ_set_CONTROL_NS(uint32_t control)
194 {
195 __ASM volatile ("MSR control_ns, %0" : : "r" (control) : "memory");
196 }
197 #endif
198
199
205 __STATIC_FORCEINLINE uint32_t __get_IPSR(void)
206 {
207 uint32_t result;
208
209 __ASM volatile ("MRS %0, ipsr" : "=r" (result) );
210 return(result);
211 }
212
213
219 __STATIC_FORCEINLINE uint32_t __get_APSR(void)
220 {
221 uint32_t result;
222
223 __ASM volatile ("MRS %0, apsr" : "=r" (result) );
224 return(result);
225 }
226
227
233 __STATIC_FORCEINLINE uint32_t __get_xPSR(void)
234 {
235 uint32_t result;
236
237 __ASM volatile ("MRS %0, xpsr" : "=r" (result) );
238 return(result);
239 }
240
241
247 __STATIC_FORCEINLINE uint32_t __get_PSP(void)
248 {
249 uint32_t result;
250
251 __ASM volatile ("MRS %0, psp" : "=r" (result) );
252 return(result);
253 }
254
255
256 #if (defined (__ARM_FEATURE_CMSE ) && (__ARM_FEATURE_CMSE == 3))
257
262 __STATIC_FORCEINLINE uint32_t __TZ_get_PSP_NS(void)
263 {
264 uint32_t result;
265
266 __ASM volatile ("MRS %0, psp_ns" : "=r" (result) );
267 return(result);
268 }
269 #endif
270
271
277 __STATIC_FORCEINLINE void __set_PSP(uint32_t topOfProcStack)
278 {
279 __ASM volatile ("MSR psp, %0" : : "r" (topOfProcStack) : );
280 }
281
282
283 #if (defined (__ARM_FEATURE_CMSE ) && (__ARM_FEATURE_CMSE == 3))
284
289 __STATIC_FORCEINLINE void __TZ_set_PSP_NS(uint32_t topOfProcStack)
290 {
291 __ASM volatile ("MSR psp_ns, %0" : : "r" (topOfProcStack) : );
292 }
293 #endif
294
295
301 __STATIC_FORCEINLINE uint32_t __get_MSP(void)
302 {
303 uint32_t result;
304
305 __ASM volatile ("MRS %0, msp" : "=r" (result) );
306 return(result);
307 }
308
309
310 #if (defined (__ARM_FEATURE_CMSE ) && (__ARM_FEATURE_CMSE == 3))
311
316 __STATIC_FORCEINLINE uint32_t __TZ_get_MSP_NS(void)
317 {
318 uint32_t result;
319
320 __ASM volatile ("MRS %0, msp_ns" : "=r" (result) );
321 return(result);
322 }
323 #endif
324
325
331 __STATIC_FORCEINLINE void __set_MSP(uint32_t topOfMainStack)
332 {
333 __ASM volatile ("MSR msp, %0" : : "r" (topOfMainStack) : );
334 }
335
336
337 #if (defined (__ARM_FEATURE_CMSE ) && (__ARM_FEATURE_CMSE == 3))
338
343 __STATIC_FORCEINLINE void __TZ_set_MSP_NS(uint32_t topOfMainStack)
344 {
345 __ASM volatile ("MSR msp_ns, %0" : : "r" (topOfMainStack) : );
346 }
347 #endif
348
349
350 #if (defined (__ARM_FEATURE_CMSE ) && (__ARM_FEATURE_CMSE == 3))
351
356 __STATIC_FORCEINLINE uint32_t __TZ_get_SP_NS(void)
357 {
358 uint32_t result;
359
360 __ASM volatile ("MRS %0, sp_ns" : "=r" (result) );
361 return(result);
362 }
363
364
370 __STATIC_FORCEINLINE void __TZ_set_SP_NS(uint32_t topOfStack)
371 {
372 __ASM volatile ("MSR sp_ns, %0" : : "r" (topOfStack) : );
373 }
374 #endif
375
376
382 __STATIC_FORCEINLINE uint32_t __get_PRIMASK(void)
383 {
384 uint32_t result;
385
386 __ASM volatile ("MRS %0, primask" : "=r" (result) :: "memory");
387 return(result);
388 }
389
390
391 #if (defined (__ARM_FEATURE_CMSE ) && (__ARM_FEATURE_CMSE == 3))
392
397 __STATIC_FORCEINLINE uint32_t __TZ_get_PRIMASK_NS(void)
398 {
399 uint32_t result;
400
401 __ASM volatile ("MRS %0, primask_ns" : "=r" (result) :: "memory");
402 return(result);
403 }
404 #endif
405
406
412 __STATIC_FORCEINLINE void __set_PRIMASK(uint32_t priMask)
413 {
414 __ASM volatile ("MSR primask, %0" : : "r" (priMask) : "memory");
415 }
416
417
418 #if (defined (__ARM_FEATURE_CMSE ) && (__ARM_FEATURE_CMSE == 3))
419
424 __STATIC_FORCEINLINE void __TZ_set_PRIMASK_NS(uint32_t priMask)
425 {
426 __ASM volatile ("MSR primask_ns, %0" : : "r" (priMask) : "memory");
427 }
428 #endif
429
430
431 #if ((defined (__ARM_ARCH_7M__ ) && (__ARM_ARCH_7M__ == 1)) || \
432 (defined (__ARM_ARCH_7EM__ ) && (__ARM_ARCH_7EM__ == 1)) || \
433 (defined (__ARM_ARCH_8M_MAIN__ ) && (__ARM_ARCH_8M_MAIN__ == 1)) )
434
439 __STATIC_FORCEINLINE void __enable_fault_irq(void)
440 {
441 __ASM volatile ("cpsie f" : : : "memory");
442 }
443
444
450 __STATIC_FORCEINLINE void __disable_fault_irq(void)
451 {
452 __ASM volatile ("cpsid f" : : : "memory");
453 }
454
455
461 __STATIC_FORCEINLINE uint32_t __get_BASEPRI(void)
462 {
463 uint32_t result;
464
465 __ASM volatile ("MRS %0, basepri" : "=r" (result) );
466 return(result);
467 }
468
469
470 #if (defined (__ARM_FEATURE_CMSE ) && (__ARM_FEATURE_CMSE == 3))
471
476 __STATIC_FORCEINLINE uint32_t __TZ_get_BASEPRI_NS(void)
477 {
478 uint32_t result;
479
480 __ASM volatile ("MRS %0, basepri_ns" : "=r" (result) );
481 return(result);
482 }
483 #endif
484
485
491 __STATIC_FORCEINLINE void __set_BASEPRI(uint32_t basePri)
492 {
493 __ASM volatile ("MSR basepri, %0" : : "r" (basePri) : "memory");
494 }
495
496
497 #if (defined (__ARM_FEATURE_CMSE ) && (__ARM_FEATURE_CMSE == 3))
498
503 __STATIC_FORCEINLINE void __TZ_set_BASEPRI_NS(uint32_t basePri)
504 {
505 __ASM volatile ("MSR basepri_ns, %0" : : "r" (basePri) : "memory");
506 }
507 #endif
508
509
516 __STATIC_FORCEINLINE void __set_BASEPRI_MAX(uint32_t basePri)
517 {
518 __ASM volatile ("MSR basepri_max, %0" : : "r" (basePri) : "memory");
519 }
520
521
527 __STATIC_FORCEINLINE uint32_t __get_FAULTMASK(void)
528 {
529 uint32_t result;
530
531 __ASM volatile ("MRS %0, faultmask" : "=r" (result) );
532 return(result);
533 }
534
535
536 #if (defined (__ARM_FEATURE_CMSE ) && (__ARM_FEATURE_CMSE == 3))
537
542 __STATIC_FORCEINLINE uint32_t __TZ_get_FAULTMASK_NS(void)
543 {
544 uint32_t result;
545
546 __ASM volatile ("MRS %0, faultmask_ns" : "=r" (result) );
547 return(result);
548 }
549 #endif
550
551
557 __STATIC_FORCEINLINE void __set_FAULTMASK(uint32_t faultMask)
558 {
559 __ASM volatile ("MSR faultmask, %0" : : "r" (faultMask) : "memory");
560 }
561
562
563 #if (defined (__ARM_FEATURE_CMSE ) && (__ARM_FEATURE_CMSE == 3))
564
569 __STATIC_FORCEINLINE void __TZ_set_FAULTMASK_NS(uint32_t faultMask)
570 {
571 __ASM volatile ("MSR faultmask_ns, %0" : : "r" (faultMask) : "memory");
572 }
573 #endif
574
575 #endif /* ((defined (__ARM_ARCH_7M__ ) && (__ARM_ARCH_7M__ == 1)) || \
576 (defined (__ARM_ARCH_7EM__ ) && (__ARM_ARCH_7EM__ == 1)) || \
577 (defined (__ARM_ARCH_8M_MAIN__ ) && (__ARM_ARCH_8M_MAIN__ == 1)) ) */
578
579
580 #if ((defined (__ARM_ARCH_8M_MAIN__ ) && (__ARM_ARCH_8M_MAIN__ == 1)) || \
581 (defined (__ARM_ARCH_8M_BASE__ ) && (__ARM_ARCH_8M_BASE__ == 1)) )
582
592 __STATIC_FORCEINLINE uint32_t __get_PSPLIM(void)
593 {
594 #if (!(defined (__ARM_ARCH_8M_MAIN__ ) && (__ARM_ARCH_8M_MAIN__ == 1)) && \
595 (!defined (__ARM_FEATURE_CMSE) || (__ARM_FEATURE_CMSE < 3)))
596 // without main extensions, the non-secure PSPLIM is RAZ/WI
597 return 0U;
598 #else
599 uint32_t result;
600 __ASM volatile ("MRS %0, psplim" : "=r" (result) );
601 return result;
602 #endif
603 }
604
605 #if (defined (__ARM_FEATURE_CMSE) && (__ARM_FEATURE_CMSE == 3))
606
614 __STATIC_FORCEINLINE uint32_t __TZ_get_PSPLIM_NS(void)
615 {
616 #if (!(defined (__ARM_ARCH_8M_MAIN__ ) && (__ARM_ARCH_8M_MAIN__ == 1)))
617 // without main extensions, the non-secure PSPLIM is RAZ/WI
618 return 0U;
619 #else
620 uint32_t result;
621 __ASM volatile ("MRS %0, psplim_ns" : "=r" (result) );
622 return result;
623 #endif
624 }
625 #endif
626
627
637 __STATIC_FORCEINLINE void __set_PSPLIM(uint32_t ProcStackPtrLimit)
638 {
639 #if (!(defined (__ARM_ARCH_8M_MAIN__ ) && (__ARM_ARCH_8M_MAIN__ == 1)) && \
640 (!defined (__ARM_FEATURE_CMSE) || (__ARM_FEATURE_CMSE < 3)))
641 // without main extensions, the non-secure PSPLIM is RAZ/WI
642 (void)ProcStackPtrLimit;
643 #else
644 __ASM volatile ("MSR psplim, %0" : : "r" (ProcStackPtrLimit));
645 #endif
646 }
647
648
649 #if (defined (__ARM_FEATURE_CMSE ) && (__ARM_FEATURE_CMSE == 3))
650
658 __STATIC_FORCEINLINE void __TZ_set_PSPLIM_NS(uint32_t ProcStackPtrLimit)
659 {
660 #if (!(defined (__ARM_ARCH_8M_MAIN__ ) && (__ARM_ARCH_8M_MAIN__ == 1)))
661 // without main extensions, the non-secure PSPLIM is RAZ/WI
662 (void)ProcStackPtrLimit;
663 #else
664 __ASM volatile ("MSR psplim_ns, %0\n" : : "r" (ProcStackPtrLimit));
665 #endif
666 }
667 #endif
668
669
679 __STATIC_FORCEINLINE uint32_t __get_MSPLIM(void)
680 {
681 #if (!(defined (__ARM_ARCH_8M_MAIN__ ) && (__ARM_ARCH_8M_MAIN__ == 1)) && \
682 (!defined (__ARM_FEATURE_CMSE) || (__ARM_FEATURE_CMSE < 3)))
683 // without main extensions, the non-secure MSPLIM is RAZ/WI
684 return 0U;
685 #else
686 uint32_t result;
687 __ASM volatile ("MRS %0, msplim" : "=r" (result) );
688 return result;
689 #endif
690 }
691
692
693 #if (defined (__ARM_FEATURE_CMSE ) && (__ARM_FEATURE_CMSE == 3))
694
702 __STATIC_FORCEINLINE uint32_t __TZ_get_MSPLIM_NS(void)
703 {
704 #if (!(defined (__ARM_ARCH_8M_MAIN__ ) && (__ARM_ARCH_8M_MAIN__ == 1)))
705 // without main extensions, the non-secure MSPLIM is RAZ/WI
706 return 0U;
707 #else
708 uint32_t result;
709 __ASM volatile ("MRS %0, msplim_ns" : "=r" (result) );
710 return result;
711 #endif
712 }
713 #endif
714
715
725 __STATIC_FORCEINLINE void __set_MSPLIM(uint32_t MainStackPtrLimit)
726 {
727 #if (!(defined (__ARM_ARCH_8M_MAIN__ ) && (__ARM_ARCH_8M_MAIN__ == 1)) && \
728 (!defined (__ARM_FEATURE_CMSE) || (__ARM_FEATURE_CMSE < 3)))
729 // without main extensions, the non-secure MSPLIM is RAZ/WI
730 (void)MainStackPtrLimit;
731 #else
732 __ASM volatile ("MSR msplim, %0" : : "r" (MainStackPtrLimit));
733 #endif
734 }
735
736
737 #if (defined (__ARM_FEATURE_CMSE ) && (__ARM_FEATURE_CMSE == 3))
738
746 __STATIC_FORCEINLINE void __TZ_set_MSPLIM_NS(uint32_t MainStackPtrLimit)
747 {
748 #if (!(defined (__ARM_ARCH_8M_MAIN__ ) && (__ARM_ARCH_8M_MAIN__ == 1)))
749 // without main extensions, the non-secure MSPLIM is RAZ/WI
750 (void)MainStackPtrLimit;
751 #else
752 __ASM volatile ("MSR msplim_ns, %0" : : "r" (MainStackPtrLimit));
753 #endif
754 }
755 #endif
756
757 #endif /* ((defined (__ARM_ARCH_8M_MAIN__ ) && (__ARM_ARCH_8M_MAIN__ == 1)) || \
758 (defined (__ARM_ARCH_8M_BASE__ ) && (__ARM_ARCH_8M_BASE__ == 1)) ) */
759
760
766 __STATIC_FORCEINLINE uint32_t __get_FPSCR(void)
767 {
768 #if ((defined (__FPU_PRESENT) && (__FPU_PRESENT == 1U)) && \
769 (defined (__FPU_USED ) && (__FPU_USED == 1U)) )
770 #if __has_builtin(__builtin_arm_get_fpscr)
771 // Re-enable using built-in when GCC has been fixed
772 // || (__GNUC__ > 7) || (__GNUC__ == 7 && __GNUC_MINOR__ >= 2)
773 /* see https://gcc.gnu.org/ml/gcc-patches/2017-04/msg00443.html */
774 return __builtin_arm_get_fpscr();
775 #else
776 uint32_t result;
777
778 __ASM volatile ("VMRS %0, fpscr" : "=r" (result) );
779 return(result);
780 #endif
781 #else
782 return(0U);
783 #endif
784 }
785
786
792 __STATIC_FORCEINLINE void __set_FPSCR(uint32_t fpscr)
793 {
794 #if ((defined (__FPU_PRESENT) && (__FPU_PRESENT == 1U)) && \
795 (defined (__FPU_USED ) && (__FPU_USED == 1U)) )
796 #if __has_builtin(__builtin_arm_set_fpscr)
797 // Re-enable using built-in when GCC has been fixed
798 // || (__GNUC__ > 7) || (__GNUC__ == 7 && __GNUC_MINOR__ >= 2)
799 /* see https://gcc.gnu.org/ml/gcc-patches/2017-04/msg00443.html */
800 __builtin_arm_set_fpscr(fpscr);
801 #else
802 __ASM volatile ("VMSR fpscr, %0" : : "r" (fpscr) : "vfpcc", "memory");
803 #endif
804 #else
805 (void)fpscr;
806 #endif
807 }
808
809
813 /* ########################## Core Instruction Access ######################### */
819 /* Define macros for porting to both thumb1 and thumb2.
820 * For thumb1, use low register (r0-r7), specified by constraint "l"
821 * Otherwise, use general registers, specified by constraint "r" */
822 #if defined (__thumb__) && !defined (__thumb2__)
823 #define __CMSIS_GCC_OUT_REG(r) "=l" (r)
824 #define __CMSIS_GCC_RW_REG(r) "+l" (r)
825 #define __CMSIS_GCC_USE_REG(r) "l" (r)
826 #else
827 #define __CMSIS_GCC_OUT_REG(r) "=r" (r)
828 #define __CMSIS_GCC_RW_REG(r) "+r" (r)
829 #define __CMSIS_GCC_USE_REG(r) "r" (r)
830 #endif
831
836 #define __NOP() __ASM volatile ("nop")
837
842 #define __WFI() __ASM volatile ("wfi")
843
844
850 #define __WFE() __ASM volatile ("wfe")
851
852
857 #define __SEV() __ASM volatile ("sev")
858
859
866 __STATIC_FORCEINLINE void __ISB(void)
867 {
868 __ASM volatile ("isb 0xF":::"memory");
869 }
870
871
877 __STATIC_FORCEINLINE void __DSB(void)
878 {
879 __ASM volatile ("dsb 0xF":::"memory");
880 }
881
882
888 __STATIC_FORCEINLINE void __DMB(void)
889 {
890 __ASM volatile ("dmb 0xF":::"memory");
891 }
892
893
900 __STATIC_FORCEINLINE uint32_t __REV(uint32_t value)
901 {
902 #if (__GNUC__ > 4) || (__GNUC__ == 4 && __GNUC_MINOR__ >= 5)
903 return __builtin_bswap32(value);
904 #else
905 uint32_t result;
906
907 __ASM volatile ("rev %0, %1" : __CMSIS_GCC_OUT_REG (result) : __CMSIS_GCC_USE_REG (value) );
908 return result;
909 #endif
910 }
911
912
919 __STATIC_FORCEINLINE uint32_t __REV16(uint32_t value)
920 {
921 uint32_t result;
922
923 __ASM volatile ("rev16 %0, %1" : __CMSIS_GCC_OUT_REG (result) : __CMSIS_GCC_USE_REG (value) );
924 return result;
925 }
926
927
934 __STATIC_FORCEINLINE int16_t __REVSH(int16_t value)
935 {
936 #if (__GNUC__ > 4) || (__GNUC__ == 4 && __GNUC_MINOR__ >= 8)
937 return (int16_t)__builtin_bswap16(value);
938 #else
939 int16_t result;
940
941 __ASM volatile ("revsh %0, %1" : __CMSIS_GCC_OUT_REG (result) : __CMSIS_GCC_USE_REG (value) );
942 return result;
943 #endif
944 }
945
946
954 __STATIC_FORCEINLINE uint32_t __ROR(uint32_t op1, uint32_t op2)
955 {
956 op2 %= 32U;
957 if (op2 == 0U)
958 {
959 return op1;
960 }
961 return (op1 >> op2) | (op1 << (32U - op2));
962 }
963
964
972 #define __BKPT(value) __ASM volatile ("bkpt "#value)
973
974
981 __STATIC_FORCEINLINE uint32_t __RBIT(uint32_t value)
982 {
983 uint32_t result;
984
985 #if ((defined (__ARM_ARCH_7M__ ) && (__ARM_ARCH_7M__ == 1)) || \
986 (defined (__ARM_ARCH_7EM__ ) && (__ARM_ARCH_7EM__ == 1)) || \
987 (defined (__ARM_ARCH_8M_MAIN__ ) && (__ARM_ARCH_8M_MAIN__ == 1)) )
988 __ASM volatile ("rbit %0, %1" : "=r" (result) : "r" (value) );
989 #else
990 uint32_t s = (4U /*sizeof(v)*/ * 8U) - 1U; /* extra shift needed at end */
991
992 result = value; /* r will be reversed bits of v; first get LSB of v */
993 for (value >>= 1U; value != 0U; value >>= 1U)
994 {
995 result <<= 1U;
996 result |= value & 1U;
997 s--;
998 }
999 result <<= s; /* shift when v's highest bits are zero */
1000 #endif
1001 return result;
1002 }
1003
1004
1011 #define __CLZ (uint8_t)__builtin_clz
1012
1013
1014 #if ((defined (__ARM_ARCH_7M__ ) && (__ARM_ARCH_7M__ == 1)) || \
1015 (defined (__ARM_ARCH_7EM__ ) && (__ARM_ARCH_7EM__ == 1)) || \
1016 (defined (__ARM_ARCH_8M_MAIN__ ) && (__ARM_ARCH_8M_MAIN__ == 1)) || \
1017 (defined (__ARM_ARCH_8M_BASE__ ) && (__ARM_ARCH_8M_BASE__ == 1)) )
1018
1024 __STATIC_FORCEINLINE uint8_t __LDREXB(volatile uint8_t *addr)
1025 {
1026 uint32_t result;
1027
1028 #if (__GNUC__ > 4) || (__GNUC__ == 4 && __GNUC_MINOR__ >= 8)
1029 __ASM volatile ("ldrexb %0, %1" : "=r" (result) : "Q" (*addr) );
1030 #else
1031 /* Prior to GCC 4.8, "Q" will be expanded to [rx, #0] which is not
1032 accepted by assembler. So has to use following less efficient pattern.
1033 */
1034 __ASM volatile ("ldrexb %0, [%1]" : "=r" (result) : "r" (addr) : "memory" );
1035 #endif
1036 return ((uint8_t) result); /* Add explicit type cast here */
1037 }
1038
1039
1046 __STATIC_FORCEINLINE uint16_t __LDREXH(volatile uint16_t *addr)
1047 {
1048 uint32_t result;
1049
1050 #if (__GNUC__ > 4) || (__GNUC__ == 4 && __GNUC_MINOR__ >= 8)
1051 __ASM volatile ("ldrexh %0, %1" : "=r" (result) : "Q" (*addr) );
1052 #else
1053 /* Prior to GCC 4.8, "Q" will be expanded to [rx, #0] which is not
1054 accepted by assembler. So has to use following less efficient pattern.
1055 */
1056 __ASM volatile ("ldrexh %0, [%1]" : "=r" (result) : "r" (addr) : "memory" );
1057 #endif
1058 return ((uint16_t) result); /* Add explicit type cast here */
1059 }
1060
1061
1068 __STATIC_FORCEINLINE uint32_t __LDREXW(volatile uint32_t *addr)
1069 {
1070 uint32_t result;
1071
1072 __ASM volatile ("ldrex %0, %1" : "=r" (result) : "Q" (*addr) );
1073 return(result);
1074 }
1075
1076
1085 __STATIC_FORCEINLINE uint32_t __STREXB(uint8_t value, volatile uint8_t *addr)
1086 {
1087 uint32_t result;
1088
1089 __ASM volatile ("strexb %0, %2, %1" : "=&r" (result), "=Q" (*addr) : "r" ((uint32_t)value) );
1090 return(result);
1091 }
1092
1093
1102 __STATIC_FORCEINLINE uint32_t __STREXH(uint16_t value, volatile uint16_t *addr)
1103 {
1104 uint32_t result;
1105
1106 __ASM volatile ("strexh %0, %2, %1" : "=&r" (result), "=Q" (*addr) : "r" ((uint32_t)value) );
1107 return(result);
1108 }
1109
1110
1119 __STATIC_FORCEINLINE uint32_t __STREXW(uint32_t value, volatile uint32_t *addr)
1120 {
1121 uint32_t result;
1122
1123 __ASM volatile ("strex %0, %2, %1" : "=&r" (result), "=Q" (*addr) : "r" (value) );
1124 return(result);
1125 }
1126
1127
1132 __STATIC_FORCEINLINE void __CLREX(void)
1133 {
1134 __ASM volatile ("clrex" ::: "memory");
1135 }
1136
1137 #endif /* ((defined (__ARM_ARCH_7M__ ) && (__ARM_ARCH_7M__ == 1)) || \
1138 (defined (__ARM_ARCH_7EM__ ) && (__ARM_ARCH_7EM__ == 1)) || \
1139 (defined (__ARM_ARCH_8M_MAIN__ ) && (__ARM_ARCH_8M_MAIN__ == 1)) || \
1140 (defined (__ARM_ARCH_8M_BASE__ ) && (__ARM_ARCH_8M_BASE__ == 1)) ) */
1141
1142
1143 #if ((defined (__ARM_ARCH_7M__ ) && (__ARM_ARCH_7M__ == 1)) || \
1144 (defined (__ARM_ARCH_7EM__ ) && (__ARM_ARCH_7EM__ == 1)) || \
1145 (defined (__ARM_ARCH_8M_MAIN__ ) && (__ARM_ARCH_8M_MAIN__ == 1)) )
1146
1153 #define __SSAT(ARG1,ARG2) \
1154 __extension__ \
1155 ({ \
1156 int32_t __RES, __ARG1 = (ARG1); \
1157 __ASM ("ssat %0, %1, %2" : "=r" (__RES) : "I" (ARG2), "r" (__ARG1) ); \
1158 __RES; \
1159 })
1160
1161
1169 #define __USAT(ARG1,ARG2) \
1170 __extension__ \
1171 ({ \
1172 uint32_t __RES, __ARG1 = (ARG1); \
1173 __ASM ("usat %0, %1, %2" : "=r" (__RES) : "I" (ARG2), "r" (__ARG1) ); \
1174 __RES; \
1175 })
1176
1177
1185 __STATIC_FORCEINLINE uint32_t __RRX(uint32_t value)
1186 {
1187 uint32_t result;
1188
1189 __ASM volatile ("rrx %0, %1" : __CMSIS_GCC_OUT_REG (result) : __CMSIS_GCC_USE_REG (value) );
1190 return(result);
1191 }
1192
1193
1200 __STATIC_FORCEINLINE uint8_t __LDRBT(volatile uint8_t *ptr)
1201 {
1202 uint32_t result;
1203
1204 #if (__GNUC__ > 4) || (__GNUC__ == 4 && __GNUC_MINOR__ >= 8)
1205 __ASM volatile ("ldrbt %0, %1" : "=r" (result) : "Q" (*ptr) );
1206 #else
1207 /* Prior to GCC 4.8, "Q" will be expanded to [rx, #0] which is not
1208 accepted by assembler. So has to use following less efficient pattern.
1209 */
1210 __ASM volatile ("ldrbt %0, [%1]" : "=r" (result) : "r" (ptr) : "memory" );
1211 #endif
1212 return ((uint8_t) result); /* Add explicit type cast here */
1213 }
1214
1215
1222 __STATIC_FORCEINLINE uint16_t __LDRHT(volatile uint16_t *ptr)
1223 {
1224 uint32_t result;
1225
1226 #if (__GNUC__ > 4) || (__GNUC__ == 4 && __GNUC_MINOR__ >= 8)
1227 __ASM volatile ("ldrht %0, %1" : "=r" (result) : "Q" (*ptr) );
1228 #else
1229 /* Prior to GCC 4.8, "Q" will be expanded to [rx, #0] which is not
1230 accepted by assembler. So has to use following less efficient pattern.
1231 */
1232 __ASM volatile ("ldrht %0, [%1]" : "=r" (result) : "r" (ptr) : "memory" );
1233 #endif
1234 return ((uint16_t) result); /* Add explicit type cast here */
1235 }
1236
1237
1244 __STATIC_FORCEINLINE uint32_t __LDRT(volatile uint32_t *ptr)
1245 {
1246 uint32_t result;
1247
1248 __ASM volatile ("ldrt %0, %1" : "=r" (result) : "Q" (*ptr) );
1249 return(result);
1250 }
1251
1252
1259 __STATIC_FORCEINLINE void __STRBT(uint8_t value, volatile uint8_t *ptr)
1260 {
1261 __ASM volatile ("strbt %1, %0" : "=Q" (*ptr) : "r" ((uint32_t)value) );
1262 }
1263
1264
1271 __STATIC_FORCEINLINE void __STRHT(uint16_t value, volatile uint16_t *ptr)
1272 {
1273 __ASM volatile ("strht %1, %0" : "=Q" (*ptr) : "r" ((uint32_t)value) );
1274 }
1275
1276
1283 __STATIC_FORCEINLINE void __STRT(uint32_t value, volatile uint32_t *ptr)
1284 {
1285 __ASM volatile ("strt %1, %0" : "=Q" (*ptr) : "r" (value) );
1286 }
1287
1288 #else /* ((defined (__ARM_ARCH_7M__ ) && (__ARM_ARCH_7M__ == 1)) || \
1289 (defined (__ARM_ARCH_7EM__ ) && (__ARM_ARCH_7EM__ == 1)) || \
1290 (defined (__ARM_ARCH_8M_MAIN__ ) && (__ARM_ARCH_8M_MAIN__ == 1)) ) */
1291
1299 __STATIC_FORCEINLINE int32_t __SSAT(int32_t val, uint32_t sat)
1300 {
1301 if ((sat >= 1U) && (sat <= 32U))
1302 {
1303 const int32_t max = (int32_t)((1U << (sat - 1U)) - 1U);
1304 const int32_t min = -1 - max ;
1305 if (val > max)
1306 {
1307 return max;
1308 }
1309 else if (val < min)
1310 {
1311 return min;
1312 }
1313 }
1314 return val;
1315 }
1316
1324 __STATIC_FORCEINLINE uint32_t __USAT(int32_t val, uint32_t sat)
1325 {
1326 if (sat <= 31U)
1327 {
1328 const uint32_t max = ((1U << sat) - 1U);
1329 if (val > (int32_t)max)
1330 {
1331 return max;
1332 }
1333 else if (val < 0)
1334 {
1335 return 0U;
1336 }
1337 }
1338 return (uint32_t)val;
1339 }
1340
1341 #endif /* ((defined (__ARM_ARCH_7M__ ) && (__ARM_ARCH_7M__ == 1)) || \
1342 (defined (__ARM_ARCH_7EM__ ) && (__ARM_ARCH_7EM__ == 1)) || \
1343 (defined (__ARM_ARCH_8M_MAIN__ ) && (__ARM_ARCH_8M_MAIN__ == 1)) ) */
1344
1345
1346 #if ((defined (__ARM_ARCH_8M_MAIN__ ) && (__ARM_ARCH_8M_MAIN__ == 1)) || \
1347 (defined (__ARM_ARCH_8M_BASE__ ) && (__ARM_ARCH_8M_BASE__ == 1)) )
1348
1354 __STATIC_FORCEINLINE uint8_t __LDAB(volatile uint8_t *ptr)
1355 {
1356 uint32_t result;
1357
1358 __ASM volatile ("ldab %0, %1" : "=r" (result) : "Q" (*ptr) );
1359 return ((uint8_t) result);
1360 }
1361
1362
1369 __STATIC_FORCEINLINE uint16_t __LDAH(volatile uint16_t *ptr)
1370 {
1371 uint32_t result;
1372
1373 __ASM volatile ("ldah %0, %1" : "=r" (result) : "Q" (*ptr) );
1374 return ((uint16_t) result);
1375 }
1376
1377
1384 __STATIC_FORCEINLINE uint32_t __LDA(volatile uint32_t *ptr)
1385 {
1386 uint32_t result;
1387
1388 __ASM volatile ("lda %0, %1" : "=r" (result) : "Q" (*ptr) );
1389 return(result);
1390 }
1391
1392
1399 __STATIC_FORCEINLINE void __STLB(uint8_t value, volatile uint8_t *ptr)
1400 {
1401 __ASM volatile ("stlb %1, %0" : "=Q" (*ptr) : "r" ((uint32_t)value) );
1402 }
1403
1404
1411 __STATIC_FORCEINLINE void __STLH(uint16_t value, volatile uint16_t *ptr)
1412 {
1413 __ASM volatile ("stlh %1, %0" : "=Q" (*ptr) : "r" ((uint32_t)value) );
1414 }
1415
1416
1423 __STATIC_FORCEINLINE void __STL(uint32_t value, volatile uint32_t *ptr)
1424 {
1425 __ASM volatile ("stl %1, %0" : "=Q" (*ptr) : "r" ((uint32_t)value) );
1426 }
1427
1428
1435 __STATIC_FORCEINLINE uint8_t __LDAEXB(volatile uint8_t *ptr)
1436 {
1437 uint32_t result;
1438
1439 __ASM volatile ("ldaexb %0, %1" : "=r" (result) : "Q" (*ptr) );
1440 return ((uint8_t) result);
1441 }
1442
1443
1450 __STATIC_FORCEINLINE uint16_t __LDAEXH(volatile uint16_t *ptr)
1451 {
1452 uint32_t result;
1453
1454 __ASM volatile ("ldaexh %0, %1" : "=r" (result) : "Q" (*ptr) );
1455 return ((uint16_t) result);
1456 }
1457
1458
1465 __STATIC_FORCEINLINE uint32_t __LDAEX(volatile uint32_t *ptr)
1466 {
1467 uint32_t result;
1468
1469 __ASM volatile ("ldaex %0, %1" : "=r" (result) : "Q" (*ptr) );
1470 return(result);
1471 }
1472
1473
1482 __STATIC_FORCEINLINE uint32_t __STLEXB(uint8_t value, volatile uint8_t *ptr)
1483 {
1484 uint32_t result;
1485
1486 __ASM volatile ("stlexb %0, %2, %1" : "=&r" (result), "=Q" (*ptr) : "r" ((uint32_t)value) );
1487 return(result);
1488 }
1489
1490
1499 __STATIC_FORCEINLINE uint32_t __STLEXH(uint16_t value, volatile uint16_t *ptr)
1500 {
1501 uint32_t result;
1502
1503 __ASM volatile ("stlexh %0, %2, %1" : "=&r" (result), "=Q" (*ptr) : "r" ((uint32_t)value) );
1504 return(result);
1505 }
1506
1507
1516 __STATIC_FORCEINLINE uint32_t __STLEX(uint32_t value, volatile uint32_t *ptr)
1517 {
1518 uint32_t result;
1519
1520 __ASM volatile ("stlex %0, %2, %1" : "=&r" (result), "=Q" (*ptr) : "r" ((uint32_t)value) );
1521 return(result);
1522 }
1523
1524 #endif /* ((defined (__ARM_ARCH_8M_MAIN__ ) && (__ARM_ARCH_8M_MAIN__ == 1)) || \
1525 (defined (__ARM_ARCH_8M_BASE__ ) && (__ARM_ARCH_8M_BASE__ == 1)) ) */
1526 /* end of group CMSIS_Core_InstructionInterface */
1528
1529
1530 /* ################### Compiler specific Intrinsics ########################### */
1536 #if (defined (__ARM_FEATURE_DSP) && (__ARM_FEATURE_DSP == 1))
1537
1538 __STATIC_FORCEINLINE uint32_t __SADD8(uint32_t op1, uint32_t op2)
1539 {
1540 uint32_t result;
1541
1542 __ASM volatile ("sadd8 %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1543 return(result);
1544 }
1545
1546 __STATIC_FORCEINLINE uint32_t __QADD8(uint32_t op1, uint32_t op2)
1547 {
1548 uint32_t result;
1549
1550 __ASM volatile ("qadd8 %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1551 return(result);
1552 }
1553
1554 __STATIC_FORCEINLINE uint32_t __SHADD8(uint32_t op1, uint32_t op2)
1555 {
1556 uint32_t result;
1557
1558 __ASM volatile ("shadd8 %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1559 return(result);
1560 }
1561
1562 __STATIC_FORCEINLINE uint32_t __UADD8(uint32_t op1, uint32_t op2)
1563 {
1564 uint32_t result;
1565
1566 __ASM volatile ("uadd8 %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1567 return(result);
1568 }
1569
1570 __STATIC_FORCEINLINE uint32_t __UQADD8(uint32_t op1, uint32_t op2)
1571 {
1572 uint32_t result;
1573
1574 __ASM volatile ("uqadd8 %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1575 return(result);
1576 }
1577
1578 __STATIC_FORCEINLINE uint32_t __UHADD8(uint32_t op1, uint32_t op2)
1579 {
1580 uint32_t result;
1581
1582 __ASM volatile ("uhadd8 %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1583 return(result);
1584 }
1585
1586
1587 __STATIC_FORCEINLINE uint32_t __SSUB8(uint32_t op1, uint32_t op2)
1588 {
1589 uint32_t result;
1590
1591 __ASM volatile ("ssub8 %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1592 return(result);
1593 }
1594
1595 __STATIC_FORCEINLINE uint32_t __QSUB8(uint32_t op1, uint32_t op2)
1596 {
1597 uint32_t result;
1598
1599 __ASM volatile ("qsub8 %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1600 return(result);
1601 }
1602
1603 __STATIC_FORCEINLINE uint32_t __SHSUB8(uint32_t op1, uint32_t op2)
1604 {
1605 uint32_t result;
1606
1607 __ASM volatile ("shsub8 %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1608 return(result);
1609 }
1610
1611 __STATIC_FORCEINLINE uint32_t __USUB8(uint32_t op1, uint32_t op2)
1612 {
1613 uint32_t result;
1614
1615 __ASM volatile ("usub8 %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1616 return(result);
1617 }
1618
1619 __STATIC_FORCEINLINE uint32_t __UQSUB8(uint32_t op1, uint32_t op2)
1620 {
1621 uint32_t result;
1622
1623 __ASM volatile ("uqsub8 %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1624 return(result);
1625 }
1626
1627 __STATIC_FORCEINLINE uint32_t __UHSUB8(uint32_t op1, uint32_t op2)
1628 {
1629 uint32_t result;
1630
1631 __ASM volatile ("uhsub8 %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1632 return(result);
1633 }
1634
1635
1636 __STATIC_FORCEINLINE uint32_t __SADD16(uint32_t op1, uint32_t op2)
1637 {
1638 uint32_t result;
1639
1640 __ASM volatile ("sadd16 %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1641 return(result);
1642 }
1643
1644 __STATIC_FORCEINLINE uint32_t __QADD16(uint32_t op1, uint32_t op2)
1645 {
1646 uint32_t result;
1647
1648 __ASM volatile ("qadd16 %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1649 return(result);
1650 }
1651
1652 __STATIC_FORCEINLINE uint32_t __SHADD16(uint32_t op1, uint32_t op2)
1653 {
1654 uint32_t result;
1655
1656 __ASM volatile ("shadd16 %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1657 return(result);
1658 }
1659
1660 __STATIC_FORCEINLINE uint32_t __UADD16(uint32_t op1, uint32_t op2)
1661 {
1662 uint32_t result;
1663
1664 __ASM volatile ("uadd16 %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1665 return(result);
1666 }
1667
1668 __STATIC_FORCEINLINE uint32_t __UQADD16(uint32_t op1, uint32_t op2)
1669 {
1670 uint32_t result;
1671
1672 __ASM volatile ("uqadd16 %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1673 return(result);
1674 }
1675
1676 __STATIC_FORCEINLINE uint32_t __UHADD16(uint32_t op1, uint32_t op2)
1677 {
1678 uint32_t result;
1679
1680 __ASM volatile ("uhadd16 %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1681 return(result);
1682 }
1683
1684 __STATIC_FORCEINLINE uint32_t __SSUB16(uint32_t op1, uint32_t op2)
1685 {
1686 uint32_t result;
1687
1688 __ASM volatile ("ssub16 %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1689 return(result);
1690 }
1691
1692 __STATIC_FORCEINLINE uint32_t __QSUB16(uint32_t op1, uint32_t op2)
1693 {
1694 uint32_t result;
1695
1696 __ASM volatile ("qsub16 %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1697 return(result);
1698 }
1699
1700 __STATIC_FORCEINLINE uint32_t __SHSUB16(uint32_t op1, uint32_t op2)
1701 {
1702 uint32_t result;
1703
1704 __ASM volatile ("shsub16 %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1705 return(result);
1706 }
1707
1708 __STATIC_FORCEINLINE uint32_t __USUB16(uint32_t op1, uint32_t op2)
1709 {
1710 uint32_t result;
1711
1712 __ASM volatile ("usub16 %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1713 return(result);
1714 }
1715
1716 __STATIC_FORCEINLINE uint32_t __UQSUB16(uint32_t op1, uint32_t op2)
1717 {
1718 uint32_t result;
1719
1720 __ASM volatile ("uqsub16 %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1721 return(result);
1722 }
1723
1724 __STATIC_FORCEINLINE uint32_t __UHSUB16(uint32_t op1, uint32_t op2)
1725 {
1726 uint32_t result;
1727
1728 __ASM volatile ("uhsub16 %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1729 return(result);
1730 }
1731
1732 __STATIC_FORCEINLINE uint32_t __SASX(uint32_t op1, uint32_t op2)
1733 {
1734 uint32_t result;
1735
1736 __ASM volatile ("sasx %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1737 return(result);
1738 }
1739
1740 __STATIC_FORCEINLINE uint32_t __QASX(uint32_t op1, uint32_t op2)
1741 {
1742 uint32_t result;
1743
1744 __ASM volatile ("qasx %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1745 return(result);
1746 }
1747
1748 __STATIC_FORCEINLINE uint32_t __SHASX(uint32_t op1, uint32_t op2)
1749 {
1750 uint32_t result;
1751
1752 __ASM volatile ("shasx %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1753 return(result);
1754 }
1755
1756 __STATIC_FORCEINLINE uint32_t __UASX(uint32_t op1, uint32_t op2)
1757 {
1758 uint32_t result;
1759
1760 __ASM volatile ("uasx %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1761 return(result);
1762 }
1763
1764 __STATIC_FORCEINLINE uint32_t __UQASX(uint32_t op1, uint32_t op2)
1765 {
1766 uint32_t result;
1767
1768 __ASM volatile ("uqasx %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1769 return(result);
1770 }
1771
1772 __STATIC_FORCEINLINE uint32_t __UHASX(uint32_t op1, uint32_t op2)
1773 {
1774 uint32_t result;
1775
1776 __ASM volatile ("uhasx %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1777 return(result);
1778 }
1779
1780 __STATIC_FORCEINLINE uint32_t __SSAX(uint32_t op1, uint32_t op2)
1781 {
1782 uint32_t result;
1783
1784 __ASM volatile ("ssax %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1785 return(result);
1786 }
1787
1788 __STATIC_FORCEINLINE uint32_t __QSAX(uint32_t op1, uint32_t op2)
1789 {
1790 uint32_t result;
1791
1792 __ASM volatile ("qsax %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1793 return(result);
1794 }
1795
1796 __STATIC_FORCEINLINE uint32_t __SHSAX(uint32_t op1, uint32_t op2)
1797 {
1798 uint32_t result;
1799
1800 __ASM volatile ("shsax %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1801 return(result);
1802 }
1803
1804 __STATIC_FORCEINLINE uint32_t __USAX(uint32_t op1, uint32_t op2)
1805 {
1806 uint32_t result;
1807
1808 __ASM volatile ("usax %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1809 return(result);
1810 }
1811
1812 __STATIC_FORCEINLINE uint32_t __UQSAX(uint32_t op1, uint32_t op2)
1813 {
1814 uint32_t result;
1815
1816 __ASM volatile ("uqsax %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1817 return(result);
1818 }
1819
1820 __STATIC_FORCEINLINE uint32_t __UHSAX(uint32_t op1, uint32_t op2)
1821 {
1822 uint32_t result;
1823
1824 __ASM volatile ("uhsax %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1825 return(result);
1826 }
1827
1828 __STATIC_FORCEINLINE uint32_t __USAD8(uint32_t op1, uint32_t op2)
1829 {
1830 uint32_t result;
1831
1832 __ASM volatile ("usad8 %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1833 return(result);
1834 }
1835
1836 __STATIC_FORCEINLINE uint32_t __USADA8(uint32_t op1, uint32_t op2, uint32_t op3)
1837 {
1838 uint32_t result;
1839
1840 __ASM volatile ("usada8 %0, %1, %2, %3" : "=r" (result) : "r" (op1), "r" (op2), "r" (op3) );
1841 return(result);
1842 }
1843
1844 #define __SSAT16(ARG1,ARG2) \
1845 ({ \
1846 int32_t __RES, __ARG1 = (ARG1); \
1847 __ASM ("ssat16 %0, %1, %2" : "=r" (__RES) : "I" (ARG2), "r" (__ARG1) ); \
1848 __RES; \
1849 })
1850
1851 #define __USAT16(ARG1,ARG2) \
1852 ({ \
1853 uint32_t __RES, __ARG1 = (ARG1); \
1854 __ASM ("usat16 %0, %1, %2" : "=r" (__RES) : "I" (ARG2), "r" (__ARG1) ); \
1855 __RES; \
1856 })
1857
1858 __STATIC_FORCEINLINE uint32_t __UXTB16(uint32_t op1)
1859 {
1860 uint32_t result;
1861
1862 __ASM volatile ("uxtb16 %0, %1" : "=r" (result) : "r" (op1));
1863 return(result);
1864 }
1865
1866 __STATIC_FORCEINLINE uint32_t __UXTAB16(uint32_t op1, uint32_t op2)
1867 {
1868 uint32_t result;
1869
1870 __ASM volatile ("uxtab16 %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1871 return(result);
1872 }
1873
1874 __STATIC_FORCEINLINE uint32_t __SXTB16(uint32_t op1)
1875 {
1876 uint32_t result;
1877
1878 __ASM volatile ("sxtb16 %0, %1" : "=r" (result) : "r" (op1));
1879 return(result);
1880 }
1881
1882 __STATIC_FORCEINLINE uint32_t __SXTAB16(uint32_t op1, uint32_t op2)
1883 {
1884 uint32_t result;
1885
1886 __ASM volatile ("sxtab16 %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1887 return(result);
1888 }
1889
1890 __STATIC_FORCEINLINE uint32_t __SMUAD (uint32_t op1, uint32_t op2)
1891 {
1892 uint32_t result;
1893
1894 __ASM volatile ("smuad %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1895 return(result);
1896 }
1897
1898 __STATIC_FORCEINLINE uint32_t __SMUADX (uint32_t op1, uint32_t op2)
1899 {
1900 uint32_t result;
1901
1902 __ASM volatile ("smuadx %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1903 return(result);
1904 }
1905
1906 __STATIC_FORCEINLINE uint32_t __SMLAD (uint32_t op1, uint32_t op2, uint32_t op3)
1907 {
1908 uint32_t result;
1909
1910 __ASM volatile ("smlad %0, %1, %2, %3" : "=r" (result) : "r" (op1), "r" (op2), "r" (op3) );
1911 return(result);
1912 }
1913
1914 __STATIC_FORCEINLINE uint32_t __SMLADX (uint32_t op1, uint32_t op2, uint32_t op3)
1915 {
1916 uint32_t result;
1917
1918 __ASM volatile ("smladx %0, %1, %2, %3" : "=r" (result) : "r" (op1), "r" (op2), "r" (op3) );
1919 return(result);
1920 }
1921
1922 __STATIC_FORCEINLINE uint64_t __SMLALD (uint32_t op1, uint32_t op2, uint64_t acc)
1923 {
1924 union llreg_u{
1925 uint32_t w32[2];
1926 uint64_t w64;
1927 } llr;
1928 llr.w64 = acc;
1929
1930 #ifndef __ARMEB__ /* Little endian */
1931 __ASM volatile ("smlald %0, %1, %2, %3" : "=r" (llr.w32[0]), "=r" (llr.w32[1]): "r" (op1), "r" (op2) , "0" (llr.w32[0]), "1" (llr.w32[1]) );
1932 #else /* Big endian */
1933 __ASM volatile ("smlald %0, %1, %2, %3" : "=r" (llr.w32[1]), "=r" (llr.w32[0]): "r" (op1), "r" (op2) , "0" (llr.w32[1]), "1" (llr.w32[0]) );
1934 #endif
1935
1936 return(llr.w64);
1937 }
1938
1939 __STATIC_FORCEINLINE uint64_t __SMLALDX (uint32_t op1, uint32_t op2, uint64_t acc)
1940 {
1941 union llreg_u{
1942 uint32_t w32[2];
1943 uint64_t w64;
1944 } llr;
1945 llr.w64 = acc;
1946
1947 #ifndef __ARMEB__ /* Little endian */
1948 __ASM volatile ("smlaldx %0, %1, %2, %3" : "=r" (llr.w32[0]), "=r" (llr.w32[1]): "r" (op1), "r" (op2) , "0" (llr.w32[0]), "1" (llr.w32[1]) );
1949 #else /* Big endian */
1950 __ASM volatile ("smlaldx %0, %1, %2, %3" : "=r" (llr.w32[1]), "=r" (llr.w32[0]): "r" (op1), "r" (op2) , "0" (llr.w32[1]), "1" (llr.w32[0]) );
1951 #endif
1952
1953 return(llr.w64);
1954 }
1955
1956 __STATIC_FORCEINLINE uint32_t __SMUSD (uint32_t op1, uint32_t op2)
1957 {
1958 uint32_t result;
1959
1960 __ASM volatile ("smusd %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1961 return(result);
1962 }
1963
1964 __STATIC_FORCEINLINE uint32_t __SMUSDX (uint32_t op1, uint32_t op2)
1965 {
1966 uint32_t result;
1967
1968 __ASM volatile ("smusdx %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
1969 return(result);
1970 }
1971
1972 __STATIC_FORCEINLINE uint32_t __SMLSD (uint32_t op1, uint32_t op2, uint32_t op3)
1973 {
1974 uint32_t result;
1975
1976 __ASM volatile ("smlsd %0, %1, %2, %3" : "=r" (result) : "r" (op1), "r" (op2), "r" (op3) );
1977 return(result);
1978 }
1979
1980 __STATIC_FORCEINLINE uint32_t __SMLSDX (uint32_t op1, uint32_t op2, uint32_t op3)
1981 {
1982 uint32_t result;
1983
1984 __ASM volatile ("smlsdx %0, %1, %2, %3" : "=r" (result) : "r" (op1), "r" (op2), "r" (op3) );
1985 return(result);
1986 }
1987
1988 __STATIC_FORCEINLINE uint64_t __SMLSLD (uint32_t op1, uint32_t op2, uint64_t acc)
1989 {
1990 union llreg_u{
1991 uint32_t w32[2];
1992 uint64_t w64;
1993 } llr;
1994 llr.w64 = acc;
1995
1996 #ifndef __ARMEB__ /* Little endian */
1997 __ASM volatile ("smlsld %0, %1, %2, %3" : "=r" (llr.w32[0]), "=r" (llr.w32[1]): "r" (op1), "r" (op2) , "0" (llr.w32[0]), "1" (llr.w32[1]) );
1998 #else /* Big endian */
1999 __ASM volatile ("smlsld %0, %1, %2, %3" : "=r" (llr.w32[1]), "=r" (llr.w32[0]): "r" (op1), "r" (op2) , "0" (llr.w32[1]), "1" (llr.w32[0]) );
2000 #endif
2001
2002 return(llr.w64);
2003 }
2004
2005 __STATIC_FORCEINLINE uint64_t __SMLSLDX (uint32_t op1, uint32_t op2, uint64_t acc)
2006 {
2007 union llreg_u{
2008 uint32_t w32[2];
2009 uint64_t w64;
2010 } llr;
2011 llr.w64 = acc;
2012
2013 #ifndef __ARMEB__ /* Little endian */
2014 __ASM volatile ("smlsldx %0, %1, %2, %3" : "=r" (llr.w32[0]), "=r" (llr.w32[1]): "r" (op1), "r" (op2) , "0" (llr.w32[0]), "1" (llr.w32[1]) );
2015 #else /* Big endian */
2016 __ASM volatile ("smlsldx %0, %1, %2, %3" : "=r" (llr.w32[1]), "=r" (llr.w32[0]): "r" (op1), "r" (op2) , "0" (llr.w32[1]), "1" (llr.w32[0]) );
2017 #endif
2018
2019 return(llr.w64);
2020 }
2021
2022 __STATIC_FORCEINLINE uint32_t __SEL (uint32_t op1, uint32_t op2)
2023 {
2024 uint32_t result;
2025
2026 __ASM volatile ("sel %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
2027 return(result);
2028 }
2029
2030 __STATIC_FORCEINLINE int32_t __QADD( int32_t op1, int32_t op2)
2031 {
2032 int32_t result;
2033
2034 __ASM volatile ("qadd %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
2035 return(result);
2036 }
2037
2038 __STATIC_FORCEINLINE int32_t __QSUB( int32_t op1, int32_t op2)
2039 {
2040 int32_t result;
2041
2042 __ASM volatile ("qsub %0, %1, %2" : "=r" (result) : "r" (op1), "r" (op2) );
2043 return(result);
2044 }
2045
2046 #if 0
2047 #define __PKHBT(ARG1,ARG2,ARG3) \
2048 ({ \
2049 uint32_t __RES, __ARG1 = (ARG1), __ARG2 = (ARG2); \
2050 __ASM ("pkhbt %0, %1, %2, lsl %3" : "=r" (__RES) : "r" (__ARG1), "r" (__ARG2), "I" (ARG3) ); \
2051 __RES; \
2052 })
2053
2054 #define __PKHTB(ARG1,ARG2,ARG3) \
2055 ({ \
2056 uint32_t __RES, __ARG1 = (ARG1), __ARG2 = (ARG2); \
2057 if (ARG3 == 0) \
2058 __ASM ("pkhtb %0, %1, %2" : "=r" (__RES) : "r" (__ARG1), "r" (__ARG2) ); \
2059 else \
2060 __ASM ("pkhtb %0, %1, %2, asr %3" : "=r" (__RES) : "r" (__ARG1), "r" (__ARG2), "I" (ARG3) ); \
2061 __RES; \
2062 })
2063 #endif
2064
2065 #define __PKHBT(ARG1,ARG2,ARG3) ( ((((uint32_t)(ARG1)) ) & 0x0000FFFFUL) | \
2066 ((((uint32_t)(ARG2)) << (ARG3)) & 0xFFFF0000UL) )
2067
2068 #define __PKHTB(ARG1,ARG2,ARG3) ( ((((uint32_t)(ARG1)) ) & 0xFFFF0000UL) | \
2069 ((((uint32_t)(ARG2)) >> (ARG3)) & 0x0000FFFFUL) )
2070
2071 __STATIC_FORCEINLINE int32_t __SMMLA (int32_t op1, int32_t op2, int32_t op3)
2072 {
2073 int32_t result;
2074
2075 __ASM volatile ("smmla %0, %1, %2, %3" : "=r" (result): "r" (op1), "r" (op2), "r" (op3) );
2076 return(result);
2077 }
2078
2079 #endif /* (__ARM_FEATURE_DSP == 1) */
2080
2083 #pragma GCC diagnostic pop
2084
2085 #endif /* __CMSIS_GCC_H */
__get_CONTROL
__STATIC_INLINE uint32_t __get_CONTROL(void)
Enable IRQ Interrupts
Definition: cmsis_armcc.h:130
__get_IPSR
__STATIC_INLINE uint32_t __get_IPSR(void)
Get IPSR Register
Definition: cmsis_armcc.h:154
__USAT
__STATIC_FORCEINLINE uint32_t __USAT(int32_t val, uint32_t sat)
Unsigned Saturate
Definition: cmsis_armclang.h:1146
__get_PSP
__STATIC_INLINE uint32_t __get_PSP(void)
Get Process Stack Pointer
Definition: cmsis_armcc.h:190
__attribute__
__attribute__((section(".rev16_text"))) __STATIC_INLINE __ASM uint32_t __REV16(uint32_t value)
Reverse byte order (16 bit)
Definition: cmsis_armcc.h:463
__set_PSP
__STATIC_INLINE void __set_PSP(uint32_t topOfProcStack)
Set Process Stack Pointer
Definition: cmsis_armcc.h:202
__DMB
__STATIC_FORCEINLINE void __DMB(void)
Data Memory Barrier
Definition: cmsis_gcc.h:888
__get_xPSR
__STATIC_INLINE uint32_t __get_xPSR(void)
Get xPSR Register
Definition: cmsis_armcc.h:178
__REVSH
__STATIC_FORCEINLINE int16_t __REVSH(int16_t value)
Reverse byte order (16 bit)
Definition: cmsis_gcc.h:934
__set_MSP
__STATIC_INLINE void __set_MSP(uint32_t topOfMainStack)
Set Main Stack Pointer
Definition: cmsis_armcc.h:226
__DSB
__STATIC_FORCEINLINE void __DSB(void)
Data Synchronization Barrier
Definition: cmsis_gcc.h:877
__set_PRIMASK
__STATIC_INLINE void __set_PRIMASK(uint32_t priMask)
Set Priority Mask
Definition: cmsis_armcc.h:250
__REV16
__STATIC_FORCEINLINE uint32_t __REV16(uint32_t value)
Reverse byte order (16 bit)
Definition: cmsis_gcc.h:919
__disable_irq
__STATIC_FORCEINLINE void __disable_irq(void)
Disable IRQ Interrupts
Definition: cmsis_gcc.h:140
__RBIT
__STATIC_FORCEINLINE uint32_t __RBIT(uint32_t value)
Reverse bit order of value
Definition: cmsis_gcc.h:981
__set_FPSCR
__STATIC_INLINE void __set_FPSCR(uint32_t fpscr)
Set FPSCR
Definition: cmsis_armcc.h:362
__get_APSR
__STATIC_INLINE uint32_t __get_APSR(void)
Get APSR Register
Definition: cmsis_armcc.h:166
__get_PRIMASK
__STATIC_INLINE uint32_t __get_PRIMASK(void)
Get Priority Mask
Definition: cmsis_armcc.h:238
__get_MSP
__STATIC_INLINE uint32_t __get_MSP(void)
Get Main Stack Pointer
Definition: cmsis_armcc.h:214
__get_FPSCR
__STATIC_INLINE uint32_t __get_FPSCR(void)
Get FPSCR
Definition: cmsis_armcc.h:345
__ROR
__STATIC_FORCEINLINE uint32_t __ROR(uint32_t op1, uint32_t op2)
Rotate Right in unsigned value (32 bit)
Definition: cmsis_armclang.h:876
__set_CONTROL
__STATIC_INLINE void __set_CONTROL(uint32_t control)
Set Control Register
Definition: cmsis_armcc.h:142
__enable_irq
__STATIC_FORCEINLINE void __enable_irq(void)
Enable IRQ Interrupts
Definition: cmsis_gcc.h:129
__SSAT
__STATIC_FORCEINLINE int32_t __SSAT(int32_t val, uint32_t sat)
Signed Saturate
Definition: cmsis_armclang.h:1121
__ISB
__STATIC_FORCEINLINE void __ISB(void)
Instruction Synchronization Barrier
Definition: cmsis_gcc.h:866
__REV
__STATIC_FORCEINLINE uint32_t __REV(uint32_t value)
Reverse byte order (32 bit)
Definition: cmsis_gcc.h:900