/**
  @page PCA_Input_Capture PCA input capture example
  
  @verbatim
  ****************** (C) COPYRIGHT 2023 megawin Technology *******************
  * @file    PCA/PCA_Input_Capture/readme.txt 
  * @author  megawin Application Team
  * @version V0.0.5
  * @date    13-August-2024
  * @brief   Description of the PCA PCA_Input_Capture example.
  ******************************************************************************
  * THE PRESENT FIRMWARE WHICH IS FOR GUIDANCE ONLY AIMS AT PROVIDING CUSTOMERS
  * WITH CODING INFORMATION REGARDING THEIR PRODUCTS IN ORDER FOR THEM TO SAVE
  * TIME. AS A RESULT, MEGAWIN SHALL NOT BE HELD LIABLE FOR ANY DIRECT,
  * INDIRECT OR CONSEQUENTIAL DAMAGES WITH RESPECT TO ANY CLAIMS ARISING FROM
  * THE CONTENT OF SUCH FIRMWARE AND/OR THE USE MADE BY CUSTOMERS OF THE
  * CODING INFORMATION CONTAINED HEREIN IN CONNECTION WITH THEIR PRODUCTS.
  ******************************************************************************
   @endverbatim

@par 例程描述 

本例程演示使用PCA外设去测量外部信号的频率。

本例程系统时钟工作在24Mhz。

串口1按照如下配置：
- 波特率：115200
- 数据位：8


@par 目录内容 

  - PCA/PCA_Input_Capture/PCA_Input_Capture.uvprojx    MDK5工程文件
  - PCA/PCA_Input_Capture/PCA_Input_Capture.uvoptx     MDK5工程配置文件
  - PCA/PCA_Input_Capture/JLinkSettings.ini            Jlink配置文件
  - PCA/PCA_Input_Capture/main.c                       主程序


@par 硬件和软件环境 

  - 硬件平台搭建
    - 芯片管脚按如下连接：
      - UART1 (PD5, PD6) 连接到串口
      - 将PCA通道3(PC6)连接到外部信号

@par 如何使用？ 

为了使程序工作，您必须执行以下操作 :
 - 使用 MDK5 打开此例程文件夹中的 PCA_Input_Capture.uvprojx 工程
 - 重新编译该工程并下载到目标存储器中
 - 运行此例程
   
 * <h3><center>&copy; COPYRIGHT 2023 megawin Technology</center></h3>
 */
