MG32L003 Standard Peripherals Firmware Library

宏定义 | 函数 | 变量
system_mg32l003.c 文件参考

CMSIS Device System Source File for MG32L003 Device Series 更多...

`#include "mg32l003.h"`

## 宏定义
#define | HSI_VALUE_24M ((uint32_t)24000000)
#define | HSI_VALUE_22M ((uint32_t)22120000)
#define | HSI_VALUE_16M ((uint32_t)16000000)
#define | HSI_VALUE_8M ((uint32_t)8000000)
#define | HSI_VALUE_4M ((uint32_t)4000000)
#define | VECT_TAB_OFFSET 0x00000000U

## 函数
void | SystemInit (void)
| Setup the microcontroller system Initialize the Embedded Flash Interface, the PLL and update the SystemCoreClock variable. 更多...
void | SystemCoreClockUpdate (void)
| Update SystemCoreClock variable according to Clock Register Values. The SystemCoreClock variable contains the core clock (HCLK), it can be used by the user application to setup the SysTick timer or configure other parameters. 更多...

## 变量
uint32_t | SystemCoreClock = 4000000

## 详细描述

CMSIS Device System Source File for MG32L003 Device Series

版本
  V0.0.5

日期
  13-August-2024

## 宏定义说明

## ◆ HSI_VALUE_16M

#define HSI_VALUE_16M ((uint32_t)16000000)

Value of the Internal oscillator select 16MHz

## ◆ HSI_VALUE_22M

#define HSI_VALUE_22M ((uint32_t)22120000)

Value of the Internal oscillator select 22.12MHz

## ◆ HSI_VALUE_24M

#define HSI_VALUE_24M ((uint32_t)24000000)

Value of the Internal oscillator select 24MHz

## ◆ HSI_VALUE_4M

#define HSI_VALUE_4M ((uint32_t)4000000)

Value of the Internal oscillator select 4MHz

## ◆ HSI_VALUE_8M

#define HSI_VALUE_8M ((uint32_t)8000000)

Value of the Internal oscillator select 8MHz

## ◆ VECT_TAB_OFFSET

#define VECT_TAB_OFFSET 0x00000000U

< Uncomment the following line if you need to relocate your vector Table in Internal SRAM. Vector Table base offset field.