
T3344 003:882 SEGGER J-Link V6.35g (beta) Log File (0000ms, 0011ms total)
T3344 003:882 DLL Compiled: Oct 19 2018 17:34:51 (0000ms, 0011ms total)
T3344 003:882 Logging started @ 2024-11-07 13:08 (0000ms, 0011ms total)
T3344 003:882 JLINK_SetWarnOutHandler(...) (0000ms, 0011ms total)
T3344 003:882 JLINK_OpenEx(...)
Firmware: J-Link V9 compiled Dec 13 2022 11:14:50
Hardware: V9.20
S/N: 25952311
Feature(s): RDI, GDB, FlashDL, FlashBP, JFlash
TELNET listener socket opened on port 19021WEBSRV 
Starting webserver (0026ms, 0037ms total)
T3344 003:882 WEBSRV Webserver running on local port 19080 (0026ms, 0037ms total)
T3344 003:882   returns O.K. (0026ms, 0037ms total)
T3344 003:908 JLINK_GetEmuCaps()  returns 0xB9FF7BBF (0001ms, 0038ms total)
T3344 003:909 JLINK_TIF_GetAvailable(...) (0000ms, 0038ms total)
T3344 003:909 JLINK_SetErrorOutHandler(...) (0000ms, 0038ms total)
T3344 003:909 JLINK_ExecCommand("ProjectFile = "G:\M0PLUS\MG32L003\Renaming\EN\Code\MG32L003_StdPeriph_Lib_V0.0.5\Projects\MG32L003_StdPeriph_Examples\TIM\TIM1_6Steps_PWM\JLinkSettings.ini"", ...). XML file found at: H:\Keil_v5\ARM\Segger\JLinkDevices.xml (0005ms, 0043ms total)
T3344 003:909 H:\Keil_v5\ARM\Segger\JLinkDevices.xml evaluated successfully.  returns 0x00 (0066ms, 0104ms total)
T3344 003:975 JLINK_ExecCommand("Device = ARMCM0P", ...). Device "CORTEX-M0" selected.  returns 0x00 (0001ms, 0105ms total)
T3344 003:976 JLINK_ExecCommand("DisableConnectionTimeout", ...).   returns 0x01 (0000ms, 0105ms total)
T3344 003:976 JLINK_GetHardwareVersion()  returns 0x16760 (0000ms, 0105ms total)
T3344 003:976 JLINK_GetDLLVersion()  returns 63507 (0000ms, 0105ms total)
T3344 003:976 JLINK_GetFirmwareString(...) (0000ms, 0105ms total)
T3344 003:976 JLINK_GetDLLVersion()  returns 63507 (0000ms, 0105ms total)
T3344 003:976 JLINK_GetCompileDateTime() (0000ms, 0105ms total)
T3344 003:976 JLINK_GetFirmwareString(...) (0000ms, 0105ms total)
T3344 003:976 JLINK_GetHardwareVersion()  returns 0x16760 (0000ms, 0105ms total)
T3344 003:976 JLINK_TIF_Select(JLINKARM_TIF_SWD)  returns 0x00 (0001ms, 0106ms total)
T3344 003:977 JLINK_SetSpeed(5000) (0000ms, 0106ms total)
T3344 003:977 JLINK_SetResetType(JLINKARM_RESET_TYPE_NORMAL)  returns JLINKARM_RESET_TYPE_NORMAL (0000ms, 0106ms total)
T3344 003:977 JLINK_Reset() >0x10B TIF>Found SW-DP with ID 0x2BA01477 >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x28 TIF>Scanning AP map to find all available APs >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF>AP[1]: Stopped AP scan as end of AP map has been reachedAP[0]: AHB-AP (IDR: 0x24770011)Iterating through AP map to find AHB-AP to use
 >0x42 TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF> >0x42 TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF>AP[0]: Core foundAP[0]: AHB-AP ROM base: 0xE00FF000 >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF>CPUID register: 0x412FC231. Implementer code: 0x41 (ARM)Found Cortex-M3 r2p1, Little endian.
Identified core does not match configuration. (Found: Cortex-M3, Configured: Cortex-M0) -- Max. mem block: 0x00010D68 -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_WriteMem(4 bytes @ 0xE000EDF0) -- CPU_ReadMem(4 bytes @ 0xE0002000)FPUnit: 6 code (BP) slots and 2 literal slots -- CPU_ReadMem(4 bytes @ 0xE000EDFC) -- CPU_WriteMem(4 bytes @ 0xE000EDFC) -- CPU_ReadMem(4 bytes @ 0xE0001000) -- CPU_WriteMem(4 bytes @ 0xE0001000) -- CPU_ReadMem(4 bytes @ 0xE000ED88) -- CPU_WriteMem(4 bytes @ 0xE000ED88)
 -- CPU_ReadMem(4 bytes @ 0xE000ED88) -- CPU_WriteMem(4 bytes @ 0xE000ED88)CoreSight components:ROMTbl[0] @ E00FF000 -- CPU_ReadMem(16 bytes @ 0xE00FF000) -- CPU_ReadMem(16 bytes @ 0xE000EFF0) -- CPU_ReadMem(16 bytes @ 0xE000EFE0)ROMTbl[0][0]: E000E000, CID: B105E00D, PID: 000BB000 SCS -- CPU_ReadMem(16 bytes @ 0xE0001FF0) -- CPU_ReadMem(16 bytes @ 0xE0001FE0)ROMTbl[0][1]: E0001000, CID: B105E00D, PID: 003BB002 DWT -- CPU_ReadMem(16 bytes @ 0xE0002FF0) -- CPU_ReadMem(16 bytes @ 0xE0002FE0)
ROMTbl[0][2]: E0002000, CID: B105E00D, PID: 002BB003 FPB -- CPU_ReadMem(16 bytes @ 0xE0000FF0) -- CPU_ReadMem(16 bytes @ 0xE0000FE0)ROMTbl[0][3]: E0000000, CID: B105E00D, PID: 003BB001 ITM -- CPU_ReadMem(16 bytes @ 0xE00FF010) -- CPU_ReadMem(16 bytes @ 0xE0040FF0) -- CPU_ReadMem(16 bytes @ 0xE0040FE0)ROMTbl[0][4]: E0040000, CID: B105900D, PID: 003BB923 TPIU-Lite -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000EDF0) -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000EDFC)
Reset: Halt core after reset via DEMCR.VC_CORERESET. >0x35 TIF>Reset: Reset device via AIRCR.SYSRESETREQ. -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000ED0C) >0x0D TIF> >0x28 TIF> -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000EDF0) -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000EDFC) -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_WriteMem(4 bytes @ 0xE0002000) -- CPU_ReadMem(4 bytes @ 0xE000EDFC)
 -- CPU_ReadMem(4 bytes @ 0xE0001000) (0185ms, 0291ms total)
T3344 004:162 JLINK_GetId() >0x0D TIF> >0x21 TIF>  returns 0x2BA01477 (0000ms, 0291ms total)
T3344 004:169 JLINK_GetFirmwareString(...) (0000ms, 0291ms total)
T3344 006:563 JLINK_Close() -- CPU_ReadMem(4 bytes @ 0xE0001000) -- CPU_WriteMem(4 bytes @ 0xE0001004) >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x28 TIF> (0017ms, 0308ms total)
T3344 006:563  (0017ms, 0308ms total)
T3344 006:563 Closed (0017ms, 0308ms total)
