MG32L003 Standard Peripherals Firmware Library

宏定义
VCMP_Interrupt_Trigger_Selection
MG32L003_StdPeriph_Driver » VCMP » VCMP_Exported_Constants

## 宏定义
#define | VCMP_HIGH_INT VCMP_CR1_HIGHINTEN
#define | VCMP_RISE_INT VCMP_CR1_RISEINTEN
#define | VCMP_FALL_INT VCMP_CR1_FALLINTEN
#define | VCMP_INT_MASK (VCMP_HIGH_INT | VCMP_RISE_INT | VCMP_FALL_INT)
#define | IS_VCMP_INT(VCMP_INT)

## 详细描述

## 宏定义说明

## ◆ IS_VCMP_INT

#define IS_VCMP_INT | ( |  | VCMP_INT | ) |

值:
(((VCMP_INT) == VCMP_HIGH_INT) || ((VCMP_INT) == VCMP_RISE_INT) || \
((VCMP_INT) == VCMP_FALL_INT))
VCMP_FALL_INT
#define VCMP_FALL_INT
Definition: mg32l003_vcmp.h:106
VCMP_RISE_INT
#define VCMP_RISE_INT
Definition: mg32l003_vcmp.h:105
VCMP_HIGH_INT
#define VCMP_HIGH_INT
Definition: mg32l003_vcmp.h:104

## ◆ VCMP_FALL_INT

#define VCMP_FALL_INT VCMP_CR1_FALLINTEN

VCMP INTERRUPT FALL TRIGER ENABLE

## ◆ VCMP_HIGH_INT

#define VCMP_HIGH_INT VCMP_CR1_HIGHINTEN

VCMP INTERRUPT HIGHT LEVEL TRIGER ENABLE

## ◆ VCMP_RISE_INT

#define VCMP_RISE_INT VCMP_CR1_RISEINTEN

VCMP INTERRUPT RISE TRIGER ENABLE