MG32L003 Standard Peripherals Firmware Library

结构体 | 宏定义 | 函数
mg32l003_rtc.h 文件参考

This file contains all the functions prototypes for the RTC firmware library. 更多...

`#include "mg32l003.h"`

浏览源代码.

## 结构体
struct | RTC_TimeTypeDef
| RTC Time structure definition 更多...
struct | RTC_DateTypeDef
| RTC Date structure definition 更多...
struct | RTC_AlarmEnableTypeDef
| RTC ALARM Enable structure definition 更多...
struct | RTC_AlarmTypeDef
| RTC Alarm structure definition 更多...
struct | RTC_InitTypeDef
| RTC Init structures definition 更多...
struct | RTC_HandleTypeDef
| Time Handle Structure definition 更多...

## 宏定义
#define | RTC_HOURFORMAT_24 RTC_CR_FMT
#define | RTC_HOURFORMAT_12 0x00000000U
#define | IS_RTC_HOUR_FORMAT(FORMAT)
#define | IS_RTC_HOUR12(HOUR) (((HOUR) > 0) && ((HOUR) <= 12))
#define | IS_RTC_HOUR24(HOUR) ((HOUR) <= 23)
#define | IS_RTC_MINUTES(MINUTES) ((MINUTES) <= 59)
#define | IS_RTC_SECONDS(SECONDS) ((SECONDS) <= 59)
#define | RTC_H12_AM ((uint8_t)0x00)
#define | RTC_H12_PM ((uint8_t)0x01)
#define | IS_RTC_H12(PM) (((PM) == RTC_H12_AM) || ((PM) == RTC_H12_PM))
#define | IS_RTC_YEAR(YEAR) ((YEAR) <= 99)
#define | RTC_Month_January ((uint8_t)0x01)
#define | RTC_Month_February ((uint8_t)0x02)
#define | RTC_Month_March ((uint8_t)0x03)
#define | RTC_Month_April ((uint8_t)0x04)
#define | RTC_Month_May ((uint8_t)0x05)
#define | RTC_Month_June ((uint8_t)0x06)
#define | RTC_Month_July ((uint8_t)0x07)
#define | RTC_Month_August ((uint8_t)0x08)
#define | RTC_Month_September ((uint8_t)0x09)
#define | RTC_Month_October ((uint8_t)0x10)
#define | RTC_Month_November ((uint8_t)0x11)
#define | RTC_Month_December ((uint8_t)0x12)
#define | IS_RTC_MONTH(MONTH) (((MONTH) >= 1) && ((MONTH) <= 12))
#define | IS_RTC_DATE(DATE) (((DATE) >= 1) && ((DATE) <= 31))
#define | IS_RTC_CEN(CEN) ((CEN) <= 1)
#define | RTC_Weekday_Monday ((uint8_t)0x00)
#define | RTC_Weekday_Tuesday ((uint8_t)0x01)
#define | RTC_Weekday_Wednesday ((uint8_t)0x02)
#define | RTC_Weekday_Thursday ((uint8_t)0x03)
#define | RTC_Weekday_Friday ((uint8_t)0x04)
#define | RTC_Weekday_Saturday ((uint8_t)0x05)
#define | RTC_Weekday_Sunday ((uint8_t)0x06)
#define | IS_RTC_WEEKDAY(WEEKDAY)
#define | RTC_Format_BIN ((uint32_t)0x000000000)
#define | RTC_Format_BCD ((uint32_t)0x000000001)
#define | IS_RTC_FORMAT(FORMAT) (((FORMAT) == RTC_Format_BIN) || ((FORMAT) == RTC_Format_BCD))
#define | RTC_CLOCK_LSE (0x00UL << RTC_CLKCR_RTCCKSEL_Pos)
#define | RTC_CLOCK_LSI (0x01UL << RTC_CLKCR_RTCCKSEL_Pos)
#define | RTC_CLOCK_HSE (0x02UL << RTC_CLKCR_RTCCKSEL_Pos)
#define | IS_RTC_CLK_SOURCE(CLK)
#define | IS_RTC_HSE_DIV(DIV) (((DIV) <= 0x7F))
#define | RTC_IT_ALR2 ((uint32_t)0x00000020)
#define | RTC_IT_ALR1 ((uint32_t)0x00000010)
#define | IS_RTC_CONFIG_IT(IT) (((IT) != (uint32_t)RESET) && (((IT)&0xFFFFFFCF) == (uint32_t)RESET))
#define | IS_RTC_GET_IT(IT) (((IT) == RTC_IT_ALR1) || ((IT) == RTC_IT_ALR1))
#define | IS_RTC_CLEAR_IT(IT) (((IT) != (uint32_t)RESET) && (((IT)&0xFFFFFFCF) == (uint32_t)RESET))
#define | RTC_ALARM_1 0x00U
#define | RTC_ALARM_2 0x01U
#define | RTC_CLK_SOURCE_LSE (0x00000000)
#define | RTC_CLK_SOURCE_LSI (0x00010000)
#define | RTC_CLK_SOURCE_HSEDIV (0x00020000)
#define | RTC_ALARM2_CLOSE ((uint8_t)0x00)
#define | RTC_ALARM2_1S ((uint8_t)0x01)
#define | RTC_ALARM2_1P2S ((uint8_t)0x02)
#define | RTC_ALARM2_1P4S ((uint8_t)0x03)
#define | RTC_ALARM2_1P8S ((uint8_t)0x04)
#define | RTC_ALARM2_1P16S ((uint8_t)0x05)
#define | RTC_ALARM2_1P32S ((uint8_t)0x06)
#define | RTC_ALARM2_1P64S ((uint8_t)0x07)
#define | RTC_ALARM2_1P128S ((uint8_t)0x08)
#define | RTC_ALARM2_10S ((uint8_t)0x09)
#define | RTC_ALARM2_30S ((uint8_t)0x0A)
#define | RTC_ALARM2_1M ((uint8_t)0x0B)
#define | RTC_ALARM2_30M ((uint8_t)0x0C)
#define | RTC_ALARM2_60M ((uint8_t)0x0D)
#define | RTC_ALARM2_12H ((uint8_t)0x0E)
#define | RTC_ALARM2_24H ((uint8_t)0x0F)
#define | IS_RTC_ALARM_2_PERIOD(PERIOD)
#define | RTC_FLAG_ALR2F RTC_ISR_ALM2_F /* Alarm 2 flag */
#define | RTC_FLAG_ALR1F RTC_ISR_ALM1_F /* Alarm 1 flag */
#define | RTC_FLAG_RSF RTC_ISR_RSF /* Registers Synchronized flag */
#define | RTC_FLAG_WAITF RTC_ISR_WAITF /* Initialization mode flag */
#define | RTC_FLAG_WAIT RTC_ISR_WAIT /* Shift operation pending flag */
#define | IS_RTC_GET_FLAG(FLAG)
#define | RTC_CalibPeriod_60sec ((uint32_t)0x00000000)
#define | RTC_CalibPeriod_30sec ((uint32_t)0x00000100)
#define | RTC_CalibPeriod_15sec ((uint32_t)0x00000200)
#define | RTC_CalibPeriod_6sec ((uint32_t)0x00000300)
#define | IS_RTC_CALIB_PERIOD(PERIOD)
#define | IS_RTC_CALIB_MINUS(VALUE) ((VALUE) <= 0x0000007F)

## 函数
ErrorStatus | RTC_Init (RTC_InitTypeDef *RTC_InitStruct)
| Initializes the RTC registers according to the specified parameters in RTC_InitStruct. 更多...
void | RTC_WriteProtectionCmd (FunctionalState NewState)
| Enables or disables the RTC registers write protection. 更多...
ErrorStatus | RTC_EnterInitMode (void)
| Enters the RTC Initialization mode. 更多...
void | RTC_ExitInitMode (void)
| Exits the RTC Initialization mode. 更多...
ErrorStatus | RTC_WaitForSynchro (void)
| Waits until the RTC Time and Date registers (RTC_TR and RTC_DR) are synchronized with RTC APB clock. 更多...
void | RTC_BypassShadowCmd (FunctionalState NewState)
| Enables or Disables the Bypass Shadow feature. 更多...
ErrorStatus | RTC_SetTime (uint32_t RTC_Format, RTC_TimeTypeDef *RTC_TimeStruct)
| Set the RTC current time. 更多...
void | RTC_TimeStructInit (RTC_TimeTypeDef *RTC_TimeStruct)
| Fills each RTC_TimeStruct member with its default value (Time = 00h:00min:00sec). 更多...
void | RTC_GetTime (uint32_t RTC_Format, RTC_TimeTypeDef *RTC_TimeStruct)
| Get the RTC current Time. 更多...
ErrorStatus | RTC_SetDate (uint32_t RTC_Format, RTC_DateTypeDef *RTC_DateStruct)
| Set the RTC current date. 更多...
void | RTC_DateStructInit (RTC_DateTypeDef *RTC_DateStruct)
| Fills each RTC_DateStruct member with its default value (Monday, January 01 xx00). 更多...
void | RTC_GetDate (uint32_t RTC_Format, RTC_DateTypeDef *RTC_DateStruct)
| Get the RTC current date. 更多...
void | RTC_SetAlarm1 (uint32_t RTC_Format, RTC_AlarmTypeDef *RTC_AlarmStruct)
| Set the specified RTC Alarm1. 更多...
void | RTC_AlarmStructInit (RTC_AlarmTypeDef *RTC_AlarmStruct)
void | RTC_Alarm1Cmd (FunctionalState NewState)
| Enables or disables the specified RTC Alarm. 更多...
void | RTC_GetAlarm1 (uint32_t RTC_Format, RTC_AlarmTypeDef *RTC_AlarmStruct)
| Get the RTC Alarm value and masks. 更多...
ErrorStatus | RTC_AlarmCmd (uint32_t RTC_Alarm, FunctionalState NewState)
void | RTC_SetALARM2Period (uint32_t Period)
| Set the specified RTC Alarm2. 更多...
void | RTC_1HZ_Config (FunctionalState NewState)
| Deactive the specified 1HZ out 更多...
void | RTC_CalibConfig (uint32_t RTC_CalibPeriod, uint32_t RTC_CalibMinusPulsesValue)
| Configures the Calibration Settings. 更多...
void | RTC_ITConfig (uint32_t RTC_IT, FunctionalState NewState)
| Enables or disables the specified RTC interrupts. 更多...
ITStatus | RTC_GetITStatus (uint32_t RTC_IT)
void | RTC_ClearITPendingBit (uint32_t RTC_IT)
| Clears the RTC's interrupt pending bits. 更多...

## 详细描述

This file contains all the functions prototypes for the RTC firmware library.

作者
  megawinTech Application Team

版本
  V0.0.5

日期
  13-August-2024