
T263C 000:212 SEGGER J-Link V6.35g (beta) Log File (0000ms, 0012ms total)
T263C 000:212 DLL Compiled: Oct 19 2018 17:34:51 (0000ms, 0012ms total)
T263C 000:212 Logging started @ 2024-11-07 14:16 (0000ms, 0012ms total)
T263C 000:213 JLINK_SetWarnOutHandler(...) (0000ms, 0012ms total)
T263C 000:213 JLINK_OpenEx(...)
Firmware: J-Link V9 compiled Dec 13 2022 11:14:50
Hardware: V9.20
S/N: 25952311
Feature(s): RDI, GDB, FlashDL, FlashBP, JFlash
TELNET listener socket opened on port 19021WEBSRV 
Starting webserver (0023ms, 0035ms total)
T263C 000:213 WEBSRV Webserver running on local port 19080 (0023ms, 0035ms total)
T263C 000:213   returns O.K. (0023ms, 0035ms total)
T263C 000:236 JLINK_GetEmuCaps()  returns 0xB9FF7BBF (0002ms, 0037ms total)
T263C 000:238 JLINK_TIF_GetAvailable(...) (0000ms, 0037ms total)
T263C 000:238 JLINK_SetErrorOutHandler(...) (0000ms, 0037ms total)
T263C 000:238 JLINK_ExecCommand("ProjectFile = "G:\M0PLUS\MG32L003\Renaming\EN\Code\MG32L003_StdPeriph_Lib_V0.0.5\Projects\MG32L003_StdPeriph_Examples\LPTIM\LPTIM_SleepMode\JLinkSettings.ini"", ...). XML file found at: H:\Keil_v5\ARM\Segger\JLinkDevices.xml (0004ms, 0041ms total)
T263C 000:238 H:\Keil_v5\ARM\Segger\JLinkDevices.xml evaluated successfully.  returns 0x00 (0079ms, 0116ms total)
T263C 000:318 JLINK_ExecCommand("Device = MG32L003F8P6", ...). Device "CORTEX-M0+" selected.  returns 0x00 (0019ms, 0824ms total)
T263C 004:120 JLINK_ExecCommand("DisableConnectionTimeout", ...).   returns 0x01 (0000ms, 0824ms total)
T263C 004:120 JLINK_GetHardwareVersion()  returns 0x16760 (0000ms, 0824ms total)
T263C 004:120 JLINK_GetDLLVersion()  returns 63507 (0000ms, 0824ms total)
T263C 004:120 JLINK_GetFirmwareString(...) (0000ms, 0824ms total)
T263C 004:120 JLINK_GetDLLVersion()  returns 63507 (0000ms, 0824ms total)
T263C 004:120 JLINK_GetCompileDateTime() (0000ms, 0824ms total)
T263C 004:120 JLINK_GetFirmwareString(...) (0000ms, 0824ms total)
T263C 004:120 JLINK_GetHardwareVersion()  returns 0x16760 (0001ms, 0825ms total)
T263C 004:121 JLINK_TIF_Select(JLINKARM_TIF_JTAG)  returns 0x00 (0000ms, 0825ms total)
T263C 004:121 JLINK_SetSpeed(5000) (0000ms, 0825ms total)
T263C 004:122 JLINK_SetResetType(JLINKARM_RESET_TYPE_NORMAL)  returns JLINKARM_RESET_TYPE_NORMAL (0000ms, 0825ms total)
T263C 004:122 JLINK_Reset() >0x2F8 JTAG>Could not measure total IR len. TDO is constant high. >0xC8 JTAG> >0x2F8 JTAG>Could not measure total IR len. TDO is constant high. >0xC8 JTAG>JLINK_GetIdData(...) >0x2F8 JTAG>Could not measure total IR len. TDO is constant high. >0xC8 JTAG> >0x2F8 JTAG>Could not measure total IR len. TDO is constant high. >0xC8 JTAG> (0154ms, 1133ms total)
T263C 004:430 JLINK_GetIdData(...) >0x2F8 JTAG>Could not measure total IR len. TDO is constant high. >0xC8 JTAG> >0x2F8 JTAG>Could not measure total IR len. TDO is constant high. >0xC8 JTAG> (0154ms, 1287ms total)
T263C 004:590 JLINK_GetFirmwareString(...) (0000ms, 1287ms total)
T263C 008:997 JLINK_Close() (0005ms, 1292ms total)
T263C 008:997  (0005ms, 1292ms total)
T263C 008:997 Closed (0005ms, 1292ms total)
