G04:AMPARAMS|DCode=13|XSize=47mil|YSize=7mil|CornerRadius=0mil|HoleSize=0mil|Usage=FLASHONLY|Rotation=135.000|XOffset=0mil|YOffset=0mil|HoleType=Round|Shape=Round|*
%AMOVALD13*
21,1,0.040,0.007,0.000,0.000,135.0*
1,1,0.007,0.014,-0.014*
1,1,0.007,-0.014,0.014*
%
G04:AMPARAMS|DCode=14|XSize=47mil|YSize=7mil|CornerRadius=0mil|HoleSize=0mil|Usage=FLASHONLY|Rotation=135.000|XOffset=0mil|YOffset=0mil|HoleType=Round|Shape=Rectangle|*
%AMROTATEDRECTD14*
4,1,4,0.019,-0.014,0.014,-0.019,-0.019,0.014,-0.014,0.019,0.019,-0.014,0.0*
%
G04:AMPARAMS|DCode=15|XSize=47mil|YSize=7mil|CornerRadius=0mil|HoleSize=0mil|Usage=FLASHONLY|Rotation=225.000|XOffset=0mil|YOffset=0mil|HoleType=Round|Shape=Round|*
%AMOVALD15*
21,1,0.040,0.007,0.000,0.000,225.0*
1,1,0.007,0.014,0.014*
1,1,0.007,-0.014,-0.014*
%
G04:AMPARAMS|DCode=16|XSize=47mil|YSize=7mil|CornerRadius=0mil|HoleSize=0mil|Usage=FLASHONLY|Rotation=225.000|XOffset=0mil|YOffset=0mil|HoleType=Round|Shape=Rectangle|*
%AMROTATEDRECTD16*
4,1,4,0.014,0.019,0.019,0.014,-0.014,-0.019,-0.019,-0.014,0.014,0.019,0.0*
%
G04:AMPARAMS|DCode=65|XSize=55mil|YSize=15mil|CornerRadius=0mil|HoleSize=0mil|Usage=FLASHONLY|Rotation=135.000|XOffset=0mil|YOffset=0mil|HoleType=Round|Shape=Round|*
%AMOVALD65*
21,1,0.040,0.015,0.000,0.000,135.0*
1,1,0.015,0.014,-0.014*
1,1,0.015,-0.014,0.014*
%
G04:AMPARAMS|DCode=66|XSize=55mil|YSize=15mil|CornerRadius=0mil|HoleSize=0mil|Usage=FLASHONLY|Rotation=135.000|XOffset=0mil|YOffset=0mil|HoleType=Round|Shape=Rectangle|*
%AMROTATEDRECTD66*
4,1,4,0.025,-0.014,0.014,-0.025,-0.025,0.014,-0.014,0.025,0.025,-0.014,0.0*
%
G04:AMPARAMS|DCode=67|XSize=55mil|YSize=15mil|CornerRadius=0mil|HoleSize=0mil|Usage=FLASHONLY|Rotation=225.000|XOffset=0mil|YOffset=0mil|HoleType=Round|Shape=Round|*
%AMOVALD67*
21,1,0.040,0.015,0.000,0.000,225.0*
1,1,0.015,0.014,0.014*
1,1,0.015,-0.014,-0.014*
%
G04:AMPARAMS|DCode=68|XSize=55mil|YSize=15mil|CornerRadius=0mil|HoleSize=0mil|Usage=FLASHONLY|Rotation=225.000|XOffset=0mil|YOffset=0mil|HoleType=Round|Shape=Rectangle|*
%AMROTATEDRECTD68*
4,1,4,0.014,0.025,0.025,0.014,-0.014,-0.025,-0.025,-0.014,0.014,0.025,0.0*
%
