G04:AMPARAMS|DCode=22|XSize=47mil|YSize=7mil|CornerRadius=0mil|HoleSize=0mil|Usage=FLASHONLY|Rotation=135.000|XOffset=0mil|YOffset=0mil|HoleType=Round|Shape=Round|*
%AMOVALD22*
21,1,0.040,0.007,0.000,0.000,135.0*
1,1,0.007,0.014,-0.014*
1,1,0.007,-0.014,0.014*
%
G04:AMPARAMS|DCode=23|XSize=47mil|YSize=7mil|CornerRadius=0mil|HoleSize=0mil|Usage=FLASHONLY|Rotation=135.000|XOffset=0mil|YOffset=0mil|HoleType=Round|Shape=Rectangle|*
%AMROTATEDRECTD23*
4,1,4,0.019,-0.014,0.014,-0.019,-0.019,0.014,-0.014,0.019,0.019,-0.014,0.0*
%
G04:AMPARAMS|DCode=24|XSize=47mil|YSize=7mil|CornerRadius=0mil|HoleSize=0mil|Usage=FLASHONLY|Rotation=225.000|XOffset=0mil|YOffset=0mil|HoleType=Round|Shape=Round|*
%AMOVALD24*
21,1,0.040,0.007,0.000,0.000,225.0*
1,1,0.007,0.014,0.014*
1,1,0.007,-0.014,-0.014*
%
G04:AMPARAMS|DCode=25|XSize=47mil|YSize=7mil|CornerRadius=0mil|HoleSize=0mil|Usage=FLASHONLY|Rotation=225.000|XOffset=0mil|YOffset=0mil|HoleType=Round|Shape=Rectangle|*
%AMROTATEDRECTD25*
4,1,4,0.014,0.019,0.019,0.014,-0.014,-0.019,-0.019,-0.014,0.014,0.019,0.0*
%
G04:AMPARAMS|DCode=79|XSize=55mil|YSize=15mil|CornerRadius=0mil|HoleSize=0mil|Usage=FLASHONLY|Rotation=135.000|XOffset=0mil|YOffset=0mil|HoleType=Round|Shape=Round|*
%AMOVALD79*
21,1,0.040,0.015,0.000,0.000,135.0*
1,1,0.015,0.014,-0.014*
1,1,0.015,-0.014,0.014*
%
G04:AMPARAMS|DCode=80|XSize=55mil|YSize=15mil|CornerRadius=0mil|HoleSize=0mil|Usage=FLASHONLY|Rotation=135.000|XOffset=0mil|YOffset=0mil|HoleType=Round|Shape=Rectangle|*
%AMROTATEDRECTD80*
4,1,4,0.025,-0.014,0.014,-0.025,-0.025,0.014,-0.014,0.025,0.025,-0.014,0.0*
%
G04:AMPARAMS|DCode=81|XSize=55mil|YSize=15mil|CornerRadius=0mil|HoleSize=0mil|Usage=FLASHONLY|Rotation=225.000|XOffset=0mil|YOffset=0mil|HoleType=Round|Shape=Round|*
%AMOVALD81*
21,1,0.040,0.015,0.000,0.000,225.0*
1,1,0.015,0.014,0.014*
1,1,0.015,-0.014,-0.014*
%
G04:AMPARAMS|DCode=82|XSize=55mil|YSize=15mil|CornerRadius=0mil|HoleSize=0mil|Usage=FLASHONLY|Rotation=225.000|XOffset=0mil|YOffset=0mil|HoleType=Round|Shape=Rectangle|*
%AMROTATEDRECTD82*
4,1,4,0.014,0.025,0.025,0.014,-0.014,-0.025,-0.025,-0.014,0.014,0.025,0.0*
%
