Next: ARM, Up: Embedded Processors [Contents][Index]

#### 21.3.1 Synopsys ARC

GDB provides the following ARC-specific commands:

`set debug arc`

  Control the level of ARC specific debug messages. Use 0 for no messages (the default), 1 for debug messages, and 2 for even more debug messages.

`show debug arc`

  Show the level of ARC specific debugging in operation.

`maint print arc arc-instruction address`

  Print internal disassembler information about instruction at a given address.