Next: NDS32, Previous: MMIX, Up: Machine Dependent [Contents][Index]

### 4.9 `ld` and MSP430

For the MSP430 it is possible to select the MPU architecture. The flag ‘`-m [mpu type]`’ will select an appropriate linker script for selected MPU type. (To get a list of known MPUs just pass ‘`-m help`’ option to the linker).

The linker will recognize some extra sections which are MSP430 specific:

`‘`.vectors`’`

  Defines a portion of ROM where interrupt vectors located.

`‘`.bootloader`’`

  Defines the bootloader portion of the ROM (if applicable). Any code in this section will be uploaded to the MPU.

`‘`.infomem`’`

  Defines an information memory section (if applicable). Any code in this section will be uploaded to the MPU.

`‘`.infomemnobits`’`

  This is the same as the ‘`.infomem`’ section except that any code in this section will not be uploaded to the MPU.

`‘`.noinit`’`

  Denotes a portion of RAM located above ‘`.bss`’ section.

  The last two sections are used by gcc.

`--code-region=[either,lower,upper,none]`

  This will transform .text* sections to [either,lower,upper].text* sections. The argument passed to GCC for -mcode-region is propagated to the linker using this option.

`--data-region=[either,lower,upper,none]`

  This will transform .data*, .bss* and .rodata* sections to [either,lower,upper].[data,bss,rodata]* sections. The argument passed to GCC for -mdata-region is propagated to the linker using this option.

`--disable-sec-transformation`

  Prevent the transformation of sections as specified by the `--code-region` and `--data-region` options. This is useful if you are compiling and linking using a single call to the GCC wrapper, and want to compile the source files using -m[code,data]-region but not transform the sections for prebuilt libraries and objects.

Next: NDS32, Previous: MMIX, Up: Machine Dependent [Contents][Index]