APPLICATION: USB 3 Gen X Command Verifier
TEST SUITE: Chapter 9 Tests [USB 2 devices].cvtests
OPERATING SYSTEM:
WORKSTATION: R140LUCASYANG
DATE: Monday, April 10, 2023
TIME: 09:57:21 AM
OPERATOR: LucasYang
NUMBER OF TESTS: 28
LOG NAME: Chapter 9 Tests - USB 2 - 2023-04-10 09-55-41
RESULT: passed

Initialize Test Suite
INFO
Test log initialized.
INFO
Log Level: Normal
INFO
User Input module initialized
INFO
Windows 10 Pro (Build 19041.1.amd64fre.vb_release.191206-1406)
INFO
CVApp.exe ver 4.1.0.0
INFO
BaseUtilities.dll ver 4.1.0.0
INFO
CommandVerifierLog.dll ver 4.1.0.0
INFO
GuiHelper.dll ver 4.1.0.0
INFO
TestUtilities.dll ver 4.1.0.0
INFO
TestSuiteEngine.dll ver 4.1.0.0
INFO
xhci_DevIOCTL.dll ver 2.2.7.0
INFO
xhci_TestServices.dll ver 2.2.7.0
INFO
USBUtilities.dll ver 1.4.5.1
INFO
StackSwitcher.dll ver 1.4.5.1
INFO
xhci_CommandVerifierServices.dll ver 2.2.7.0
INFO
VIFReader.dll ver 4.1.0.0
INFO
USB2_USBCommandVerifierServices.dll ver 2.2.7.0
INFO
USB2_USBCommandVerifier.dll ver 2.2.7.0
INFO
XHCISpecVersion: 1.20.
INFO
Host 1 selected: xHCI Host: VID=0x8086, PID=0x43ED (PCI /A� 0 �n 20 �x 0)
INFO
User selection from list: "FS Device (HID) addr=2: VID=0E6A, PID=032C"
INFO
Please select USB 2 Device to test
INFO
USB 2 Device Under Test is operating at Full Speed.
INFO
Topology: XHCI HC -- DUT
Get Number Of Configurations
INFO
USB Version number of device: 1.10
INFO
Number of configurations: 1.
Get Number Of Configurations - Other Speed
INFO
Number of Other Speed configurations: 0.
TD 9.1 - Device Descriptor Test (Configuration Index 0) - default
Passed
INFO
Start time: Apr 10, 2023 - 09:55:51
INFO
Device descriptor length : 0x12
INFO
Device descriptor type : 0x1
INFO
Major version : 0x1
INFO
Minor version : 0x10
INFO
Device supports different class spec. on different interfaces : 0xEF
INFO
Device class code indicates [Miscellaneous-Device] Device.
INFO
Device sub class : 2 (Common class)
INFO
Device protocol : 1 (Interface Association Descriptor)
INFO
Device sub class : 0x2
INFO
Device protocol : 0x1
INFO
Device MaxPacketSize0 : 0x40
INFO
Vendor information for VendorID : 0xE6A, Megawin Technology Co., Ltd.
INFO
Device ProductID : 0x32C
INFO
Device BCD : 0x100
INFO
Checking iManufacturer String Descriptor: index = 0x01.
INFO
String Descriptor : "Megawin Technology Inc.". (ENGLISH_US)
INFO
Checking iProduct String Descriptor: index = 0x02.
INFO
String Descriptor : "USB Keyboard with EasyCOM & EasyHID". (ENGLISH_US)
INFO
Checking iSerialNumber String Descriptor: index = 0x03.
INFO
String Descriptor : "V1.00". (ENGLISH_US)
INFO
Number of configurations device supports : 0x1
INFO
Stop time: Apr 10, 2023 - 09:55:52
INFO
Duration: 1 second.
INFO
Stopping Test [ TD 9.1 - Device Descriptor Test (Configuration Index 0) - default: Number of: Fails (0); Aborts (0); Warnings (0) ]
TD 9.2 - Configuration Descriptor Test (Configuration Index 0) - default
Passed
INFO
Start time: Apr 10, 2023 - 09:55:52
INFO
Configuration descriptor contains descriptor of type : 0xB (Interface Association Descriptor)
INFO
Configuration descriptor contains descriptor of type : 0x4 (Interface Descriptor)
INFO
Configuration descriptor contains descriptor of type : 0x24
INFO
Configuration descriptor contains descriptor of type : 0x24
INFO
Configuration descriptor contains descriptor of type : 0x24
INFO
Configuration descriptor contains descriptor of type : 0x24
INFO
Configuration descriptor contains descriptor of type : 0x5 (Endpoint Descriptor)
INFO
Configuration descriptor contains descriptor of type : 0x4 (Interface Descriptor)
INFO
Configuration descriptor contains descriptor of type : 0x5 (Endpoint Descriptor)
INFO
Configuration descriptor contains descriptor of type : 0x5 (Endpoint Descriptor)
INFO
Configuration descriptor contains descriptor of type : 0x4 (Interface Descriptor)
INFO
Configuration descriptor contains descriptor of type : 0x21 (HID Descriptor)
INFO
Configuration descriptor contains descriptor of type : 0x5 (Endpoint Descriptor)
INFO
Configuration descriptor contains descriptor of type : 0x4 (Interface Descriptor)
INFO
Configuration descriptor contains descriptor of type : 0x21 (HID Descriptor)
INFO
Configuration descriptor contains descriptor of type : 0x5 (Endpoint Descriptor)
INFO
Configuration descriptor contains descriptor of type : 0x4 (Interface Descriptor)
INFO
Configuration descriptor contains descriptor of type : 0x21 (HID Descriptor)
INFO
Configuration descriptor contains descriptor of type : 0x5 (Endpoint Descriptor)
INFO
Configuration descriptor contains descriptor of type : 0x5 (Endpoint Descriptor)
INFO
Number of interface descriptors found 0x5
INFO
Number of alternate interface descriptors found : 0x0
INFO
Number of endpoint descriptors found : 0x7
INFO
Configuration descriptor length : 0x9
INFO
Configuration descriptor type : 0x2
INFO
Configuration descriptor TotalLength : 0x9D
INFO
Configuration descriptor NumInterfaces : 0x5
INFO
Configuration descriptor ConfigurationValue: 0x1
INFO
Checking iConfiguration String Descriptor: index = 0x00.
INFO
The device omits this string descriptor.
INFO
Configuration descriptor bmAttributes : 0xA0
INFO
Device supports remote wake up
INFO
MaxPower = 250 PowerMultiplier = 2
INFO
Maximum power device requires : 500mA
INFO
Device is BUS POWERED
INFO
Stop time: Apr 10, 2023 - 09:55:53
INFO
Duration: 1 second.
INFO
Stopping Test [ TD 9.2 - Configuration Descriptor Test (Configuration Index 0) - default: Number of: Fails (0); Aborts (0); Warnings (0) ]
TD 9.3 Interface Association Descriptor Test (Config 0)
Passed
INFO
Start time: Apr 10, 2023 - 09:55:53
INFO
Device has 4 functions, of which 1 has an Interface Association descriptor.
INFO
Interface Association Descriptor :
INFO
bLength = 0x08
INFO
bDescriptorType = 0x0b
INFO
bFirstInterface = 0
INFO
bInterfaceCount = 2
INFO
bFunctionClass = 0x02
INFO
bFunctionSubClass = 0x02
INFO
bFunctionProtocol = 0x01
INFO
iFunction = 0x00
INFO
Running TD 9.8 : String Descriptor Test for iFunction : 0x00.
INFO
Checking iFunction String Descriptor: index = 0x00.
INFO
The device omits this string descriptor.
INFO
Found Interface Descriptor with number : 0
INFO
Found Interface Descriptor with number : 1
INFO
Function #2 does not have an Interface Association Descriptor.
INFO
Function #3 does not have an Interface Association Descriptor.
INFO
Function #4 does not have an Interface Association Descriptor.
INFO
INFO
Stop time: Apr 10, 2023 - 09:55:54
INFO
Duration: 1 second.
INFO
Stopping Test [ TD 9.3 Interface Association Descriptor Test (Config 0): Number of: Fails (0); Aborts (0); Warnings (0) ]
TD 9.4 - Interface Descriptor Test (Configuration Index 0) - default
Passed
INFO
Start time: Apr 10, 2023 - 09:55:54
INFO
Bandwidth check passed
INFO
Testing Interface number : 0x0 Alternate setting : 0x0
INFO
Interface descriptor length : 0x9
INFO
Interface descriptor bDescriptorType : 0x4
INFO
Interface descriptor bAlternateSetting : 0x0
INFO
Interface descriptor bNumEndPoints: 0x1
INFO
Interface descriptor bInterfaceClass reserved for assignment by the USB-IF : 0x02.
INFO
Interface class code indicates [CDC-Control] Interface.
INFO
Interface sub class : 2 <not defined>
INFO
Interface protocol : 1 <not defined>
INFO
Interface descriptor bInterfaceSubClass : 0x02.
INFO
Interface descriptor bInterfaceProtocol assigned by the USB-IF : 0x01.
INFO
Interface descriptor iInterface : 0x0
INFO
Testing Interface number : 0x1 Alternate setting : 0x0
INFO
Interface descriptor length : 0x9
INFO
Interface descriptor bDescriptorType : 0x4
INFO
Interface descriptor bAlternateSetting : 0x0
INFO
Interface descriptor bNumEndPoints: 0x2
INFO
Interface descriptor bInterfaceClass reserved for assignment by the USB-IF : 0x0A.
INFO
Interface class code indicates [CDC-Data] Interface.
INFO
Interface sub class : 0 <not defined>
INFO
Interface protocol : 0 <not defined>
INFO
Interface descriptor bInterfaceSubClass : 0x00.
INFO
Device does not use a class-specific protocol on this interface.
INFO
Interface descriptor iInterface : 0x0
INFO
Testing Interface number : 0x2 Alternate setting : 0x0
INFO
Interface descriptor length : 0x9
INFO
Interface descriptor bDescriptorType : 0x4
INFO
Interface descriptor bAlternateSetting : 0x0
INFO
Interface descriptor bNumEndPoints: 0x1
INFO
Interface descriptor bInterfaceClass reserved for assignment by the USB-IF : 0x03.
INFO
Interface class code indicates [HID] Interface.
INFO
Interface sub class : 1 <not defined>
INFO
Interface protocol : 1 <not defined>
INFO
Interface descriptor bInterfaceSubClass : 0x01.
INFO
Interface descriptor bInterfaceProtocol assigned by the USB-IF : 0x01.
INFO
Interface descriptor iInterface : 0x0
INFO
Testing Interface number : 0x3 Alternate setting : 0x0
INFO
Interface descriptor length : 0x9
INFO
Interface descriptor bDescriptorType : 0x4
INFO
Interface descriptor bAlternateSetting : 0x0
INFO
Interface descriptor bNumEndPoints: 0x1
INFO
Interface descriptor bInterfaceClass reserved for assignment by the USB-IF : 0x03.
INFO
Interface class code indicates [HID] Interface.
INFO
Interface sub class : 0 <not defined>
INFO
Interface protocol : 0 <not defined>
INFO
Interface descriptor bInterfaceSubClass : 0x00.
INFO
Device does not use a class-specific protocol on this interface.
INFO
Interface descriptor iInterface : 0x0
INFO
Testing Interface number : 0x4 Alternate setting : 0x0
INFO
Interface descriptor length : 0x9
INFO
Interface descriptor bDescriptorType : 0x4
INFO
Interface descriptor bAlternateSetting : 0x0
INFO
Interface descriptor bNumEndPoints: 0x2
INFO
Interface descriptor bInterfaceClass reserved for assignment by the USB-IF : 0x03.
INFO
Interface class code indicates [HID] Interface.
INFO
Interface sub class : 0 <not defined>
INFO
Interface protocol : 0 <not defined>
INFO
Interface descriptor bInterfaceSubClass : 0x00.
INFO
Device does not use a class-specific protocol on this interface.
INFO
Interface descriptor iInterface : 0x0
INFO
Stop time: Apr 10, 2023 - 09:55:55
INFO
Duration: 1 second.
INFO
Stopping Test [ TD 9.4 - Interface Descriptor Test (Configuration Index 0) - default: Number of: Fails (0); Aborts (0); Warnings (0) ]
TD 9.5 - Endpoint Descriptor Test (Configuration Index 0) - default
Passed
INFO
Start time: Apr 10, 2023 - 09:55:55
INFO
Testing Interface number : 0x0 Alternate setting : 0x0
INFO
Endpoint descriptor length : 0x7
INFO
Endpoint descriptor type : 0x5
INFO
Endpoint Type : Interrupt, Number : 0x3, Direction : IN
INFO
Endpoint descriptor bmAttributes : 0x3
INFO
Endpoint descriptor raw MaxPacketSize : 0xA
INFO
Endpoint descriptor interval : 0x1
INFO
Testing Interface number : 0x1 Alternate setting : 0x0
INFO
Endpoint descriptor length : 0x7
INFO
Endpoint descriptor type : 0x5
INFO
Endpoint Type : Bulk, Number : 0x4, Direction : IN
INFO
Endpoint descriptor bmAttributes : 0x2
INFO
Endpoint descriptor raw MaxPacketSize : 0x40
INFO
Endpoint descriptor interval : 0x0
INFO
Endpoint descriptor length : 0x7
INFO
Endpoint descriptor type : 0x5
INFO
Endpoint Type : Bulk, Number : 0x4, Direction : OUT
INFO
Endpoint descriptor bmAttributes : 0x2
INFO
Endpoint descriptor raw MaxPacketSize : 0x40
INFO
Endpoint descriptor interval : 0x0
INFO
Testing Interface number : 0x2 Alternate setting : 0x0
INFO
Endpoint descriptor length : 0x7
INFO
Endpoint descriptor type : 0x5
INFO
Endpoint Type : Interrupt, Number : 0x1, Direction : IN
INFO
Endpoint descriptor bmAttributes : 0x3
INFO
Endpoint descriptor raw MaxPacketSize : 0x8
INFO
Endpoint descriptor interval : 0x1
INFO
Testing Interface number : 0x3 Alternate setting : 0x0
INFO
Endpoint descriptor length : 0x7
INFO
Endpoint descriptor type : 0x5
INFO
Endpoint Type : Interrupt, Number : 0x2, Direction : IN
INFO
Endpoint descriptor bmAttributes : 0x3
INFO
Endpoint descriptor raw MaxPacketSize : 0x8
INFO
Endpoint descriptor interval : 0x1
INFO
Testing Interface number : 0x4 Alternate setting : 0x0
INFO
Endpoint descriptor length : 0x7
INFO
Endpoint descriptor type : 0x5
INFO
Endpoint Type : Interrupt, Number : 0x5, Direction : IN
INFO
Endpoint descriptor bmAttributes : 0x3
INFO
Endpoint descriptor raw MaxPacketSize : 0x40
INFO
Endpoint descriptor interval : 0x1
INFO
Endpoint descriptor length : 0x7
INFO
Endpoint descriptor type : 0x5
INFO
Endpoint Type : Interrupt, Number : 0x5, Direction : OUT
INFO
Endpoint descriptor bmAttributes : 0x3
INFO
Endpoint descriptor raw MaxPacketSize : 0x40
INFO
Endpoint descriptor interval : 0x1
INFO
Stop time: Apr 10, 2023 - 09:55:56
INFO
Duration: 1 second.
INFO
Stopping Test [ TD 9.5 - Endpoint Descriptor Test (Configuration Index 0) - default: Number of: Fails (0); Aborts (0); Warnings (0) ]
TD 9.7 - BOS Descriptor Test - Device State Default
Passed
INFO
Start time: Apr 10, 2023 - 09:55:56
INFO
Configuration Index 0x00 has a Configuration Value of 1
INFO
USB Version number of device: 1.10
INFO
Device supports version of the USB Protocol that does not support BOS Descriptor
INFO
Stop time: Apr 10, 2023 - 09:55:57
INFO
Duration: 1 second.
INFO
Stopping Test [ TD 9.7 - BOS Descriptor Test - Device State Default: Number of: Fails (0); Aborts (0); Warnings (0) ]
TD 9.30 Configuration Summary Descriptor Test - Device State Default
Passed
INFO
Start time: Apr 10, 2023 - 09:55:57
INFO
Initialized the device to the Default state.
INFO
Retrieved Device Descriptor.
INFO
Device Under Test supports USB Version 0x1.0x10.
INFO
Configuration Summary Descriptors are not supported in this version. (Requires BOS descriptor)
INFO
Stop time: Apr 10, 2023 - 09:55:58
INFO
Duration: 1 second.
INFO
Stopping Test [ TD 9.30 Configuration Summary Descriptor Test - Device State Default: Number of: Fails (0); Aborts (0); Warnings (0) ]
TD 9.1 - Device Descriptor Test (Configuration Index 0) - addressed
Passed
INFO
Start time: Apr 10, 2023 - 09:55:58
INFO
Device descriptor length : 0x12
INFO
Device descriptor type : 0x1
INFO
Major version : 0x1
INFO
Minor version : 0x10
INFO
Device supports different class spec. on different interfaces : 0xEF
INFO
Device class code indicates [Miscellaneous-Device] Device.
INFO
Device sub class : 2 (Common class)
INFO
Device protocol : 1 (Interface Association Descriptor)
INFO
Device sub class : 0x2
INFO
Device protocol : 0x1
INFO
Device MaxPacketSize0 : 0x40
INFO
Vendor information for VendorID : 0xE6A, Megawin Technology Co., Ltd.
INFO
Device ProductID : 0x32C
INFO
Device BCD : 0x100
INFO
Checking iManufacturer String Descriptor: index = 0x01.
INFO
String Descriptor : "Megawin Technology Inc.". (ENGLISH_US)
INFO
Checking iProduct String Descriptor: index = 0x02.
INFO
String Descriptor : "USB Keyboard with EasyCOM & EasyHID". (ENGLISH_US)
INFO
Checking iSerialNumber String Descriptor: index = 0x03.
INFO
String Descriptor : "V1.00". (ENGLISH_US)
INFO
Number of configurations device supports : 0x1
INFO
Stop time: Apr 10, 2023 - 09:55:59
INFO
Duration: 1 second.
INFO
Stopping Test [ TD 9.1 - Device Descriptor Test (Configuration Index 0) - addressed: Number of: Fails (0); Aborts (0); Warnings (0) ]
TD 9.2 - Configuration Descriptor Test (Configuration Index 0) - addressed
Passed
INFO
Start time: Apr 10, 2023 - 09:55:59
INFO
Configuration descriptor contains descriptor of type : 0xB (Interface Association Descriptor)
INFO
Configuration descriptor contains descriptor of type : 0x4 (Interface Descriptor)
INFO
Configuration descriptor contains descriptor of type : 0x24
INFO
Configuration descriptor contains descriptor of type : 0x24
INFO
Configuration descriptor contains descriptor of type : 0x24
INFO
Configuration descriptor contains descriptor of type : 0x24
INFO
Configuration descriptor contains descriptor of type : 0x5 (Endpoint Descriptor)
INFO
Configuration descriptor contains descriptor of type : 0x4 (Interface Descriptor)
INFO
Configuration descriptor contains descriptor of type : 0x5 (Endpoint Descriptor)
INFO
Configuration descriptor contains descriptor of type : 0x5 (Endpoint Descriptor)
INFO
Configuration descriptor contains descriptor of type : 0x4 (Interface Descriptor)
INFO
Configuration descriptor contains descriptor of type : 0x21 (HID Descriptor)
INFO
Configuration descriptor contains descriptor of type : 0x5 (Endpoint Descriptor)
INFO
Configuration descriptor contains descriptor of type : 0x4 (Interface Descriptor)
INFO
Configuration descriptor contains descriptor of type : 0x21 (HID Descriptor)
INFO
Configuration descriptor contains descriptor of type : 0x5 (Endpoint Descriptor)
INFO
Configuration descriptor contains descriptor of type : 0x4 (Interface Descriptor)
INFO
Configuration descriptor contains descriptor of type : 0x21 (HID Descriptor)
INFO
Configuration descriptor contains descriptor of type : 0x5 (Endpoint Descriptor)
INFO
Configuration descriptor contains descriptor of type : 0x5 (Endpoint Descriptor)
INFO
Number of interface descriptors found 0x5
INFO
Number of alternate interface descriptors found : 0x0
INFO
Number of endpoint descriptors found : 0x7
INFO
Configuration descriptor length : 0x9
INFO
Configuration descriptor type : 0x2
INFO
Configuration descriptor TotalLength : 0x9D
INFO
Configuration descriptor NumInterfaces : 0x5
INFO
Configuration descriptor ConfigurationValue: 0x1
INFO
Checking iConfiguration String Descriptor: index = 0x00.
INFO
The device omits this string descriptor.
INFO
Configuration descriptor bmAttributes : 0xA0
INFO
Device supports remote wake up
INFO
MaxPower = 250 PowerMultiplier = 2
INFO
Maximum power device requires : 500mA
INFO
Device is BUS POWERED
INFO
Stop time: Apr 10, 2023 - 09:56:00
INFO
Duration: 1 second.
INFO
Stopping Test [ TD 9.2 - Configuration Descriptor Test (Configuration Index 0) - addressed: Number of: Fails (0); Aborts (0); Warnings (0) ]
TD 9.3 Interface Association Descriptor Test (Config 0)
Passed
INFO
Start time: Apr 10, 2023 - 09:56:00
INFO
Device has 4 functions, of which 1 has an Interface Association descriptor.
INFO
Interface Association Descriptor :
INFO
bLength = 0x08
INFO
bDescriptorType = 0x0b
INFO
bFirstInterface = 0
INFO
bInterfaceCount = 2
INFO
bFunctionClass = 0x02
INFO
bFunctionSubClass = 0x02
INFO
bFunctionProtocol = 0x01
INFO
iFunction = 0x00
INFO
Running TD 9.8 : String Descriptor Test for iFunction : 0x00.
INFO
Checking iFunction String Descriptor: index = 0x00.
INFO
The device omits this string descriptor.
INFO
Found Interface Descriptor with number : 0
INFO
Found Interface Descriptor with number : 1
INFO
Function #2 does not have an Interface Association Descriptor.
INFO
Function #3 does not have an Interface Association Descriptor.
INFO
Function #4 does not have an Interface Association Descriptor.
INFO
INFO
Stop time: Apr 10, 2023 - 09:56:01
INFO
Duration: 1 second.
INFO
Stopping Test [ TD 9.3 Interface Association Descriptor Test (Config 0): Number of: Fails (0); Aborts (0); Warnings (0) ]
TD 9.4 - Interface Descriptor Test (Configuration Index 0) - addressed
Passed
INFO
Start time: Apr 10, 2023 - 09:56:01
INFO
Bandwidth check passed
INFO
Testing Interface number : 0x0 Alternate setting : 0x0
INFO
Interface descriptor length : 0x9
INFO
Interface descriptor bDescriptorType : 0x4
INFO
Interface descriptor bAlternateSetting : 0x0
INFO
Interface descriptor bNumEndPoints: 0x1
INFO
Interface descriptor bInterfaceClass reserved for assignment by the USB-IF : 0x02.
INFO
Interface class code indicates [CDC-Control] Interface.
INFO
Interface sub class : 2 <not defined>
INFO
Interface protocol : 1 <not defined>
INFO
Interface descriptor bInterfaceSubClass : 0x02.
INFO
Interface descriptor bInterfaceProtocol assigned by the USB-IF : 0x01.
INFO
Interface descriptor iInterface : 0x0
INFO
Testing Interface number : 0x1 Alternate setting : 0x0
INFO
Interface descriptor length : 0x9
INFO
Interface descriptor bDescriptorType : 0x4
INFO
Interface descriptor bAlternateSetting : 0x0
INFO
Interface descriptor bNumEndPoints: 0x2
INFO
Interface descriptor bInterfaceClass reserved for assignment by the USB-IF : 0x0A.
INFO
Interface class code indicates [CDC-Data] Interface.
INFO
Interface sub class : 0 <not defined>
INFO
Interface protocol : 0 <not defined>
INFO
Interface descriptor bInterfaceSubClass : 0x00.
INFO
Device does not use a class-specific protocol on this interface.
INFO
Interface descriptor iInterface : 0x0
INFO
Testing Interface number : 0x2 Alternate setting : 0x0
INFO
Interface descriptor length : 0x9
INFO
Interface descriptor bDescriptorType : 0x4
INFO
Interface descriptor bAlternateSetting : 0x0
INFO
Interface descriptor bNumEndPoints: 0x1
INFO
Interface descriptor bInterfaceClass reserved for assignment by the USB-IF : 0x03.
INFO
Interface class code indicates [HID] Interface.
INFO
Interface sub class : 1 <not defined>
INFO
Interface protocol : 1 <not defined>
INFO
Interface descriptor bInterfaceSubClass : 0x01.
INFO
Interface descriptor bInterfaceProtocol assigned by the USB-IF : 0x01.
INFO
Interface descriptor iInterface : 0x0
INFO
Testing Interface number : 0x3 Alternate setting : 0x0
INFO
Interface descriptor length : 0x9
INFO
Interface descriptor bDescriptorType : 0x4
INFO
Interface descriptor bAlternateSetting : 0x0
INFO
Interface descriptor bNumEndPoints: 0x1
INFO
Interface descriptor bInterfaceClass reserved for assignment by the USB-IF : 0x03.
INFO
Interface class code indicates [HID] Interface.
INFO
Interface sub class : 0 <not defined>
INFO
Interface protocol : 0 <not defined>
INFO
Interface descriptor bInterfaceSubClass : 0x00.
INFO
Device does not use a class-specific protocol on this interface.
INFO
Interface descriptor iInterface : 0x0
INFO
Testing Interface number : 0x4 Alternate setting : 0x0
INFO
Interface descriptor length : 0x9
INFO
Interface descriptor bDescriptorType : 0x4
INFO
Interface descriptor bAlternateSetting : 0x0
INFO
Interface descriptor bNumEndPoints: 0x2
INFO
Interface descriptor bInterfaceClass reserved for assignment by the USB-IF : 0x03.
INFO
Interface class code indicates [HID] Interface.
INFO
Interface sub class : 0 <not defined>
INFO
Interface protocol : 0 <not defined>
INFO
Interface descriptor bInterfaceSubClass : 0x00.
INFO
Device does not use a class-specific protocol on this interface.
INFO
Interface descriptor iInterface : 0x0
INFO
Stop time: Apr 10, 2023 - 09:56:02
INFO
Duration: 1 second.
INFO
Stopping Test [ TD 9.4 - Interface Descriptor Test (Configuration Index 0) - addressed: Number of: Fails (0); Aborts (0); Warnings (0) ]
TD 9.5 - Endpoint Descriptor Test (Configuration Index 0) - addressed
Passed
INFO
Start time: Apr 10, 2023 - 09:56:02
INFO
Testing Interface number : 0x0 Alternate setting : 0x0
INFO
Endpoint descriptor length : 0x7
INFO
Endpoint descriptor type : 0x5
INFO
Endpoint Type : Interrupt, Number : 0x3, Direction : IN
INFO
Endpoint descriptor bmAttributes : 0x3
INFO
Endpoint descriptor raw MaxPacketSize : 0xA
INFO
Endpoint descriptor interval : 0x1
INFO
Testing Interface number : 0x1 Alternate setting : 0x0
INFO
Endpoint descriptor length : 0x7
INFO
Endpoint descriptor type : 0x5
INFO
Endpoint Type : Bulk, Number : 0x4, Direction : IN
INFO
Endpoint descriptor bmAttributes : 0x2
INFO
Endpoint descriptor raw MaxPacketSize : 0x40
INFO
Endpoint descriptor interval : 0x0
INFO
Endpoint descriptor length : 0x7
INFO
Endpoint descriptor type : 0x5
INFO
Endpoint Type : Bulk, Number : 0x4, Direction : OUT
INFO
Endpoint descriptor bmAttributes : 0x2
INFO
Endpoint descriptor raw MaxPacketSize : 0x40
INFO
Endpoint descriptor interval : 0x0
INFO
Testing Interface number : 0x2 Alternate setting : 0x0
INFO
Endpoint descriptor length : 0x7
INFO
Endpoint descriptor type : 0x5
INFO
Endpoint Type : Interrupt, Number : 0x1, Direction : IN
INFO
Endpoint descriptor bmAttributes : 0x3
INFO
Endpoint descriptor raw MaxPacketSize : 0x8
INFO
Endpoint descriptor interval : 0x1
INFO
Testing Interface number : 0x3 Alternate setting : 0x0
INFO
Endpoint descriptor length : 0x7
INFO
Endpoint descriptor type : 0x5
INFO
Endpoint Type : Interrupt, Number : 0x2, Direction : IN
INFO
Endpoint descriptor bmAttributes : 0x3
INFO
Endpoint descriptor raw MaxPacketSize : 0x8
INFO
Endpoint descriptor interval : 0x1
INFO
Testing Interface number : 0x4 Alternate setting : 0x0
INFO
Endpoint descriptor length : 0x7
INFO
Endpoint descriptor type : 0x5
INFO
Endpoint Type : Interrupt, Number : 0x5, Direction : IN
INFO
Endpoint descriptor bmAttributes : 0x3
INFO
Endpoint descriptor raw MaxPacketSize : 0x40
INFO
Endpoint descriptor interval : 0x1
INFO
Endpoint descriptor length : 0x7
INFO
Endpoint descriptor type : 0x5
INFO
Endpoint Type : Interrupt, Number : 0x5, Direction : OUT
INFO
Endpoint descriptor bmAttributes : 0x3
INFO
Endpoint descriptor raw MaxPacketSize : 0x40
INFO
Endpoint descriptor interval : 0x1
INFO
Stop time: Apr 10, 2023 - 09:56:03
INFO
Duration: 1 second.
INFO
Stopping Test [ TD 9.5 - Endpoint Descriptor Test (Configuration Index 0) - addressed: Number of: Fails (0); Aborts (0); Warnings (0) ]
TD 9.7 - BOS Descriptor Test - Device State Addressed
Passed
INFO
Start time: Apr 10, 2023 - 09:56:03
INFO
Configuration Index 0x00 has a Configuration Value of 1
INFO
USB Version number of device: 1.10
INFO
Device supports version of the USB Protocol that does not support BOS Descriptor
INFO
Stop time: Apr 10, 2023 - 09:56:04
INFO
Duration: 1 second.
INFO
Stopping Test [ TD 9.7 - BOS Descriptor Test - Device State Addressed: Number of: Fails (0); Aborts (0); Warnings (0) ]
TD 9.30 Configuration Summary Descriptor Test - Device State Addressed
Passed
INFO
Start time: Apr 10, 2023 - 09:56:04
INFO
Initialized the device to the Addressed state.
INFO
Retrieved Device Descriptor.
INFO
Device Under Test supports USB Version 0x1.0x10.
INFO
Configuration Summary Descriptors are not supported in this version. (Requires BOS descriptor)
INFO
Stop time: Apr 10, 2023 - 09:56:05
INFO
Duration: 1 second.
INFO
Stopping Test [ TD 9.30 Configuration Summary Descriptor Test - Device State Addressed: Number of: Fails (0); Aborts (0); Warnings (0) ]
TD 9.1 - Device Descriptor Test (Configuration Index 0) - configured
Passed
INFO
Start time: Apr 10, 2023 - 09:56:06
INFO
Device descriptor length : 0x12
INFO
Device descriptor type : 0x1
INFO
Major version : 0x1
INFO
Minor version : 0x10
INFO
Device supports different class spec. on different interfaces : 0xEF
INFO
Device class code indicates [Miscellaneous-Device] Device.
INFO
Device sub class : 2 (Common class)
INFO
Device protocol : 1 (Interface Association Descriptor)
INFO
Device sub class : 0x2
INFO
Device protocol : 0x1
INFO
Device MaxPacketSize0 : 0x40
INFO
Vendor information for VendorID : 0xE6A, Megawin Technology Co., Ltd.
INFO
Device ProductID : 0x32C
INFO
Device BCD : 0x100
INFO
Checking iManufacturer String Descriptor: index = 0x01.
INFO
String Descriptor : "Megawin Technology Inc.". (ENGLISH_US)
INFO
Checking iProduct String Descriptor: index = 0x02.
INFO
String Descriptor : "USB Keyboard with EasyCOM & EasyHID". (ENGLISH_US)
INFO
Checking iSerialNumber String Descriptor: index = 0x03.
INFO
String Descriptor : "V1.00". (ENGLISH_US)
INFO
Number of configurations device supports : 0x1
INFO
Stop time: Apr 10, 2023 - 09:56:07
INFO
Duration: 1 second.
INFO
Stopping Test [ TD 9.1 - Device Descriptor Test (Configuration Index 0) - configured: Number of: Fails (0); Aborts (0); Warnings (0) ]
TD 9.2 - Configuration Descriptor Test (Configuration Index 0) - configured
Passed
INFO
Start time: Apr 10, 2023 - 09:56:07
INFO
Configuration descriptor contains descriptor of type : 0xB (Interface Association Descriptor)
INFO
Configuration descriptor contains descriptor of type : 0x4 (Interface Descriptor)
INFO
Configuration descriptor contains descriptor of type : 0x24
INFO
Configuration descriptor contains descriptor of type : 0x24
INFO
Configuration descriptor contains descriptor of type : 0x24
INFO
Configuration descriptor contains descriptor of type : 0x24
INFO
Configuration descriptor contains descriptor of type : 0x5 (Endpoint Descriptor)
INFO
Configuration descriptor contains descriptor of type : 0x4 (Interface Descriptor)
INFO
Configuration descriptor contains descriptor of type : 0x5 (Endpoint Descriptor)
INFO
Configuration descriptor contains descriptor of type : 0x5 (Endpoint Descriptor)
INFO
Configuration descriptor contains descriptor of type : 0x4 (Interface Descriptor)
INFO
Configuration descriptor contains descriptor of type : 0x21 (HID Descriptor)
INFO
Configuration descriptor contains descriptor of type : 0x5 (Endpoint Descriptor)
INFO
Configuration descriptor contains descriptor of type : 0x4 (Interface Descriptor)
INFO
Configuration descriptor contains descriptor of type : 0x21 (HID Descriptor)
INFO
Configuration descriptor contains descriptor of type : 0x5 (Endpoint Descriptor)
INFO
Configuration descriptor contains descriptor of type : 0x4 (Interface Descriptor)
INFO
Configuration descriptor contains descriptor of type : 0x21 (HID Descriptor)
INFO
Configuration descriptor contains descriptor of type : 0x5 (Endpoint Descriptor)
INFO
Configuration descriptor contains descriptor of type : 0x5 (Endpoint Descriptor)
INFO
Number of interface descriptors found 0x5
INFO
Number of alternate interface descriptors found : 0x0
INFO
Number of endpoint descriptors found : 0x7
INFO
Configuration descriptor length : 0x9
INFO
Configuration descriptor type : 0x2
INFO
Configuration descriptor TotalLength : 0x9D
INFO
Configuration descriptor NumInterfaces : 0x5
INFO
Configuration descriptor ConfigurationValue: 0x1
INFO
Checking iConfiguration String Descriptor: index = 0x00.
INFO
The device omits this string descriptor.
INFO
Configuration descriptor bmAttributes : 0xA0
INFO
Device supports remote wake up
INFO
MaxPower = 250 PowerMultiplier = 2
INFO
Maximum power device requires : 500mA
INFO
Device is BUS POWERED
INFO
Device is currently BUS POWERED
INFO
Currently remote wakeup is DISABLED
INFO
Stop time: Apr 10, 2023 - 09:56:08
INFO
Duration: 1 second.
INFO
Stopping Test [ TD 9.2 - Configuration Descriptor Test (Configuration Index 0) - configured: Number of: Fails (0); Aborts (0); Warnings (0) ]
TD 9.3 Interface Association Descriptor Test (Config 0)
Passed
INFO
Start time: Apr 10, 2023 - 09:56:08
INFO
Device has 4 functions, of which 1 has an Interface Association descriptor.
INFO
Interface Association Descriptor :
INFO
bLength = 0x08
INFO
bDescriptorType = 0x0b
INFO
bFirstInterface = 0
INFO
bInterfaceCount = 2
INFO
bFunctionClass = 0x02
INFO
bFunctionSubClass = 0x02
INFO
bFunctionProtocol = 0x01
INFO
iFunction = 0x00
INFO
Running TD 9.8 : String Descriptor Test for iFunction : 0x00.
INFO
Checking iFunction String Descriptor: index = 0x00.
INFO
The device omits this string descriptor.
INFO
Found Interface Descriptor with number : 0
INFO
Found Interface Descriptor with number : 1
INFO
Function #2 does not have an Interface Association Descriptor.
INFO
Function #3 does not have an Interface Association Descriptor.
INFO
Function #4 does not have an Interface Association Descriptor.
INFO
INFO
Stop time: Apr 10, 2023 - 09:56:09
INFO
Duration: 1 second.
INFO
Stopping Test [ TD 9.3 Interface Association Descriptor Test (Config 0): Number of: Fails (0); Aborts (0); Warnings (0) ]
TD 9.4 - Interface Descriptor Test (Configuration Index 0) - configured
Passed
INFO
Start time: Apr 10, 2023 - 09:56:09
INFO
Bandwidth check passed
INFO
Testing Interface number : 0x0 Alternate setting : 0x0
INFO
Interface descriptor length : 0x9
INFO
Interface descriptor bDescriptorType : 0x4
INFO
Interface descriptor bAlternateSetting : 0x0
INFO
Interface descriptor bNumEndPoints: 0x1
INFO
Interface descriptor bInterfaceClass reserved for assignment by the USB-IF : 0x02.
INFO
Interface class code indicates [CDC-Control] Interface.
INFO
Interface sub class : 2 <not defined>
INFO
Interface protocol : 1 <not defined>
INFO
Interface descriptor bInterfaceSubClass : 0x02.
INFO
Interface descriptor bInterfaceProtocol assigned by the USB-IF : 0x01.
INFO
Interface descriptor iInterface : 0x0
INFO
Testing Interface number : 0x1 Alternate setting : 0x0
INFO
Interface descriptor length : 0x9
INFO
Interface descriptor bDescriptorType : 0x4
INFO
Interface descriptor bAlternateSetting : 0x0
INFO
Interface descriptor bNumEndPoints: 0x2
INFO
Interface descriptor bInterfaceClass reserved for assignment by the USB-IF : 0x0A.
INFO
Interface class code indicates [CDC-Data] Interface.
INFO
Interface sub class : 0 <not defined>
INFO
Interface protocol : 0 <not defined>
INFO
Interface descriptor bInterfaceSubClass : 0x00.
INFO
Device does not use a class-specific protocol on this interface.
INFO
Interface descriptor iInterface : 0x0
INFO
Testing Interface number : 0x2 Alternate setting : 0x0
INFO
Interface descriptor length : 0x9
INFO
Interface descriptor bDescriptorType : 0x4
INFO
Interface descriptor bAlternateSetting : 0x0
INFO
Interface descriptor bNumEndPoints: 0x1
INFO
Interface descriptor bInterfaceClass reserved for assignment by the USB-IF : 0x03.
INFO
Interface class code indicates [HID] Interface.
INFO
Interface sub class : 1 <not defined>
INFO
Interface protocol : 1 <not defined>
INFO
Interface descriptor bInterfaceSubClass : 0x01.
INFO
Interface descriptor bInterfaceProtocol assigned by the USB-IF : 0x01.
INFO
Interface descriptor iInterface : 0x0
INFO
Testing Interface number : 0x3 Alternate setting : 0x0
INFO
Interface descriptor length : 0x9
INFO
Interface descriptor bDescriptorType : 0x4
INFO
Interface descriptor bAlternateSetting : 0x0
INFO
Interface descriptor bNumEndPoints: 0x1
INFO
Interface descriptor bInterfaceClass reserved for assignment by the USB-IF : 0x03.
INFO
Interface class code indicates [HID] Interface.
INFO
Interface sub class : 0 <not defined>
INFO
Interface protocol : 0 <not defined>
INFO
Interface descriptor bInterfaceSubClass : 0x00.
INFO
Device does not use a class-specific protocol on this interface.
INFO
Interface descriptor iInterface : 0x0
INFO
Testing Interface number : 0x4 Alternate setting : 0x0
INFO
Interface descriptor length : 0x9
INFO
Interface descriptor bDescriptorType : 0x4
INFO
Interface descriptor bAlternateSetting : 0x0
INFO
Interface descriptor bNumEndPoints: 0x2
INFO
Interface descriptor bInterfaceClass reserved for assignment by the USB-IF : 0x03.
INFO
Interface class code indicates [HID] Interface.
INFO
Interface sub class : 0 <not defined>
INFO
Interface protocol : 0 <not defined>
INFO
Interface descriptor bInterfaceSubClass : 0x00.
INFO
Device does not use a class-specific protocol on this interface.
INFO
Interface descriptor iInterface : 0x0
INFO
Stop time: Apr 10, 2023 - 09:56:10
INFO
Duration: 1 second.
INFO
Stopping Test [ TD 9.4 - Interface Descriptor Test (Configuration Index 0) - configured: Number of: Fails (0); Aborts (0); Warnings (0) ]
TD 9.5 - Endpoint Descriptor Test (Configuration Index 0) - configured
Passed
INFO
Start time: Apr 10, 2023 - 09:56:10
INFO
Testing Interface number : 0x0 Alternate setting : 0x0
INFO
Endpoint descriptor length : 0x7
INFO
Endpoint descriptor type : 0x5
INFO
Endpoint Type : Interrupt, Number : 0x3, Direction : IN
INFO
Endpoint descriptor bmAttributes : 0x3
INFO
Endpoint descriptor raw MaxPacketSize : 0xA
INFO
Endpoint descriptor interval : 0x1
INFO
Testing Interface number : 0x1 Alternate setting : 0x0
INFO
Endpoint descriptor length : 0x7
INFO
Endpoint descriptor type : 0x5
INFO
Endpoint Type : Bulk, Number : 0x4, Direction : IN
INFO
Endpoint descriptor bmAttributes : 0x2
INFO
Endpoint descriptor raw MaxPacketSize : 0x40
INFO
Endpoint descriptor interval : 0x0
INFO
Endpoint descriptor length : 0x7
INFO
Endpoint descriptor type : 0x5
INFO
Endpoint Type : Bulk, Number : 0x4, Direction : OUT
INFO
Endpoint descriptor bmAttributes : 0x2
INFO
Endpoint descriptor raw MaxPacketSize : 0x40
INFO
Endpoint descriptor interval : 0x0
INFO
Testing Interface number : 0x2 Alternate setting : 0x0
INFO
Endpoint descriptor length : 0x7
INFO
Endpoint descriptor type : 0x5
INFO
Endpoint Type : Interrupt, Number : 0x1, Direction : IN
INFO
Endpoint descriptor bmAttributes : 0x3
INFO
Endpoint descriptor raw MaxPacketSize : 0x8
INFO
Endpoint descriptor interval : 0x1
INFO
Testing Interface number : 0x3 Alternate setting : 0x0
INFO
Endpoint descriptor length : 0x7
INFO
Endpoint descriptor type : 0x5
INFO
Endpoint Type : Interrupt, Number : 0x2, Direction : IN
INFO
Endpoint descriptor bmAttributes : 0x3
INFO
Endpoint descriptor raw MaxPacketSize : 0x8
INFO
Endpoint descriptor interval : 0x1
INFO
Testing Interface number : 0x4 Alternate setting : 0x0
INFO
Endpoint descriptor length : 0x7
INFO
Endpoint descriptor type : 0x5
INFO
Endpoint Type : Interrupt, Number : 0x5, Direction : IN
INFO
Endpoint descriptor bmAttributes : 0x3
INFO
Endpoint descriptor raw MaxPacketSize : 0x40
INFO
Endpoint descriptor interval : 0x1
INFO
Endpoint descriptor length : 0x7
INFO
Endpoint descriptor type : 0x5
INFO
Endpoint Type : Interrupt, Number : 0x5, Direction : OUT
INFO
Endpoint descriptor bmAttributes : 0x3
INFO
Endpoint descriptor raw MaxPacketSize : 0x40
INFO
Endpoint descriptor interval : 0x1
INFO
Stop time: Apr 10, 2023 - 09:56:11
INFO
Duration: 1 second.
INFO
Stopping Test [ TD 9.5 - Endpoint Descriptor Test (Configuration Index 0) - configured: Number of: Fails (0); Aborts (0); Warnings (0) ]
TD 9.7 - BOS Descriptor Test (Configuration Index 0) - Device State Configured
Passed
INFO
Start time: Apr 10, 2023 - 09:56:11
INFO
Configuration Index 0x00 has a Configuration Value of 1
INFO
Initializing the device to the Configured state with Configuration Value 1
INFO
USB Version number of device: 1.10
INFO
Device supports version of the USB Protocol that does not support BOS Descriptor
INFO
Stop time: Apr 10, 2023 - 09:56:12
INFO
Duration: 1 second.
INFO
Stopping Test [ TD 9.7 - BOS Descriptor Test (Configuration Index 0) - Device State Configured: Number of: Fails (0); Aborts (0); Warnings (0) ]
TD 9.9 - Halt Endpoint Test (Configuration Index 0)
Passed
INFO
Start time: Apr 10, 2023 - 09:56:12
INFO
Testing Interface number : 0x0 Alternate setting : 0x0
INFO
Testing EndPoint type : Interrupt, Address : 0x83
INFO
Endpoint is currently not halted for endpoint 0x83
INFO
Setting feature endpoint halt for endpoint 0x83
INFO
Endpoint is halted for endpoint 0x83
INFO
Clearing feature endpoint halt for endpoint 0x83
INFO
Endpoint is no longer halted for endpoint 0x83
INFO
Testing Interface number : 0x1 Alternate setting : 0x0
INFO
Testing EndPoint type : Bulk, Address : 0x84
INFO
Endpoint is currently not halted for endpoint 0x84
INFO
Setting feature endpoint halt for endpoint 0x84
INFO
Endpoint is halted for endpoint 0x84
INFO
Clearing feature endpoint halt for endpoint 0x84
INFO
Endpoint is no longer halted for endpoint 0x84
INFO
Testing EndPoint type : Bulk, Address : 0x4
INFO
Endpoint is currently not halted for endpoint 0x04
INFO
Setting feature endpoint halt for endpoint 0x04
INFO
Endpoint is halted for endpoint 0x04
INFO
Clearing feature endpoint halt for endpoint 0x04
INFO
Endpoint is no longer halted for endpoint 0x04
INFO
Testing Interface number : 0x2 Alternate setting : 0x0
INFO
Testing EndPoint type : Interrupt, Address : 0x81
INFO
Endpoint is currently not halted for endpoint 0x81
INFO
Setting feature endpoint halt for endpoint 0x81
INFO
Endpoint is halted for endpoint 0x81
INFO
Clearing feature endpoint halt for endpoint 0x81
INFO
Endpoint is no longer halted for endpoint 0x81
INFO
Testing Interface number : 0x3 Alternate setting : 0x0
INFO
Testing EndPoint type : Interrupt, Address : 0x82
INFO
Endpoint is currently not halted for endpoint 0x82
INFO
Setting feature endpoint halt for endpoint 0x82
INFO
Endpoint is halted for endpoint 0x82
INFO
Clearing feature endpoint halt for endpoint 0x82
INFO
Endpoint is no longer halted for endpoint 0x82
INFO
Testing Interface number : 0x4 Alternate setting : 0x0
INFO
Testing EndPoint type : Interrupt, Address : 0x85
INFO
Endpoint is currently not halted for endpoint 0x85
INFO
Setting feature endpoint halt for endpoint 0x85
INFO
Endpoint is halted for endpoint 0x85
INFO
Clearing feature endpoint halt for endpoint 0x85
INFO
Endpoint is no longer halted for endpoint 0x85
INFO
Testing EndPoint type : Interrupt, Address : 0x5
INFO
Endpoint is currently not halted for endpoint 0x05
INFO
Setting feature endpoint halt for endpoint 0x05
INFO
Endpoint is halted for endpoint 0x05
INFO
Clearing feature endpoint halt for endpoint 0x05
INFO
Endpoint is no longer halted for endpoint 0x05
INFO
Stop time: Apr 10, 2023 - 09:56:13
INFO
Duration: 1 second.
INFO
Stopping Test [ TD 9.9 - Halt Endpoint Test (Configuration Index 0): Number of: Fails (0); Aborts (0); Warnings (0) ]
TD 9.13 - SetConfiguration Test (Configuration Index 0)
Passed
INFO
Start time: Apr 10, 2023 - 09:56:13
INFO
SetConfiguration with configuration value : 0x1
INFO
Unconfigured the device
INFO
SetConfiguration with configuration value : 0x1
INFO
Stop time: Apr 10, 2023 - 09:56:14
INFO
Duration: 1 second.
INFO
Stopping Test [ TD 9.13 - SetConfiguration Test (Configuration Index 0): Number of: Fails (0); Aborts (0); Warnings (0) ]
TD 9.30 Configuration Summary Descriptor Test (Configuration Index 0x00) - Device State Configured
Passed
INFO
Start time: Apr 10, 2023 - 09:56:14
INFO
Configuration Index 0x00 has a Configuration Value of 1.
INFO
Initialized the device to the Configured state with Configuration Value 1.
INFO
Retrieved Device Descriptor.
INFO
Device Under Test supports USB Version 0x1.0x10.
INFO
Configuration Summary Descriptors are not supported in this version. (Requires BOS descriptor)
INFO
Stop time: Apr 10, 2023 - 09:56:15
INFO
Duration: 1 second.
INFO
Stopping Test [ TD 9.30 Configuration Summary Descriptor Test (Configuration Index 0x00) - Device State Configured: Number of: Fails (0); Aborts (0); Warnings (0) ]
TD 9.14 - Suspend/Resume Test (Configuration Index 0)
Passed
INFO
Start time: Apr 10, 2023 - 09:56:15
INFO
Suspended the parent port of the Device Under Test.
INFO
Resumed the parent port of the Device Under Test.
INFO
Got device descriptor of Device Under Test
INFO
Stop time: Apr 10, 2023 - 09:56:16
INFO
Duration: 1 second.
INFO
Stopping Test [ TD 9.14 - Suspend/Resume Test (Configuration Index 0): Number of: Fails (0); Aborts (0); Warnings (0) ]
TD 9.12 - Remote Wakeup Test (Configuration Index 0) - Enabled:
Passed
INFO
Start time: Apr 10, 2023 - 09:56:16
INFO
Suspended the parent port of the device
INFO
Parent port saw remote wakeup
INFO
Received a remote wake up event
INFO
Stop time: Apr 10, 2023 - 09:56:18
INFO
Duration: 2 seconds.
INFO
Stopping Test [ TD 9.12 - Remote Wakeup Test (Configuration Index 0) - Enabled:: Number of: Fails (0); Aborts (0); Warnings (0) ]
TD 9.12 - Remote Wakeup Test (Configuration Index 0) - Disabled:
Passed
INFO
Start time: Apr 10, 2023 - 09:56:18
INFO
Suspended the parent port of the device
INFO
Did not receive a wakeup event on the test device with remote wakeup disabled
INFO
Stop time: Apr 10, 2023 - 09:56:23
INFO
Duration: 5 seconds.
INFO
Stopping Test [ TD 9.12 - Remote Wakeup Test (Configuration Index 0) - Disabled:: Number of: Fails (0); Aborts (0); Warnings (0) ]
L1Suspend/Resume Test (Configuration Index 0)
Passed
INFO
Start time: Apr 10, 2023 - 09:56:23
INFO
Checking Device Under Test for LPM L1 Compatibility...
INFO
USB version of device is 1.10.
INFO
DUT is NOT compatible with LPM.
INFO
LPM is NOT required for DUT
INFO
LPM is only supported in USB version 2.01 and above.
INFO
Stop time: Apr 10, 2023 - 09:56:24
INFO
Duration: 1 second.
INFO
Stopping Test [ L1Suspend/Resume Test (Configuration Index 0): Number of: Fails (0); Aborts (0); Warnings (0) ]
TD 9.16 - Enumeration Test(repeat 150 times)
Passed
INFO
Start time: Apr 10, 2023 - 09:56:24
INFO
Device speed is Full.
INFO
Beginning enumeration test with 150 enumerations. This may take several minutes to complete.
INFO
Enumerated 150 iterations.
INFO
Device tree re-enumerated.
INFO
Recovered Device Under Test after device tree re-enumeration.
INFO
Device speed of Device Under Test: Full Speed.
INFO
Stop time: Apr 10, 2023 - 09:57:15
INFO
Duration: 51 seconds.
INFO
Stopping Test [ TD 9.16 - Enumeration Test(repeat 150 times): Number of: Fails (0); Aborts (0); Warnings (0) ]
Display Other Tests To Run
INFO
Informed user: run Connector Type Tests on this device.
INFO
Informed user: run HID Tests on this device.
Summary
INFO
TEST SUITE SUMMARY: [ Fails (0); Aborts (0); Warnings (0) ]
INFO
TEST RESULTS: [ Passed (28); Failed (0) ]