IEC60730 Project

H/W resource:
	It will spend 2 interrupt resource if User wants to verify interrupt test.
	The interrupt resource is TM00 & TM10.
	
IEC60730 clcok:
	The IEC60730 always keep in 12MHz that is IHRCO clocks source.
	
Test procedure:
	Power or Reset -> running IEC60730 test item (User can decide which ones can be executed) -> main()
	
	
