APPLICATION: USB 3 Gen X Command Verifier
TEST SUITE: HID Tests.cvtests
OPERATING SYSTEM:
WORKSTATION: R140LUCASYANG
DATE: Wednesday, November 23, 2022
TIME: 02:15:04 PM
OPERATOR: LucasYang
NUMBER OF TESTS: 5
LOG NAME: HID Tests - 2022-11-23 14-14-50
RESULT: passed

Initialize Test Suite
INFO
Test log initialized.
INFO
Log Level: Normal
INFO
User Input module initialized
INFO
Windows 10 Pro (Build 19041.1.amd64fre.vb_release.191206-1406)
INFO
CVApp.exe ver 4.1.0.0
INFO
BaseUtilities.dll ver 4.1.0.0
INFO
CommandVerifierLog.dll ver 4.1.0.0
INFO
GuiHelper.dll ver 4.1.0.0
INFO
TestUtilities.dll ver 4.1.0.0
INFO
TestSuiteEngine.dll ver 4.1.0.0
INFO
xhci_DevIOCTL.dll ver 2.2.7.0
INFO
xhci_TestServices.dll ver 2.2.7.0
INFO
USBUtilities.dll ver 1.4.5.1
INFO
StackSwitcher.dll ver 1.4.5.1
INFO
xhci_CommandVerifierServices.dll ver 2.2.7.0
INFO
VIFReader.dll ver 4.1.0.0
INFO
TParse.dll ver 1.4.5.0
INFO
xhci_HIDTests.dll ver 2.2.7.0
INFO
XHCISpecVersion: 1.20.
INFO
Host 1 selected: xHCI Host: VID=0x8086, PID=0x43ED (PCI /A� 0 �n 20 �x 0)
INFO
User selection from list: "FS Device (HID) addr=2: VID=0E6A, PID=032D"
INFO
Please select HID Device to test
INFO
HID Device Under Test is operating at Full Speed.
INFO
Topology: XHCI HC -- DUT
Get Number Of Configurations
INFO
USB Version number of device: 1.10
INFO
Number of configurations: 1.
Get Number Of Configurations - Other Speed
INFO
Number of Other Speed configurations: 0.
HID Class WhichSpecCompliant Test
Passed
INFO
Start time: Nov 23, 2022 - 14:14:58
INFO
USB Version number of device: 1.10
INFO
Interface 0x2 Alternate Setting 0x0 is draft 4 Compliant
INFO
Stop time: Nov 23, 2022 - 14:14:59
INFO
Duration: 1 second.
INFO
Stopping Test [ HID Class WhichSpecCompliant Test: Number of: Fails (0); Aborts (0); Warnings (0) ]
HID Class Descriptor Test (Configuration Index 0) - configured
Passed
INFO
Start time: Nov 23, 2022 - 14:14:59
WARNING
DeviceClass is NON ZERO
WARNING
DeviceSubClass is NON ZERO
WARNING
DeviceProtocol is NON ZERO
INFO
Testing HID descriptor for Interface 0x2
INFO
HID descriptor total length : 0x9
INFO
HID descriptor type : 0x21
INFO
HID specification version : 0x111
INFO
CountryCode : 0x0
INFO
Number of other descriptors present : 0x1
INFO
HID report descriptor length : 0x1D
INFO
Stop time: Nov 23, 2022 - 14:15:01
INFO
Duration: 2 seconds.
INFO
Stopping Test [ HID Class Descriptor Test (Configuration Index 0) - configured: Number of: Fails (0); Aborts (0); Warnings (3) ]
HID Class Protocol Test (Configuration Index 0)
Passed
INFO
Start time: Nov 23, 2022 - 14:15:01
INFO
Starting GET/SET protocol tests for interface : 2
INFO
GET/SET protocol request is optional. Skipping tests
INFO
Stop time: Nov 23, 2022 - 14:15:02
INFO
Duration: 1 second.
INFO
Stopping Test [ HID Class Protocol Test (Configuration Index 0): Number of: Fails (0); Aborts (0); Warnings (0) ]
HID Class GET/SET Idle Test (Configuration Index 0)
Passed
INFO
Start time: Nov 23, 2022 - 14:15:02
INFO
No report IDs found in report descriptor for Interface : 0x2
INFO
GET/SETIdle test for report ID 0. Setting Idle rate to : 0x7F
INFO
Stop time: Nov 23, 2022 - 14:15:03
INFO
Duration: 1 second.
INFO
Stopping Test [ HID Class GET/SET Idle Test (Configuration Index 0): Number of: Fails (0); Aborts (0); Warnings (0) ]
HID Class Report Descriptor Test (Configuration Index 0)
Passed
INFO
Start time: Nov 23, 2022 - 14:15:03
INFO
Report descriptor length: 29
INFO
Item count in report descriptor: 14
INFO
Report descriptor test passed. Proceeding to next descriptor
INFO
Stop time: Nov 23, 2022 - 14:15:04
INFO
Duration: 1 second.
INFO
Stopping Test [ HID Class Report Descriptor Test (Configuration Index 0): Number of: Fails (0); Aborts (0); Warnings (0) ]
Summary
INFO
TEST SUITE SUMMARY: [ Fails (0); Aborts (0); Warnings (3) ]
INFO
TEST RESULTS: [ Passed (5); Failed (0) ]