MG32L003 Standard Peripherals Firmware Library

宏定义 | 函数 | 变量
cmsis_gcc.h 文件参考

CMSIS compiler GCC header file 更多...

浏览源代码.

## 宏定义
#define | __has_builtin(x) (0)
#define | __ASM __asm
#define | __INLINE inline
#define | __STATIC_INLINE static inline
#define | __STATIC_FORCEINLINE __attribute__((always_inline)) static inline
#define | __NO_RETURN __attribute__((__noreturn__))
#define | __USED __attribute__((used))
#define | __WEAK __attribute__((weak))
#define | __PACKED __attribute__((packed, aligned(1)))
#define | __PACKED_STRUCT struct __attribute__((packed, aligned(1)))
#define | __PACKED_UNION union __attribute__((packed, aligned(1)))
#define | __UNALIGNED_UINT32(x) (((struct T_UINT32 *)(x))->v)
#define | __UNALIGNED_UINT16_WRITE(addr, val) (void)((((struct T_UINT16_WRITE *)(void *)(addr))->v) = (val))
#define | __UNALIGNED_UINT16_READ(addr) (((const struct T_UINT16_READ *)(const void *)(addr))->v)
#define | __UNALIGNED_UINT32_WRITE(addr, val) (void)((((struct T_UINT32_WRITE *)(void *)(addr))->v) = (val))
#define | __UNALIGNED_UINT32_READ(addr) (((const struct T_UINT32_READ *)(const void *)(addr))->v)
#define | __ALIGNED(x) __attribute__((aligned(x)))
#define | __RESTRICT __restrict
#define | __CMSIS_GCC_OUT_REG(r) "=r" (r)
#define | __CMSIS_GCC_RW_REG(r) "+r" (r)
#define | __CMSIS_GCC_USE_REG(r) "r" (r)
#define | __NOP() __ASM volatile ("nop")
| No Operation 更多...
#define | __WFI() __ASM volatile ("wfi")
| Wait For Interrupt 更多...
#define | __WFE() __ASM volatile ("wfe")
| Wait For Event 更多...
#define | __SEV() __ASM volatile ("sev")
| Send Event 更多...
#define | __BKPT(value) __ASM volatile ("bkpt "#value)
| Breakpoint 更多...
#define | __CLZ (uint8_t)__builtin_clz
| Count leading zeros 更多...

## 函数
struct | __attribute__ ((packed)) T_UINT32
__STATIC_FORCEINLINE void | __enable_irq (void)
| Enable IRQ Interrupts 更多...
__STATIC_FORCEINLINE void | __disable_irq (void)
| Disable IRQ Interrupts 更多...
__STATIC_INLINE uint32_t | __get_CONTROL (void)
| Enable IRQ Interrupts 更多...
__STATIC_INLINE void | __set_CONTROL (uint32_t control)
| Set Control Register 更多...
__STATIC_INLINE uint32_t | __get_IPSR (void)
| Get IPSR Register 更多...
__STATIC_INLINE uint32_t | __get_APSR (void)
| Get APSR Register 更多...
__STATIC_INLINE uint32_t | __get_xPSR (void)
| Get xPSR Register 更多...
__STATIC_INLINE uint32_t | __get_PSP (void)
| Get Process Stack Pointer 更多...
__STATIC_INLINE void | __set_PSP (uint32_t topOfProcStack)
| Set Process Stack Pointer 更多...
__STATIC_INLINE uint32_t | __get_MSP (void)
| Get Main Stack Pointer 更多...
__STATIC_INLINE void | __set_MSP (uint32_t topOfMainStack)
| Set Main Stack Pointer 更多...
__STATIC_INLINE uint32_t | __get_PRIMASK (void)
| Get Priority Mask 更多...
__STATIC_INLINE void | __set_PRIMASK (uint32_t priMask)
| Set Priority Mask 更多...
__STATIC_INLINE uint32_t | __get_FPSCR (void)
| Get FPSCR 更多...
__STATIC_INLINE void | __set_FPSCR (uint32_t fpscr)
| Set FPSCR 更多...
__STATIC_FORCEINLINE void | __ISB (void)
| Instruction Synchronization Barrier 更多...
__STATIC_FORCEINLINE void | __DSB (void)
| Data Synchronization Barrier 更多...
__STATIC_FORCEINLINE void | __DMB (void)
| Data Memory Barrier 更多...
__STATIC_FORCEINLINE uint32_t | __REV (uint32_t value)
| Reverse byte order (32 bit) 更多...
__STATIC_FORCEINLINE uint32_t | __REV16 (uint32_t value)
| Reverse byte order (16 bit) 更多...
__STATIC_FORCEINLINE int16_t | __REVSH (int16_t value)
| Reverse byte order (16 bit) 更多...
__STATIC_FORCEINLINE uint32_t | __ROR (uint32_t op1, uint32_t op2)
| Rotate Right in unsigned value (32 bit) 更多...
__STATIC_FORCEINLINE uint32_t | __RBIT (uint32_t value)
| Reverse bit order of value 更多...
__STATIC_FORCEINLINE int32_t | __SSAT (int32_t val, uint32_t sat)
| Signed Saturate 更多...
__STATIC_FORCEINLINE uint32_t | __USAT (int32_t val, uint32_t sat)
| Unsigned Saturate 更多...

## 变量
__PACKED_STRUCT | T_UINT16_WRITE { uint16_t v
__PACKED_STRUCT | T_UINT16_READ { uint16_t v
__PACKED_STRUCT | T_UINT32_WRITE { uint32_t v
__PACKED_STRUCT | T_UINT32_READ { uint32_t v

## 详细描述

CMSIS compiler GCC header file

版本
  V5.0.4

日期
  09. April 2018