/**
  @page TIM10_Timing TIM10_Timing example
  
  @verbatim
  ****************** (C) COPYRIGHT 2023 megawin Technology *******************
  * @file    TIM10/TIM10_Timing/readme.txt 
  * @author  megawin Application Team
  * @version V0.0.5
  * @date    13-August-2024
  * @brief   Description of the TIM10 TIM10_Timing example.
  ******************************************************************************
  * THE PRESENT FIRMWARE WHICH IS FOR GUIDANCE ONLY AIMS AT PROVIDING CUSTOMERS
  * WITH CODING INFORMATION REGARDING THEIR PRODUCTS IN ORDER FOR THEM TO SAVE
  * TIME. AS A RESULT, MEGAWIN SHALL NOT BE HELD LIABLE FOR ANY DIRECT,
  * INDIRECT OR CONSEQUENTIAL DAMAGES WITH RESPECT TO ANY CLAIMS ARISING FROM
  * THE CONTENT OF SUCH FIRMWARE AND/OR THE USE MADE BY CUSTOMERS OF THE
  * CODING INFORMATION CONTAINED HEREIN IN CONNECTION WITH THEIR PRODUCTS.
  ******************************************************************************
   @endverbatim

@par 例程描述 

本例程演示如何使用TIM10的定时功能。

本例程系统时钟工作在24Mhz。

本例程中TIM10使能定时功能，采用重装载计数方式，重装载值65295，计数值到65535时产生中断并翻转PC4管脚，在PC4管脚上输出翻转速度100K的波形。


@par 目录内容 

  - TIM10/TIM10_Timing/TIM10_Timing.uvprojx   MDK5工程文件
  - TIM10/TIM10_Timing/TIM10_Timing.uvoptx    MDK5工程配置文件
  - TIM10/TIM10_Timing/JLinkSettings.ini      Jlink配置文件
  - TIM10/TIM10_Timing/main.c                 主程序


@par 硬件和软件环境 

  - 硬件平台搭建
    - 芯片管脚连接如下：
      - PC4 管脚连接示波器


@par 如何使用？ 

为了使程序工作，您必须执行以下操作 :
 - 使用 MDK5 打开此例程文件夹中的 TIM10_Timing.uvprojx 工程
 - 重新编译该工程并下载到目标存储器中
 - 运行此例程
   
 * <h3><center>&copy; COPYRIGHT 2023 megawin Technology</center></h3>
 */
