MG32L003 Standard Peripherals Firmware Library

函数
mg32l003_owire.c 文件参考

This file provides all the OWIRE firmware functions. 更多...

`#include "mg32l003_owire.h"`
`#include "mg32l003_rcc.h"`

## 函数
void | OWIRE_DeInit (void)
| Deinitializes the OWIRE peripheral registers to their default reset values. 更多...
void | OWIRE_Init (OWIRE_InitTypeDef *OWIRE_InitStruct)
| Initializes the OWIRE mode according to the specified parameters in the OWIRE_InitTypeDef and create the associated handler. 更多...
void | OWIRE_Cmd (FunctionalState NewState)
| Enables or disables the specified OWIRE peripheral. 更多...
void | OWIRE_ITConfig (uint32_t OWIRE_IT, FunctionalState NewState)
| Enables or disables the specified OWIRE interrupts. 更多...
uint8_t | OWIRE_ReadData (void)
| Read one data from DATA register. 更多...
void | OWIRE_WriteData (uint8_t Data)
| Write one data to DATA register. 更多...
void | OWIRE_WriteCommand (uint8_t Command)
| Write command to CMD register. 更多...
FlagStatus | OWIRE_GetFlagStatus (uint32_t OWIRE_FLAG)
| Checks whether the specified the OWIRE flag is set or not. 更多...
void | OWIRE_ClearFlag (uint32_t OWIRE_FLAG)
| Clears the OWIRE's pending flags. 更多...
ITStatus | OWIRE_GetITStatus (uint32_t OWIRE_IT)
| Checks whether the OWIRE interrupt has occurred or not. 更多...
void | OWIRE_ClearITPendingBit (uint32_t OWIRE_IT)
| Clears the OWIRE's interrupt pending bits. 更多...

## 详细描述

This file provides all the OWIRE firmware functions.

作者
  megawin Application Team

版本
  V0.0.5

日期
  13-August-2024