MG32L003 Standard Peripherals Firmware Library

模块 | 宏定义
TIM_Exported_constants
MG32L003_StdPeriph_Driver » BASETIM MG32L003_StdPeriph_Driver » | TIM

## 模块
| BaseTim_Gate_Enable_Disable
| BaseTim_GatePolarity
| BaseTim_Tog_Enable_Disable
| BaseTim_Function_Count_Timer
| BaseTim_AutoReload
| BaseTim_CountLevel
| BaseTim_CountMode
| BaseTim_Prescaler
| TIM_Output_Compare_and_PWM_modes
| TIM_One_Pulse_Mode
| TIM_Channel
| TIM_Clock_Division_CKD
| TIM_Counter_Mode
| TIM_Output_Compare_Polarity
| TIM_Output_Compare_N_Polarity
| TIM_Output_Compare_state
| TIM_Output_Compare_N_state
| TIM_Capture_Compare_state
| TIM_Capture_Compare_N_state
| Break_Input_enable_disable
| Break_Polarity
| TIM_AOE_Bit_Set_Reset
| Lock_level
| OSSI_Off_State_Selection_for_Idle_mode_state
| OSSR_Off_State_Selection_for_Run_mode_state
| TIM_Output_Compare_Idle_State
| TIM_Output_Compare_N_Idle_State
| TIM_Input_Capture_Polarity
| TIM_Input_Capture_Selection
| TIM_Input_Capture_Prescaler
| TIM_interrupt_sources
| TIM_External_Trigger_Prescaler
| TIM_Internal_Trigger_Selection
| TIM_TIx_External_Clock_Source
| TIM_External_Trigger_Polarity
| TIM_Prescaler_Reload_Mode
| TIM_Forced_Action
| TIM_Encoder_Mode
| TIM_Event_Source
| TIM_Update_Source
| TIM_Output_Compare_Preload_State
| TIM_Output_Compare_Fast_State
| TIM_Output_Compare_Clear_State
| TIM_Trigger_Output_Source
| TIM_Slave_Mode
| TIM_Master_Slave_Mode
| TIM_Flags
| TIM_Input_Capture_Filer_Value
| TIM_External_Trigger_Filter

## 宏定义
#define | IS_BaseTIM_ALL_PERIPH(PERIPH)
#define | IS_TIM_ALL_PERIPH(PERIPH)
#define | IS_TIM_LIST1_PERIPH(PERIPH) (((PERIPH) == TIM1))
#define | IS_TIM_LIST2_PERIPH(PERIPH) (((PERIPH) == TIM1))
#define | IS_TIM_LIST3_PERIPH(PERIPH)
#define | IS_TIM_LIST4_PERIPH(PERIPH)
#define | IS_TIM_LIST5_PERIPH(PERIPH)
#define | IS_TIM_LIST6_PERIPH(PERIPH)
#define | IS_TIM_LIST7_PERIPH(PERIPH)
#define | IS_TIM_LIST8_PERIPH(PERIPH)
#define | IS_TIM_LIST9_PERIPH(PERIPH)

## 详细描述

## 宏定义说明

## ◆ IS_BaseTIM_ALL_PERIPH

#define IS_BaseTIM_ALL_PERIPH | ( |  | PERIPH | ) |

值:
(((PERIPH) == TIM10) || \
((PERIPH) == TIM11))

## ◆ IS_TIM_ALL_PERIPH

#define IS_TIM_ALL_PERIPH | ( |  | PERIPH | ) |

值:
(((PERIPH) == TIM1) || \
((PERIPH) == TIM2))

## ◆ IS_TIM_LIST3_PERIPH

#define IS_TIM_LIST3_PERIPH | ( |  | PERIPH | ) |

值:
(((PERIPH) == TIM1) || \
((PERIPH) == TIM2))

## ◆ IS_TIM_LIST4_PERIPH

#define IS_TIM_LIST4_PERIPH | ( |  | PERIPH | ) |

值:
(((PERIPH) == TIM1) || \
((PERIPH) == TIM2))

## ◆ IS_TIM_LIST5_PERIPH

#define IS_TIM_LIST5_PERIPH | ( |  | PERIPH | ) |

值:
(((PERIPH) == TIM1) || \
((PERIPH) == TIM2))

## ◆ IS_TIM_LIST6_PERIPH

#define IS_TIM_LIST6_PERIPH | ( |  | PERIPH | ) |

值:
(((PERIPH) == TIM1) || \
((PERIPH) == TIM2))

## ◆ IS_TIM_LIST7_PERIPH

#define IS_TIM_LIST7_PERIPH | ( |  | PERIPH | ) |

值:
(((PERIPH) == TIM1) || \
((PERIPH) == TIM2))

## ◆ IS_TIM_LIST8_PERIPH

#define IS_TIM_LIST8_PERIPH | ( |  | PERIPH | ) |

值:
(((PERIPH) == TIM1) || \
((PERIPH) == TIM2))

## ◆ IS_TIM_LIST9_PERIPH

#define IS_TIM_LIST9_PERIPH | ( |  | PERIPH | ) |

值:
(((PERIPH) == TIM1) || \
((PERIPH) == TIM2))