MG32L003 Standard Peripherals Firmware Library

宏定义
TIM_External_Trigger_Prescaler
MG32L003_StdPeriph_Driver » BASETIM MG32L003_StdPeriph_Driver » | TIM » TIM_Exported_constants

## 宏定义
#define | TIM_ExtTRGPSC_OFF ((uint16_t)0x0000)
#define | TIM_ExtTRGPSC_DIV2 ((uint16_t)0x1000)
#define | TIM_ExtTRGPSC_DIV4 ((uint16_t)0x2000)
#define | TIM_ExtTRGPSC_DIV8 ((uint16_t)0x3000)
#define | IS_TIM_EXT_PRESCALER(PRESCALER)

## 详细描述

## 宏定义说明

## ◆ IS_TIM_EXT_PRESCALER

#define IS_TIM_EXT_PRESCALER | ( |  | PRESCALER | ) |

值:
(((PRESCALER) == TIM_ExtTRGPSC_OFF) || \
((PRESCALER) == TIM_ExtTRGPSC_DIV2) || \
((PRESCALER) == TIM_ExtTRGPSC_DIV4) || \
((PRESCALER) == TIM_ExtTRGPSC_DIV8))