MG32L003 Standard Peripherals Firmware Library

宏定义
VCMP_Out_Configuration
MG32L003_StdPeriph_Driver » VCMP » VCMP_Exported_Constants

## 宏定义
#define | VCMP_OUTCFG_INV_PAD (0x01 << VCMP_OUTCFG_INV_PAD_Pos)
#define | VCMP_OUTCFG_TIM1_BKE (0x01 << VCMP_OUTCFG_TIM1BKE_Pos)
#define | VCMP_OUTCFG_TIM1CH4_GATE (0x01 << VCMP_OUTCFG_TIM1CH4_EN_Pos)
#define | VCMP_OUTCFG_INV_TIM1CH4_GATE (0x01 << VCMP_OUTCFG_INV_TIM1CH4_Pos)
#define | VCMP_OUTCFG_TIM1CH3_GATE (0x01 << VCMP_OUTCFG_TIM1CH3_EN_Pos)
#define | VCMP_OUTCFG_INV_TIM1CH3_GATE (0x01 << VCMP_OUTCFG_INV_TIM1CH3_Pos)
#define | VCMP_OUTCFG_TIM1CH2_GATE (0x01 << VCMP_OUTCFG_TIM1CH2_EN_Pos)
#define | VCMP_OUTCFG_INV_TIM1CH2_GATE (0x01 << VCMP_OUTCFG_INV_TIM1CH2_Pos)
#define | VCMP_OUTCFG_TIM1CH1_GATE (0x01 << VCMP_OUTCFG_TIM1CH1_EN_Pos)
#define | VCMP_OUTCFG_INV_TIM1CH1_GATE (0x01 << VCMP_OUTCFG_INV_TIM1CH1_Pos)
#define | VCMP_OUTCFG_PCA_EXTCLK_EN (0x01 << VCMP_OUTCFG_PCAECI_EN_Pos)
#define | VCMP_OUTCFG_PCA_CAP0_EN (0x01 << VCMP_OUTCFG_PCACAP0_EN_Pos)
#define | VCMP_OUTCFG_INV_PCA (0x01 << VCMP_OUTCFG_INV_PCA_Pos)
#define | VCMP_OUTCFG_LPTIM_EXTCLK_EN (0x01 << VCMP_OUTCFG_LPTIMEXT_EN_Pos)
#define | VCMP_OUTCFG_LPTIM_GATE (0x01 << VCMP_OUTCFG_LPTIM_EN_Pos)
#define | VCMP_OUTCFG_TIM11_GATE (0x01 << VCMP_OUTCFG_TIM11_EN_Pos)
#define | VCMP_OUTCFG_TIM10_GATE (0x01 << VCMP_OUTCFG_TIM10_EN_Pos)
#define | VCMP_OUTCFG_INV_LPTIM_TIM10_11 (0x01 << VCMP_OUTCFG_INV_TIMX_Pos)
#define | VCMP_OUTCFG_MSK (0x7FFFFU)
#define | IS_VCMP_OUTCFG(OUTCFG) (((OUTCFG) & VCMP_OUTCFG_MSK) != 0x0000U)

## 详细描述