MG32L003 Standard Peripherals Firmware Library

结构体
这里列出了所有结构体，并附带简要说明:

C__iar_u32 |
C ADC_InitTypeDef | ADC Init structure definition
C ADC_TypeDef |
C APSR_Type | Union type to access the Application Program Status Register (APSR)
C AWK_InitTypeDef | AWK Init structure definition
C AWK_TypeDef |
C BaseTim_InitTypeDef | BaseTim Init structure definition
C BASETIM_TypeDef |
C BEEP_InitTypeDef | BEEP Init structure definition
C BEEP_TypeDef |
C CLKTRIM_TypeDef |
C CONTROL_Type | Union type to access the Control Registers (CONTROL)
C CRC_TypeDef |
C DBG_TypeDef |
C FLASH_TypeDef |
C GPIO_TypeDef |
C I2C_InitTypeDef | I2C Initial Configuration Structure definition
C I2C_TypeDef |
C IPSR_Type | Union type to access the Interrupt Program Status Register (IPSR)
C IWDG_TypeDef |
C LPTIM_BaseInitTypeDef | LPTIM Time base Configuration Structure definition
C LPTIM_TypeDef |
C LPUART_InitTypeDef | LPUART Init Structure definition
C LPUART_TypeDef |
C LVD_InitTypeDef | LVD Configuration Structure definition
C LVD_TypeDef |
C NVIC_Type | Structure type to access the Nested Vectored Interrupt Controller (NVIC)
C OWIRE_InitTypeDef | OWIRE Init Structure definition
C OWIRE_IT_HandleTypeDef |
C OWIRE_TypeDef |
C PCA_BaseInitTypeDef | PCA Configuration Structure definition
C PCA_IC_InitTypeDef | PCA Input Capture Configuration Structure definition
C PCA_OC_InitTypeDef | PCA Output Compare Configuration Structure definition
C PCA_TypeDef |
C RCC_ClocksTypeDef |
C RCC_TypeDef |
C RTC_AlarmEnableTypeDef | RTC ALARM Enable structure definition
C RTC_AlarmTypeDef | RTC Alarm structure definition
C RTC_DateTypeDef | RTC Date structure definition
C RTC_HandleTypeDef | Time Handle Structure definition
C RTC_InitTypeDef | RTC Init structures definition
C RTC_TimeTypeDef | RTC Time structure definition
C RTC_TypeDef |
C SCB_Type | Structure type to access the System Control Block (SCB)
C SPI_InitTypeDef | SPI Init structure definition
C SPI_IT_HandleTypeDef |
C SPI_TypeDef |
C SYSCON_TypeDef |
C SysTick_Type | Structure type to access the System Timer (SysTick)
C TIM_BDTRInitTypeDef | BDTR structure definition
C TIM_ICInitTypeDef | TIM Input Capture Init structure definition
C TIM_OCInitTypeDef | TIM Output Compare Init structure definition
C TIM_TimeBaseInitTypeDef | TIM Time Base Init structure definition
C TIM_TypeDef |
C UART_InitTypeDef | UART Init Structure definition
C UART_TypeDef |
C VCMP_InitTypeDef | VCMP Init structure definition
C VCMP_TypeDef |
C WWDG_TypeDef |
C xPSR_Type | Union type to access the Special-Purpose Program Status Registers (xPSR)