MG32L003 Standard Peripherals Firmware Library

宏定义 | 函数 | 变量
cmsis_armcc.h 文件参考

CMSIS compiler ARMCC (Arm Compiler 5) header file 更多...

浏览源代码.

## 宏定义
#define | __ASM __asm
#define | __INLINE __inline
#define | __STATIC_INLINE static __inline
#define | __STATIC_FORCEINLINE static __forceinline
#define | __NO_RETURN __declspec(noreturn)
#define | __USED __attribute__((used))
#define | __WEAK __attribute__((weak))
#define | __PACKED __attribute__((packed))
#define | __PACKED_STRUCT __packed struct
#define | __PACKED_UNION __packed union
#define | __UNALIGNED_UINT32(x) (*((__packed uint32_t *)(x)))
#define | __UNALIGNED_UINT16_WRITE(addr, val) ((*((__packed uint16_t *)(addr))) = (val))
#define | __UNALIGNED_UINT16_READ(addr) (*((const __packed uint16_t *)(addr)))
#define | __UNALIGNED_UINT32_WRITE(addr, val) ((*((__packed uint32_t *)(addr))) = (val))
#define | __UNALIGNED_UINT32_READ(addr) (*((const __packed uint32_t *)(addr)))
#define | __ALIGNED(x) __attribute__((aligned(x)))
#define | __RESTRICT __restrict
#define | __NOP __nop
| No Operation 更多...
#define | __WFI __wfi
| Wait For Interrupt 更多...
#define | __WFE __wfe
| Wait For Event 更多...
#define | __SEV __sev
| Send Event 更多...
#define | __ISB()
| Instruction Synchronization Barrier 更多...
#define | __DSB()
| Data Synchronization Barrier 更多...
#define | __DMB()
| Data Memory Barrier 更多...
#define | __REV __rev
| Reverse byte order (32 bit) 更多...
#define | __ROR __ror
| Rotate Right in unsigned value (32 bit) 更多...
#define | __BKPT(value) __breakpoint(value)
| Breakpoint 更多...
#define | __CLZ __clz
| Count leading zeros 更多...

## 函数
__STATIC_INLINE uint32_t | __get_CONTROL (void)
| Enable IRQ Interrupts 更多...
__STATIC_INLINE void | __set_CONTROL (uint32_t control)
| Set Control Register 更多...
__STATIC_INLINE uint32_t | __get_IPSR (void)
| Get IPSR Register 更多...
__STATIC_INLINE uint32_t | __get_APSR (void)
| Get APSR Register 更多...
__STATIC_INLINE uint32_t | __get_xPSR (void)
| Get xPSR Register 更多...
__STATIC_INLINE uint32_t | __get_PSP (void)
| Get Process Stack Pointer 更多...
__STATIC_INLINE void | __set_PSP (uint32_t topOfProcStack)
| Set Process Stack Pointer 更多...
__STATIC_INLINE uint32_t | __get_MSP (void)
| Get Main Stack Pointer 更多...
__STATIC_INLINE void | __set_MSP (uint32_t topOfMainStack)
| Set Main Stack Pointer 更多...
__STATIC_INLINE uint32_t | __get_PRIMASK (void)
| Get Priority Mask 更多...
__STATIC_INLINE void | __set_PRIMASK (uint32_t priMask)
| Set Priority Mask 更多...
__STATIC_INLINE uint32_t | __get_FPSCR (void)
| Get FPSCR 更多...
__STATIC_INLINE void | __set_FPSCR (uint32_t fpscr)
| Set FPSCR 更多...
| __attribute__ ((section(".rev16_text"))) __STATIC_INLINE __ASM uint32_t __REV16(uint32_t value)
| Reverse byte order (16 bit) 更多...
| __attribute__ ((section(".revsh_text"))) __STATIC_INLINE __ASM int16_t __REVSH(int16_t value)
| Reverse byte order (16 bit) 更多...
| __attribute__ ((always_inline)) __STATIC_INLINE uint32_t __RBIT(uint32_t value)
| Reverse bit order of value 更多...

## 变量
uint32_t | sat

## 详细描述

CMSIS compiler ARMCC (Arm Compiler 5) header file

版本
  V5.0.4

日期
  10. January 2018