MG32L003 Standard Peripherals Firmware Library

宏定义
Core Definitions
Defines and Type Definitions

Definitions for base addresses, unions, and structures. 更多...

## 宏定义
#define | SCS_BASE (0xE000E000UL)
#define | SysTick_BASE (SCS_BASE + 0x0010UL)
#define | NVIC_BASE (SCS_BASE + 0x0100UL)
#define | SCB_BASE (SCS_BASE + 0x0D00UL)
#define | SCB ((SCB_Type *) SCB_BASE )
#define | SysTick ((SysTick_Type *) SysTick_BASE )
#define | NVIC ((NVIC_Type *) NVIC_BASE )

## 详细描述

Definitions for base addresses, unions, and structures.

## 宏定义说明

## ◆ NVIC

#define NVIC ((NVIC_Type *) NVIC_BASE )

NVIC configuration struct

## ◆ NVIC_BASE

#define NVIC_BASE (SCS_BASE + 0x0100UL)

NVIC Base Address

## ◆ SCB

#define SCB ((SCB_Type *) SCB_BASE )

SCB configuration struct

## ◆ SCB_BASE

#define SCB_BASE (SCS_BASE + 0x0D00UL)

System Control Block Base Address

## ◆ SCS_BASE

#define SCS_BASE (0xE000E000UL)

System Control Space Base Address

## ◆ SysTick

#define SysTick ((SysTick_Type *) SysTick_BASE )

SysTick configuration struct

## ◆ SysTick_BASE

#define SysTick_BASE (SCS_BASE + 0x0010UL)

SysTick Base Address