Next: Constants, Previous: Symbol Intro, Up: Syntax [Contents][Index]

### 3.5 Statements

A statement ends at a newline character (‘`\n`’) or a line separator character. The line separator character is target specific and described in the Syntax section of each target’s documentation. Not all targets support a line separator character. The newline or line separator character is considered to be part of the preceding statement. Newlines and separators within character constants are an exception: they do not end statements.

It is an error to end any statement with end-of-file: the last character of any input file should be a newline.

An empty statement is allowed, and may include whitespace. It is ignored.

A statement begins with zero or more labels, optionally followed by a key symbol which determines what kind of statement it is. The key symbol determines the syntax of the rest of the statement. If the symbol begins with a dot ‘`.`’ then the statement is an assembler directive: typically valid for any computer. If the symbol begins with a letter the statement is an assembly language instruction: it assembles into a machine language instruction. Different versions of `as` for different computers recognize different instructions. In fact, the same symbol may represent a different instruction in a different computer’s assembly language.

A label is a symbol immediately followed by a colon (`:`). Whitespace before a label or after a colon is permitted, but you may not have whitespace between a label’s symbol and its colon. See Labels.

For HPPA targets, labels need not be immediately followed by a colon, but the definition of a label must begin in column zero. This also implies that only one label may be defined on each line.

    label:     .directive    followed by something
    another_label:           # This is an empty statement.
               instruction   operand_1, operand_2, …

Next: Constants, Previous: Symbol Intro, Up: Syntax [Contents][Index]